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	Intermediate Cut - No Regeneration Obligation – Standards

	

	Minimum Crop Tree Basal Area Retained (M2/ha)
	Standards ID
	Additional Criteria (all areas)

	50
	1033935
	To meet the minimum BA standard - retained crop tree basal area must be comprised of merchantable trees (Pli 12.5 cm DBH, other species 17.5 cm DBH) that meet or exceed the minimum leave tree characteristics outlined below.
To qualify as an IC a minimum of 40% of the stands original BA must be retained or the minimum BA by BEC zone whichever is greater.


	45
	1033936
	

	40
	1033937
	

	35
	1033938
	

	30
	1033939
	

	26
	1033940
	

	24 min for all other BEC Zones
	1033941
	“NoRegen” Obligation Window is early 1 year and late 4 years


	18 min for the MS dk, IDF dm2, ICH mk1, ICH mw1, ESSF dk BEC Zones only
	1033942
	

	15 min for Beetle Proofing. HDR does not apply
	1033943
	When reporting the Forest Cover Inventory for an Intermediate Entry report the Total BA retained in the Inventory label and the Crop Tree BA in the Silviculture Label

	
	
	

	
	
	



Preferred and acceptable species to be retained are as specified in Table A by biogeoclimatic ecosystem classification (BEC) site series.  

Table C Stocking Standard Definitions

Minimum leave tree characteristics:  

Stands Age Class 6 and Younger:
Crop trees must meet limits defined in the Tree Wounding and Decay guidebook (Feb 97)-Long Term Retention Objective to be acceptable.
Crop trees of all species must have a height to diameter ratio (HDR) of 1.0 or less to be acceptable - except Pli which must have a HDR of 1.2 or less.
All trees must meet criteria defined in Appendix 10, Establishment to Free Growing Guidebook: Nelson Region - May 2000.

Stands Age Class 7 and Older
Crop trees must meet the limits defined in the Cruising Manual (effective June 1, 2008) for tree classes 1, 2, 5, and 8.
Crop trees of all species must have a height to diameter ratio of 1.0 (HDR) or less to be acceptable - except Pli which must have a HDR of 1.2 or less.

Table C Stocking Standard Definitions

Stands Age Class 7 and Older cont’d

All trees must meet criteria defined in Appendix 10, Establishment to Free Growing Guidebook: Nelson Region - May 2000.


Minimum Strata Size for Reforestation Obligations:

Any contiguous strata greater than one hectare, that as a result of harvesting have a basal area less than 18 m2 per ha for the MS dk, IDF dm2, ICH mk1, ICH mw1and ESSF dk BEC Zones, and 24 m2 for all other BEC Zones shall be reforested as specified in Table A by BEC site series. 

Additional information or requirements may be found in the text portion of these standards and/or in the FSP 
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