CP 410 Fuel Reduction Work Plan

In All Units other than WTRA: - the harvesting operation will harvest all merchantable stems (>=17.5m @ DBH) - Not FES funded
FES Funded:
Live Tree Thinning:
· no falling of merchantable stems is prescribed
· fall all understory remaining after logging operation
· stumps must be <=30cm tall above ground surface

Shrubs:
· healthy deciduous shrubs should be retained, where practicable
· deciduous shrubs that have an excess of 25% component of dead material should be removed

Coarse Fuels  
· where applicable, retain a minimum of 50 pieces/ha (15m spacing) >12.5cm at top & >3m in length randomly throughout the blocks.  Maximum retained CWD should not exceed 150 pieces/ha.  Excess CWD should be bucked, piled & burned
· coarse fuels should be left bucked so they flat on the ground

Fine Fuels:
· post treatment surface fuels should not exceed the following loadings:
· woody debris 7-12cm diameter should not exceed 25 tonnes/ha
· woody debris <7cm should not exceed 5 tonnes/ha
· all woody debris in excess of the above targets will be piled and burned

Pruning: (expected no pruning will be required in the harvested areas)
· prune retained conifers to 4m.  Pruned cuts should be flush with the tree stem

Debris Disposal - Burning:
· must be done in accordance with a smoke management plan developed in consultation with the SE Wildfire Branch
· burning must be conducted in a manner that minimizes impacts to the site and the retained trees
· burn piles must be constructed to facilitate effective ignition and complete combustion
· burn piles must be within the block areas.  Large number of piles will be constructed to minimize the size of any one pile - smaller piles in favour of fewer large piles to minimize scorching of or heat damage to retained trees.  To reduce the number of piles, burning should occur concurrently with thinning/piling operations (including machine treatment areas) using the hot-bed technique.  Burning cannot occur when weather conditions are not acceptable to burn
· burning is to be conducted in compliance with the BC Wildfire Act & Wildfire Regulation & any applicable Bylaws, must comply with the Environmental Management Act Open Burning Smoke Control Regulations.
· -it is the contractor's responsibility to obtain all necessary burning permits
