	
2015 Waypoint Actioning Assignment Logic, Bulkley TSA                2015-11-03


	Zone
	Criteria
	Geoprocessing Needs

	General
	In and within 1km of High to Ext Hazard Types = “assign an action”
	Select High to Ext Hazard Types within 500m of all roads FCODE’d to “gravel” or “paved” on District road files. Buffer by 1 km.

	
	[bookmark: _GoBack]Other Hazard Types = “no action-gen”
	

	Private land, Indian Reserve
	Code “F&B/ SSS”
	

	Parks, Protected
	– within 1 km of a “gravel or paved” access road, plowed or not = “F&B-prks”
	Buffer “gravel or paved” roads by 1 km

	
	- all other situations = “no action-prks”
	

	SMZ1
	– within 1 km of “gravel or paved” access road, plowed or not = “F&B-sm1”
	Develop 1km bufferfile around “gravel or paved” roads

	
	- within 300m of a plowed access road = potential for SSS by long-line skid, but only if ground probe shows sufficient currents are present = “SSS-sm1-probe”
	Develop 300m bufferfile around “2015 plowed” roads

	CE
	<4 reds = “no action-ce-le3”
	

	
	Within 1 km buffer off open roads, 4-10 reds = “F&B-ce”
	

	
	Within 300m buffer off plowed roads, individual waypoints or waypoint within 100m of each other with total >10 reds = “HVST” or “Hold to Harvest” or “SSS”, but only if ground probe shows sufficient currents are present = “HVST-ce-probe”
	Put a 100m buffer around all waypoints to develop “grouped waypoint polygons”. Dissolve into a shapefile, sum #reds. 

	LRC, FSW
	All LRC’s, FSW’s:
<5 reds = no action
Any other level of red outside 1km of 100m roadbuffs = no action
	Develop layer showing which LRC’s are >= thresholds

	
	LRC’s or FSW’s where status of thresholds is “red”, and within 1km buffer around “gravel or paved” roads = “F&B”
	

	
	LRC’s or FSW’s where status of thresholds is not “red”

Where grouped waypoint poly’s total 5-10 reds, and within 1km road buff = “F&B”

Where grouped waypoint poly’s total >10 reds, and within 300m buffer off plowed roads = “HVST” or “Hold to Harvest” or “SSS”
	

	IRM, CW’s, ETD, WHMA
	Use [“All LRC’s, FSW’s”, and “LRC’s or FSW’s where status of thresholds is not “red”]    criteria
	

	RRZ’s, WTRA’s
	“F&B” only
	



Assumptions: 
· For planning purposes and in absence of ground probe, have assumed 2 green (currents) per 1 identified red
· SSS – will be a general option in all surveyed areas where road will be plowed in winter 2015. Babine – for LBN, particularly behind the Fort; McD/ Deep Creek – all areas are within 50 km of mill.
· HVST; Hold to Harvest – major licensees to be given first dibs on a harvest opp in their Operating Area (i.e. in situation where waypoint could be coded HVST or H2H or SSS, always start by coding to HVST). If licensees advise they can’t action a waypoint in 2015, but can in 2016, then recode to Hold to Harvest (i.e. would need to hang bait in June 2016). If licensee advises they can’t action a waypoint by winter 2016, recode now to SSS and identify to SSS community. If SSS community not interested, then one final recode to F&B.
· No SSS or HRVST or Hold to Harvest in SMZ1’s or CE’s in absence of a ground probe that verifies current attack at minimum 1:1 or higher is present.


Map particulars:
· 1:50K, one map for each EMU that was surveyed
· Include:
· Waypoints, themed by Action
· Tracking
· Roads, themed by open, + open&2015 winter plowed
· Licensee operating areas
· LRMP zones from above list
· High-Extreme IBM Hazard
· Slopes >=60%
· Existing and proposed cutblocks and WTRA’s
· Cultural heritage – trails, features, CMT’s, high Arch Pot from AOA’s
· Ownership
