DSS FREP Random Sampling Contract – Block Access Notes
2023-08-09

RIP 1 – Opening_ID 1729619
· Start at junction of Hwy 16 and Hwy 37.
· Go north on Hwy 37 to start of Nass FSR (77 km, paved road). 
· Carry on north on Hwy 37 to junction with Derrick Lake FSR (7 km, paved road). Turn left off Hwy 37 onto R09210-10 Rd (unsigned) at this junction.
· Follow R09210-10 Rd to junction with R14517-10 Rd (~10 km, gravel 2WD dry/ 4WD wet resource road)
· Starting at ~4 km on the R09210-10 Rd is a 500 m rough stretch (partly washed out; repairs still underway, narrow running surface with sharp-edged rock fill). Road then smooths out.
· Carry on along R09210-10 Rd to junction with the R09210-50 Rd (~1.7 km, gravel 2WD dry/ 4WD wet resource road)
· Follow R09210-50 Rd into the north end of the block (~0.3 km, gravel 4WD resource road)

RIP 2 – Opening_ID 1733533
· Start at junction of Hwy 16 and Telkwa High Road in Witset village.
· Follow Telkwa High Road to junction with Blunt Creek FSR (aka the “2000 Rd”, aka the 6144-010 Rd ) (~0.7 km, gravel 2WD local road)
· Follow the “2000 Rd” to junction with R09533-2180 Rd (aka the “218 Rd”)(~18 km, gravel 2WD resource road)
· Follow the “218 Rd” to stream crossing at center of north end of block (~1 km, gravel 2WD resource road).
· All in-block roads are deactivated, with culvert pulls/ pullback. ATV or walk-in only (ATV recommended)

RIP 3 – Opening_ID 1756184
· Start at junction of Hwy 16 and Hwy 92 in New Hazelton (I,e, the highway to Old Hazelton)
· Follow Hwy 92 to junction with Kispiox Valley Road at Gitanmaax village (~6 km, paved road)
· Follow Kispiox Valley Road to junction with Salmon River Road (~3 km, paved road)
· Follow Salmon River Road (turns into Babine Slide FSR at km 9) to km 37.4 and junction with the block access road (use km signs) (37.4 km, 1st 9 km is well-maintained gravel 2WD local road, remainder is gravel 2WD resource road, can be rough/ potholed – recent harvest in area, expect low-moderate log haul truck traffic).
· Follow block access road (“R03780-240 Rd”) <1 km to south block edge. Major culvert pull/pullback at block edge, ATV or walk-in only from this point.
· Block access road crosses S3 stream near block edge. Flows within 2 RMA widths of south and eastern block boundary, i.e. sample-able reach.


RIP 4 – Opening_ID 1714349
· Follow RIP 3 Access Notes up to km 37.4, Babine Slide FSR and junction with R03780-240 Rd
· Carry on another ~2 km up Babine Slide FSR to junction with R03780-150 Rd (broken yellow road sign at start).
· Follow R03780-150 Rd to SW corner of block  (~8 km, gravel 4WD resource road). 
· Road pinches down to ATV width after SE corner of block
· sample-able S4 stream reaches are present, running along both the W and E edges of the block

RIP 5 - Opening_ID 1733740
· Start at Skeena Stikine District Office (Tatlow Road, Smithers)
· Follow Hwy 16 east to junction with Babine Lake Road (~4 km, paved highway)
· Follow Babine Lake Road to junction with Nilkitkwa Rd, aka the “4000 Rd” (~50 km, gravel 2WD local/ resource road)
· Follow 4000 Rd to the “455 Rd” (55 km, gravel 2WD resource road. The 4000 Rd is one of the busiest in Bulkley TSA, expect high volume log haul truck traffic). 
· Follow 455 Rd to block access road (~6 km, gravel 2WD resource road). 
· Follow block access road into block (~ 130 meters, major culvert pull/ large gravel mound at immediate start of access road, walk-in or ATV access only)
· S2, S3 and S4 stream reaches present. S3 and S4 reaches are sample-able (S4 was dry at time of recce). The S2 reach is marginal, but S2 may be an over-call as stream width looked to be <5m
· Bridges are pulled at both “S2” and “S3” stream crossing locations (per Site Plan Map) entering into south end of block. Also, all in-block roads are deactivated, with culvert pulls/ pullback. Still ATV accessible.



RIP 6 - Opening_ID 1733173
· Start at Skeena Stikine District Office (Tatlow Road, Smithers)
· Follow Hwy 16 east to junction with Babine Lake Road (~4 km, paved highway)
· Follow Babine Lake Road to junction with 3101-010 Rd (aka Upper Fulton Rd, aka “3000 Rd”) (~39 km, gravel 2WD local/ resource road)
· Follow 3000 Rd to junction with R09511 341-10 Rd (aka “338 Rd”)(38 km, gravel 2WD resource road)
· Note: active haul was occurring off the “326 Rd” during this accessibility check
· Follow the “338 Rd” to junction with R09511 340-10 Rd (aka “338-1 Rd”)(~1 km, gravel 2WD resource road)
· Follow “338-1 Rd” a few hundred metres in, to the location of a major culvert pull/ pullback. ATV or walk-in only from this point - ATV recommended. Junction with R09511 340-1-1.50 Rd is about 600 metres in from start of “338-1 Rd”.
· Follow R09511 340-1-1.50 Rd to junction with block access road R09511 CP 079-066-SP10 (~900 metres).
· Follow block access road to south edge of block (~500 metres) 
· 2 sample-able S6 reaches, one at SW block edge, the other at NE edge

RIP 7 - Opening_ID 1733539

· Follow RIP 6 Access Notes to junction with 3101-010 Rd (aka Upper Fulton Rd, aka 3000 Rd)
· Follow 3000 Rd to junction with R09511 350 RD0 (aka the “350 Rd”) (50 km, use km signs, gravel 2WD resource road (when dry), 4WD when muddy/wet. Graded to km 40 then narrows off/ potholey)
· Follow 350 Rd to junction with block access road (~3.8 km, gravel 2WD resource road). Major culvert pull/pullback just before junction (just after a bridge – covered with water but driveable). ATV or walk-in only from this point (ATV recommended)
· Follow block access road “northerly, keeping to right fork”, to south edge of block (~850 metres, ATV or walk-in). Culvert pulls/ pullback frequent, pullback material okay when dry but will get soft in wet weather and may slow ATV.
· Sample-able S3 reach on SW edge, and S4 reach on SE edge


RIP 8 - Opening_ID 1716199

· Follow RIP 6 Access Notes to junction with 3101-010 Rd (aka Upper Fulton Rd, aka 3000 Rd)
· Follow 3000 Rd to junction with block access road (~44.5 km, use km signs, gravel 2WD resource road). Major culvert pull/ pullback occurs quickly along block access road, ATV or walk-in only past this point.
· Follow block access road to south edge of block (~500 metres, ATV or walk-in)
· Sample-able S3 reach on SW block edge

