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Buffer sizes depending on plot size for SMC plots:

For a 45m square plot (0.202 ha), the buffer is an additional 9.3m on each side

For a 37m square plot (0.137 ha), the buffer is an additional 7.7m on each side

For a 33m square plot (0.109 ha), the buffer is an additional 6.8m on each side

For a 32m square plot (0.102 ha), the buffer is an additional 6.6m on each side

For a 30m square plot (0.09 ha), the buffer is an additional 6.2m on each side

For a 29m square plot (0.08 ha), the buffer is an additional 6.0m on each side

These are horizontal distances.

An additional section may be added on one side for destructive sampling.
The formula for the 45m square plot is:
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Diagonal out corner to corner is therefore 13.2m
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