INSTALLATION SUMMARY REPORT

EP# 307 INST. 2 (Fosthall)                       DATE: Oct 2013
CREW: Jesse Scott, Jake King, David Eveno, Scott Gailey
EQUIPMENT USED: hypsometer, transponder, GPS, camera, LED Headlamp, diameter tape, logger’s tape, paint, nail puller, staple gun, compass and two Allegro field computers.
ACCESS: Old access notes are excellent. After getting off the Arrow Park ferry, you have two options, either taking the Stevens Rd to Fosthall, or taking Saddle Mt Rd, while Fosthall Rd is better maintained, we found the latter preferable as it was more direct, and had considerably less logging traffic. Blue paint trails were painted from the right landing where you park to plots 1, 2, 15, 16 & 17 to the left of the landing from plots 3 through 12, and 18 to 20. The trail to plot 14 is painted from the 7km rd sign.
WEATHER CONDITIONS:  Snow was a problem.
% SLOPE & DIRECTION: The north facing slope ranged from 10 to 30 percent throughout the majority of the trial except for plots 12 and 14, which were flat.
CORNERS: PVC corner posts were found, stood up and ribboned with flagging tape. There were no center posts in this trial.

INGROWTH: Close to 800 ingress were brought in, with plots 4, 12 and 18 all having well over a hundred.
TAGS: The tags on the original trees, and older ingress were mostly the aluminum tags on nails and generally in decent condition, all nails were pulled out to an acceptable length where necessary and were replaced with write-on aluminum tags on ladder-back zip-ties when needed.  Tags on smaller trees were an absolute mess, with hundreds missing across the trial, due to it being a heavy snowfall area in the winter, and the fact that trees are too small to hold onto their tags
HEIGHT VISIBILITY: Good visibility of tops due a nice natural slope in most of the plots
AMBIGUITIES: Some lingering snow drifts, in some of the more open areas of the trial could account for some the smaller missing trees. The fact that the most recent set of ingress (1997) has not been added to the stem maps, combined with the aforementioned problems with the smaller trees keeping their tags through winter conditions, meant there was a large number of trees, that although they had paint lines and had clearly been measured before, were now completely unidentifiable, and had to be brought in as new trees. The previous contractors had failed to bring any ingress in plot 18 during the last set of measurements, so a lot of the ingress we had brought in there should have been added in 1997. Plots 12 and 14 are a lot flatter and wetter than the rest of the trial, both had seasonal run-off streams running through them in the spring, plot 12 is next to where plot 13 had been logged and because of that has the most ingress coming up.
