PL Field Pre-Work Notes-
EMS Responsibilities and Safety Responsibilities
Ensure all staff obtained training in EMS – Internal Audit begins Today, please have EMS binder on site, signs posted etc.
3 components – Fire/Landslide/Spill – STOP WORK if you are unsure.
Planting Quality  -Common issues in the Cariboo
· Open holes 
· Grass mat
· Shallow
· Too close – to naturals
· Achieving required densities
· Poor microsite selection
· Put the fir in the right spots
· Species mix – mixed bag planting we do not like to see lines 
FS 704 Questions
· Excess tree
· Missed spots – no other planted tree or accp nat (in or out) is within contract spacing
· Wide Spacing
Schedule C of the  contract
Unacceptable crop trees (to be ignored at time of planting):
· any deciduous; and
· any advanced regeneration (established prior to logging date), unless:
· no visible damage, pest or disease whatsoever;
· straight stem;
· greater than fifty percent (50%) live crown;
· greater than fifteen (15) centimetres (cm) leader; and/or
· within twenty (20) cm of ripping or disc trenching site preparation treatment.
D.	Acceptable crop trees:
· if regeneration (established after logging);
· [bookmark: _GoBack]west of the Fraser River – fifteen (15) cm total height for Douglas-fir and spruce, five (5) cm total height for pine;
· east of the Fraser River – ten (10) cm total height for Douglas-fir,spruce, and lodgepole pine;
· good color and vigour, with a dominant leader;
· no visible damage, pest or disease whatsoever;
· straight stem;
· greater than fifty percent (50%) live crown; and
· not within twenty (20) cm of ripping or disc trenching site preparation treatment.

E.	Preferred planting micro sites in order of preference are:
· within twenty (20) cm of any stump or large obstacle; obstacles such as logs and rocks must be twenty (20) cm in height to be considered a preferred microsite;
· undisturbed natural high spots;
· mineral soil, or an acceptable mixture of mineral soil and organic matter; and
· where the site is prepared by mounding or disc trenching, planting in between the site preparation may be required to ensure target densities are met.

Note:  When a preferred microsite is available at the prescribed spacing but is not used, a planting fault may result.  For example, if a stump is available to plant beside but the seedling is planted greater than twenty (20) cm from the stump in mineral soil, a planting fault may result.
Unacceptable planting micro sites are:
· rotten logs, stumps and other organic material subject to drying out;
· flooded areas or the bottom of depressions or gullies subject to flooding;
· cutbanks, roadside fill, loose humps or soil, gravel or debris subject to drought;
· within three (3) metres of major access roads or as otherwise designated in the block specifics;
· within the drip line of larger trees unless otherwise indicated in the block specifics;
· under overhead obstacles that could interfere with seedling growth; and
· within 1.5 metres (m) either side from the centreline of fences.


The use of Silvacool Two type tarps will not be allowed for providing protection to planting boxes.  Silvacool Two type tarps can be identified by the extra layer of black plastic in between the white and silver layers.
Silvacool liners must be used by all planters and they must be in all bags including the draw bag.



