AIR CODES - TFL & CANAL

HARVESTING CODE
HECTARES AFFECTED

1
Conventional logging chance
A
0.1

2
Cable Logging Chance
B
0.5

3
Not accessible
C
1.0

4
Private land
D
3.0

5
Blowdown – conventional
E
5.0

6
Blowdown - not accessible
F
7.0

ATTACK CODE
G
10.0

R
Red attack pine
H 
15.0

GR
Green attack pine
I
20.0

G 
Grey attack pine
J
25.0

FD
Douglas-fir
K
30.0

S
Spruce beetle
L
40.0

RU
Pine needle rust
M
50.0

DR
Armillaria root rot
N
60.0

LO
Looper
O
75.0



P
100.0

STEMS AFFECTED
Q
150.0

1
1   to   5 stems
R
200.0

2
6   to 10 stems
S
250.0

3
11 to 15 stems
T
300.0

4
16 to 20 stems
U
400.0

5
21 to 30 stems



6
31 to 50 stems



7
50 to 75 stems



8
Over 75 stems













SAMPLE
1R1A



(Conventional Logging, Red attack pine, 1 to 5 stems affected on 0.1 ha)

