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Submission Standards for On-block GPS’d Roads:

Landings at the End of a Road Line

If there is a turnaround or landing at the end of a road, it should be GPS’d as a closed linework extending from the end of the road centreline that indicates the outside boundaries of the landing. This means that a landing shape must not be digitized as a single line (ex: Figure 3). See images below.
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Figure 1
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Figure 2
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Figure 3
Pullouts and Landings along the Side of a Road
It will be assumed that landings and turnouts that occour along a road will be drawn from the centreline of the road and not from the edge of the road. The GPS’d shape will overlap the area that will be part of the regular road width. See Figure 5 (here the green shaded area indicates the actual road width). Please note that the actual road width shape should not be included the contractor submitted files as a linework. 
Linework should not have a gap (road width) between the centreline and the pullout. See example, Figure 7.
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Figure 5
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Figure 6
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Figure 7
Drawings for Turnarounds, Pullouts and Landings
If the contractor is GPSing a road with a turnaround, pullout or landing, then a separate drawing for that shape with measurements is optional. (If digital files are provided, the contractor can choose not to include paper drawn diagrams of the turnaround, pullout, or landing.)
Questions/Concerns

· If your GPS software does not support BC Albers Projection, you may use NAD 1983 UTM Zone 10N Projection format. However, please notify your contract administrator/GIS Staff at BCTS about your intent

· If you need further clarification on this standard, please contact GIS Staff at BCTS as soon as possible
· A copy of this document can be downloaded from this location: ftp://ftp.for.gov.bc.ca/TCC/external/!publish/Data_Standards/ArcGIS/ABR_Contracts/ 
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