LOCATION MAPS FOR TIMBER SALE PACKAGES

It is recommended that:

· Two locator maps be created for the TSL tender package 

· The location map and local access map created digitally by contractor or BCTS (No scanned maps!)

· The map be built on a clear uncluttered base map “ROADMAP” 1:250000 (Location Map) and FC1 1:20000 (Local Access Map) showing towns, roads, water bodies and major streams

· The location map and local access map created to be printed on 8 1/2 by 11 “portrait” is preferred or 8 1/2 by 14 paper

· Where all blocks in a Timber Sale cannot be shown on one map, multiple 8 1/2 by 11 maps should be made.  Multiple maps should be accompanied by a key map, which shows the areas covered by each map.

· Text within the map should be font 1 size 625
· A scale bar be used rather than a scale ratio in case the map is not printed at the intended size
· Field offices have map writing software (including digitizing tablet)for digital map production (arcview , RoadEng, power scope or other)

As a minimum standard the Location Map should contain the following elements:

· Title of Map including TSL number and block number  (if applicable)

· Scale bar and north arrow

· Map showing Timber Sale location in relation to a major center at an appropriate scale (i.e. 1:250,000)

· The block location highlighted and labeled.

· The route leading to the TSL should be red and highlighted (weight 2) on the map with kilometer markers identified or key junctions and spurs (all other roads shall be black),

· Text box describing detailed access notes from a specified point in a major center to the cut block or to a reference point identifiable on the local access map.(see below)

· All junctions noted in the access directions to be labeled on map

· UTM and/or lat/long coordinates of the cut block or central point.  This can be included in the header as shown or as an inset text box pointing to the specific location on the map

As a minimum standard the Local Access Map should contain the following elements:

· Title of Map including TSL number and block number  (if applicable)

· Scale bar and north arrow

· The block location highlighted and labeled

· Roads in the vicinity of the block at an appropriate scale (i.e. 1:20,000 to 1:30 000),

· Map should include at least one of the labeled points from the location map.

· UTM and/or lat/long coordinates of the cut block or central point

In the access directions detail the specific information required to locate the block(s) from a specified point in a major center or reference point shown on the location map. Include specific kilometre markers, junctions and other identifiable features.  For example:
Access Directions (distances approximate)

From the Highway 19 Bridge over the Campbell River

drive north for 19 kilometers to the junction of Hwy. 19 and

Browns Bay 200 on the left side of the highway

The Crane Lake main starts here.  Follow the proposed road 

centerline (flagged in pink)for 400 meters to the TSL boundary
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