February 05, 2005


Note to contractor

LOCATION MAP:

As a temporary measure, the location map must be created using “Location basemap250.dgn” as a base map and the Location map template. The contractor must ensure to show a complete road system from a known point such as Williams Lake to the work site. As this map has not been updated for a few years, it is expected that segments of “built” road are missing (road permits from other licensees) 

The contractor must either GPS the missing segment or retrieves the segment from another data source such as FC1 maps. Refer to the “Location map content file” for more information.

ACCESS MAP:

The access map must be created using “the appropriate FC1 file” as a base map and the access map template. The FC1 files are available upon request from BCTS staff. The contractor must ensure to show a complete road system within approximately 2km from the work site. As the FC1s have not been updated for a few years, it is expected that segments of road are missing (road permits from other licensees) 

The contractor must either GPS the missing segment or retrieves the segment from another data source. Refer to the “Location map content file” for more information. Do not show on-block roads within a block unless the roads are laid out and surveyed.
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