8.0 Stocking Standards Williams Lake
Section 44(1) (a), (b) and Section 45 of the Forest Planning and Practices Regulation apply to all areas harvested under this Forest Stewardship Plan except where Section 44(3) of the Forest Planning and Practices Regulation applies and areas harvested within the identified grasslands benchmark area.

Table A
	License
	
	
	BGC
	Regeneration Guide
	Free Growing Guide

	STK STD
	FSP Tracking System Name
	STK STD
	Classification
	Species
	Stocking(i)
	Regen
	Min
	Ht >
	Assessment
	Min. Height(ii)

	Descriptor
	
	Number
	
	
	Conifer
	Target
	MIN pa
	MIN p
	Min p

conifers
	Delay
	Intertree
	Brush
	Earliest
	Latest
	Species
	Ht

	
	
	Zone/SZ
	Series
	Preferred (p)
	Acceptable (a)
	
	(Max yrs)
	Dist
	%
	(yrs)
	(yrs)
	
	(m)

	BCTS even-aged
	ESSFwc3 01 - WL
	1016531
	ESSFwc3
	01
	 Sx   Bl
	 Pli3
	1200
	700
	600
	
	7
	2.0
	125
	 
	20
	Pli
	1.6

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ESSFwc3 02 - WL
	1016885
	ESSFwc3
	02
	 Sx   Bl  Pli34
	  
	1000
	500
	500
	
	7
	2.0
	125
	 
	20
	Pli
	1.2

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Others
	0.6

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ESSFwc3 03 - WL
	1017428
	ESSFwc3
	03*
	 Sx1, 32, 34   Bl 1, 32, 34
	  
	600
	400
	400
	
	7
	2.0
	125
	 
	20
	All
	0.6

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	
	

	 
	
	 
	 
	 
	 
	  
	 
	 
	 
	
	 
	 
	 
	 
	 
	 
	 

	BCTS even-aged
	ESSFwk1 01 - WL
	1017429
	ESSFwk1
	01
	 Sx   Bl   Pli34
	  
	1200
	700
	700
	
	7
	2.0
	125
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Others
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ESSFwk1 02 - WL
	1017430
	ESSFwk1
	02*
	 Sx   Bl  Pli
	 
	1000
	500
	500
	
	7
	2.0
	125
	 
	20
	Pli
	1.4

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ESSFwk1 03 - WL
	1017431
	ESSFwk1
	03
	 Sx   Pli 34
	Bl
	1200
	700
	600
	
	7
	2.0
	125
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ESSFwk1 04 - WL
	1017432
	ESSFwk1
	04
	 Sx32  Bl32 
	Pli3
	1200
	700
	600
	
	7
	2.0
	125
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Others
	1.0

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ESSFwk1 05- WL
	1017433
	ESSFwk1
	05
	 Sx   Bl
	Pli3 
	1200
	700
	600
	
	7
	2.0
	125
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ESSFwk1 06 - WL
	1017434
	ESSFwk1
	06,07
	  Bl1,32 Sx1,32 
	
	1000
	500
	500
	
	7
	1.6
	125
	 
	20
	All
	0.8

	
	ESSFwk1 07 - WL
	1017435
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	
	 

	BCTS even-aged
	ESSFxv1 01 - WL
	1017436
	ESSFxv1
	01
	Pli32 Sx32
	 Bl32,50 Pa 
	1200
	700
	600
	
	7
	2.0
	125
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ESSFxv1 02 - WL
	1017437
	ESSFxv1
	02*
	Pli Pa
	Bl28 
	800
	500
	400
	
	7
	2.0
	125
	 
	20
	Pli
	0.8

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Others
	0.6

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ESSFxv1 03 - WL
	1017438
	ESSFxv1
	03*
	Pli Pa
	  
	800
	500
	500
	
	7
	2.0
	125
	 
	20
	Pli
	0.8

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Pa
	0.6

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ESSFxv1 04 - WL
	1017439
	ESSFxv1
	04
	Pli Pa
	Bl28 Sx28 
	1000
	600
	500
	
	7
	2.0
	125
	 
	20
	Pli
	0.8

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Others
	0.6

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ESSFxv1 05 - WL
	1017440
	ESSFxv1
	05
	Pli Pa
	Bl28 Sx28 
	1200
	700
	600
	
	7
	2.0
	125
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ESSFxv1 06 - WL
	1017441
	ESSFxv1
	06
	Pli  Sx32
	Bl32 
	1200
	700
	600
	
	7
	2.0
	125
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ESSFxv1 07 - WL
	1017442
	ESSFxv1
	07
	Pli32 Sx32
	Bl32 
	1200
	700
	600
	
	7
	2.0
	125
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ESSFxv1 08 - WL
	1017443
	ESSFxv1
	08
	Pli1,32 Sx1,32
	 Bl1,32 
	600
	400
	300
	
	7
	1.6
	125
	 
	20
	Pli
	0.8

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Others
	0.6

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ESSFxv1 09 - WL
	1017444
	ESSFxv1
	09
	Sx1,32 Bl1,32
	Pli1 
	800
	500
	400
	
	7
	1.6
	125
	 
	20
	Pli
	0.8

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	0.6

	 
	
	 
	 
	 
	 
	 
	 
	 
	 
	
	 
	 
	 
	 
	 
	 
	 

	BCTS even-aged
	ESSFxv2 01 - WL
	1017445
	ESSFxv2
	01
	Pli  Bl32 Sx32 
	  Pa 
	1200
	700
	600
	
	7
	2.0
	125
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ESSFxv2 02 - WL
	1017446
	ESSFxv2
	02*
	Pli Pa
	Bl28,53 
	800
	500
	400
	
	7
	2.0
	125
	 
	20
	Pli
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	0.6

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ESSFxv2 03 - WL
	1017447
	ESSFxv2
	03*
	Pli
	Pa 
	600
	400
	300
	
	7
	2.0
	125
	 
	20
	Pli
	0.8

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Pa
	0.6

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ESSFxv2 04 - WL
	1017448
	ESSFxv2
	04
	Pli
	 Bl28 Pa 
	1200
	700
	600
	
	7
	2.0
	125
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ESSFxv2 05 - WL
	1017449
	ESSFxv2
	05
	Pli Sx
	Pa Bl 
	1200
	700
	600
	
	7
	2.0
	125
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ESSFxv2 06 - WL
	1017450
	ESSFxv2
	06
	Pli Sx
	Bl 
	1200
	700
	600
	
	7
	2.0
	125
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ESSFxv2 07 - WL
	1017451
	ESSFxv2
	07
	Pli Sx32
	 Bl32 
	1200
	700
	600
	
	7
	2.0
	125
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ESSFxv2 08 - WL
	1017452
	ESSFxv2
	8
	Sx1,32 Bl1,32
	Pli1  
	600
	400
	300
	
	7
	1.6
	125
	 
	20
	Pli
	0.8

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Others
	0.6

	 
	
	 
	 
	 
	 
	  
	 
	 
	 
	
	 
	 
	 
	 
	 
	 
	 

	BCTS even-aged
	ESSFxv2 08 - WL (2)
	1017453
	ESSFxv2
	8,9,10
	Sx1,32 Bl1,32
	Pli1, 32 
	600
	400
	300
	
	7
	1.6
	125
	 
	20
	Pli
	0.8

	
	ESSFxv2 09 - WL
	1017454
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Others
	0.6

	
	ESSFxv2 10 - WL
	1017455
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	 
	
	 
	 
	 
	 
	  
	 
	 
	 
	
	 
	 
	 
	 
	 
	 
	 

	BCTS even-aged
	ICHmk3 01 - WL
	1017457
	ICHmk3
	01
	Fdi Pli Sx
	Bl Cw37
	1200
	700
	600
	
	7
	2.0
	150
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.4

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	1.0

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	BCTS  mixedwood
	ICHmk3 01 mixed wd - WL
	1017458
	ICHmk3
	01
	Fdi, Pli, Sx, Act, At, Ep
	Bl, Cw37 , 
	1600
	1000
	800
	600
	7
	2.0
	150
	
	20
	Fdi
	1.4

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Sx, 
	1.0

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Bl, Cw
	1.0

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Others
	2.0

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ICHmk3 02 - WL
	1017459
	ICHmk3
	02* 
	Fdi  Pli
	Sx28 Bl
	1000
	500
	400
	
	7
	2.0
	150
	 
	20
	Pli
	1.4

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ICHmk3 03 - WL
	1017460
	ICHmk3
	03
	Fdi Pli
	Cw28 Sx28 Bl28 
	1000
	500
	400
	
	7
	2.0
	150
	 
	20
	Pli
	1.4

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.0

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ICHmk3 04 - WL
	1017461
	ICHmk3
	04
	Fdi32 Sx
	Bl Cw32,37 Pli
	1200
	700
	600
	
	7
	2.0
	150
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.4

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Others
	1.0

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	BCTS – mixedwood
	ICHmk3 04 mixed wd - WL
	1017462
	ICHmk3
	04
	Fdi32, Sx, Act, At, Ep
	Bl, Cw32,37   Pli
	1600
	1000
	800
	600
	7
	2.0
	150
	
	20
	Fdi
	1.4

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Sx, 
	1.0

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Bl, Cw
	1.0

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Others
	2.0

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ICHmk3 05 - WL
	1017463
	ICHmk3
	05
	Sx32 Pli
	Cw32,37Bl32
	1200
	700
	600
	
	7
	2.0
	150
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Others
	1.0

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS _ Mixedwood
	ICHmk3 05 mixed wd - WL
	1017464
	ICHmk3
	05
	Sx32, Pli, Act
	Cw32,37Bl32
	1600
	1000
	800
	600
	7
	2.0
	150
	
	20
	Pli, Act
	2.0

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Others
	1.0

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	BCTS even-aged
	ICHmk3 06 - WL
	1017465
	ICHmk3
	06
	Fdi32,34 Sx34 Cw32,34,37
	 Bl34 Pli34
	1200
	700
	600
	
	7
	1.6
	150
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.4

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	1.0

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	BCTS – Mixedwood
	ICHmk3 06 mixed wd - WL
	1017466
	ICHmk3
	06
	Fdi32,34 Sx34 Cw32,34,37, Act, Ep
	Bl34 Pli34
	1600
	1000
	800
	600
	7
	2.0
	150
	
	20
	Fdi
	1.4

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Sx, Cw
	1.0

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Bl
	1.0

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Others
	2.0

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ICHmk3 07 - WL
	1017467
	ICHmk3
	07
	Sx1,32 Cw1,32,37
	Bl1,32 Pli1
	1000
	500
	400
	
	7
	1.6
	150
	 
	20
	Pli
	1.4

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	 
	
	 
	 
	 
	 
	  
	 
	 
	 
	
	 
	 
	 
	 
	 
	 
	 

	BCTS – Mixedwood
	ICHmk3 07 mixed wd - WL
	1017469
	ICHmk3
	07
	Sx1,32 Cw1,32,37, Act
	Bl1,32 Pli1
	1200
	700
	600
	400
	7
	2.0
	150
	
	20
	Act
	2.0

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Pli
	1.4

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Others 
	0.8

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	BCTS even-aged
	ICHwk2 01 - WL
	1017470
	ICHwk2
	01
	Fdi Pli Sx
	Bl Cw37Hw37
	1200
	700
	600
	
	7
	2.0
	150
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.4

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Others
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ICHwk2 02 - WL
	1017471
	ICHwk2
	02* 
	Fdi  Pli
	Bl28 Hw28,37 
	1000
	500
	400
	
	7
	2.0
	150
	 
	20
	Pli
	1.4

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ICHwk2 03 - WL
	1017472
	ICHwk2
	03*
	Fdi Pli
	 Bl28 Atb
	1000
	500
	400
	
	7
	2.0
	150
	 
	20
	Pli
	1.4

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ICHwk2 04 - WL
	1017483
	ICHwk2
	04
	Fdi  Pli
	Hw37
	1200
	700
	600
	
	7
	2.0
	150
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.0

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Others
	1.0

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ICHwk2 05- WL
	1017485
	ICHwk2
	05
	Sx  Pli
	Cw37Bl 
	1200
	700
	600
	
	7
	2.0
	150
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ICHwk2 06- WL
	1017488
	ICHwk2
	06
	Sx32 Pli
	 Bl34 
	1200
	700
	600
	
	7
	2.0
	150
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Others
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ICHwk2 07 - WL
	1017492
	ICHwk2
	07
	Fdi1,32 Sx Cw32,37
	Bl Hw32,37 Pli
	1200
	700
	600
	
	7
	2.0
	150
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.4

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	1.0

	BCTS even-aged
	ICHwk2 08 - WL
	1017493
	ICHwk2
	08
	Sx1,32 Cw1,32,37
	Bl1,32 
	1000
	500
	400
	
	7
	2.0
	150
	 
	20
	All
	0.8

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	 
	 

	 
	
	 
	 
	 
	 
	 
	 
	 
	 
	
	 
	 
	 
	 
	 
	 
	 

	BCTS even-aged
	ICHwk4 01 - WL
	1017495
	ICHwk4
	01
	Fdi Pli Sx
	Bl Cw37Hw37
	1200
	700
	600
	
	7
	2.0
	150
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.4

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	1.0

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	BCTS – Mixedwood
	ICHwk4 01 mixed wd - WL
	1017497
	ICHwk4
	01
	Fdi, Pli, Sx, Act, At, Ep
	Bl Cw37Hw37
	1600
	1000
	8000
	600
	7
	2.0
	150
	
	20
	Pli, Act, At, Ep
	2.0

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Fdi
	1.4

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Others
	1.0

	
	
	
	 
	 
	 
	  
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ICHwk4 02 - WL
	1017499
	ICHwk4
	02* 
	Fdi  Pli
	Bl28 Hw28,37 
	1000
	500
	400
	
	7
	2.0
	150
	 
	20
	Pli
	1.4

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ICHwk4 03 - WL
	1017501
	ICHwk4
	03*
	Fdi Pli
	Sx28
	1000
	500
	400
	
	7
	2.0
	150
	 
	20
	Pli
	1.4

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ICHwk4 04 - WL
	1017503
	ICHwk4
	04
	Fdi32 Pli Sx28
	Bl28Hw32
	1200
	700
	600
	
	7
	2.0
	150
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.4

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ICHwk4 05 - WL
	1017504
	ICHwk4
	05
	Fdi Pli
	Hw37  
	1200
	700
	600
	
	7
	2.0
	150
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.4

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	1.0

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	BCTS – Mixedwood
	ICHwk4 05 mixed wd - WL
	1017505
	ICHwk4
	05
	Fdi, Pli, At, Ep
	Hw37
	1600
	1000
	800
	600
	7
	2.0
	150
	
	20
	Fdi
	1.4

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Hw
	1.0

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Others
	2.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	

	BCTS even-aged
	ICHwk4 06 - WL
	1017510
	ICHwk4
	06
	Sx32  Pli
	 Bl32 
	1200
	700
	600
	
	7
	2.0
	150
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS – Mixedwood
	ICHwk4 06 mixed wd - WL
	1017519
	ICHwk4
	06
	Sx32, Pli, Act
	Bl32
	1600
	1000
	800
	600
	7
	2.0
	150
	
	20
	Pli, Act
	2.0

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Sx, Bl
	1.0

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	BCTS even-aged
	ICHwk4 07 - WL
	1017529
	ICHwk4
	07
	Fdi1,32 Sx Cw32,37
	Bl Hw32,37 Pli
	1200
	700
	600
	
	7
	2.0
	150
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.4

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	1.0

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	BCTS – Mixedwood
	ICHwk4 07 mixed wd - WL
	1017538
	ICHwk4
	07
	Fdi1,32 Sx Cw32,37, Act, Ep
	Bl Hw32,37 Pli
	1600
	1000
	800
	600
	7
	2.0
	150
	
	20
	Fdi
	1.4

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Act, Ep, Pli
	2.0

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Others
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	ICHwk4 08 - WL
	1017539
	ICHwk4
	08
	Sx1,32 Cw1,32,37
	Bl1,32 Pli1 
	1000
	500
	400
	
	7
	1.6
	150
	 
	20
	Pli
	1.4

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	 
	 
	 
	 
	 
	 
	 
	 
	
	 
	 
	 
	 
	 
	 
	 

	BCTS – Mixedwood
	ICHwk4 08 mixed wd - WL
	1017540
	ICHwk4
	08
	Sx1,32 Cw1,32,37, Act
	Bl1,32 Pli1
	1200
	700
	600
	400
	7
	2.0
	150
	
	20
	Act
	2.0

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Pli
	1.4

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Others
	0.8

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	BCTS even-aged
	IDFdk3 01  - WL
	1017541
	IDFdk3
	01
	Fdi27,32 Pli
	Sx13,28 
	1200
	700
	600
	
	7
	2.0
	125
	 
	20
	Pli
	1.4

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Sx
	0.8

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS IDFdk3.Uneven Age:
Layer 1 
	IDFdk3 01 uneven  - WL
	1017542
	IDFdk3
	01
	Fdi27,32 Pli,
	Sx13,28
	600
	300
	250
	
	7
	0
	0
	 
	20
	Pli
	1.4

	Layer 2
	
	
	 
	 
	Fdi27,32 Pli
	Sx13,28
	800
	400
	300
	
	 
	2.0
	125
	 
	
	Fdi
	0.4

	Layer 3
	
	
	 
	 
	Fdi27,32 Pli
	Sx13,28
	1000
	500
	400
	
	 
	2.0
	125
	 
	
	Sx
	0.8

	Layer 4
	
	
	 
	 
	Fdi27,32 Pli
	Sx13,28
	1200
	700
	600
	
	 
	2.0
	125
	 
	
	 
	 

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	IDFdk3 02 - WL
	1017543
	IDFdk3
	02*
	Fdi27,28 Pli
	 
	800
	500
	500
	
	7
	2.0
	125
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Fdi
	0.8

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS IDFdk3  Uneven Age:  Layer 1 
	IDFdk3 02 uneven  - WL
	1017544
	IDFdk3
	02*
	Fdi27,32 Pli
	 
	300
	150
	150
	
	7
	0
	0
	 
	20
	Pli
	1.0

	Layer 2
	
	
	 
	 
	Fdi27,32 Pli
	 
	400
	200
	200
	
	 
	2.0
	125
	 
	
	Fdi
	0.4

	Layer 3
	
	
	 
	 
	Fdi27,32 Pli
	 
	600
	300
	300
	
	 
	2.0
	125
	 
	
	 
	 

	Layer 4
	
	
	 
	 
	Fdi27,32 Pli
	 
	800
	400
	400
	
	 
	2.0
	125
	 
	
	 
	 

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	IDFdk3 03 - WL
	1017545
	IDFdk3
	03*
	Fdi27,28 Pli28
	 
	800
	500
	500
	
	7
	2.0
	125
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Fdi
	0.8

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS IDFdk3 Uneven Age: Layer 1 
	IDFdk3 03 uneven  - WL
	1017546
	IDFdk3
	03*
	Fdi27,28 Pli28
	 
	300
	150
	150
	
	7
	0
	0
	 
	20
	Pli
	1.0

	Layer 2
	
	
	 
	 
	Fdi27,28 Pli28
	 
	400
	200
	200
	
	 
	2.0
	125
	 
	
	Fdi
	0.4

	Layer 3
	
	
	 
	 
	Fdi27,28 Pli28
	 
	600
	300
	300
	
	 
	2.0
	125
	 
	
	 
	 

	Layer 4
	
	
	 
	 
	Fdi27,28 Pli28
	 
	800
	400
	400
	
	 
	2.0
	125
	 
	
	 
	 

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	IDFdk3 04 - WL
	1017547
	IDFdk3
	04
	Fdi27,28 Pli28
	
	1000
	500
	500
	
	7
	2.0
	125
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Fdi
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	
	 

	BCTS IDFdk3 Uneven Age:  Layer 1 
	IDFdk3 04 uneven  - WL
	1017548
	IDFdk3
	04
	Fdi27,28 Pli28
	
	400
	200
	200
	
	7
	0
	0
	 
	20
	Pli
	1.0

	Layer 2
	
	
	 
	 
	Fdi27,28 Pli28
	
	600
	300
	300
	
	 
	2.0
	125
	 
	
	Fdi
	0.4

	Layer 3
	
	
	 
	 
	Fdi27,28 Pli28
	
	800
	400
	400
	
	 
	2.0
	125
	 
	
	 
	 

	 Layer 4
	
	
	 
	 
	Fdi27,28 Pli28
	
	1000
	500
	500
	
	 
	2.0
	125
	 
	
	 
	 

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	IDFdk3 05 - WL
	1017549
	IDFdk3
	05
	Fdi27 Pli
	
	1200
	700
	700
	
	7
	2.0
	125
	 
	20
	Pli
	1.4

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS IDFdk3  Uneven Age:  Layer 1 
	IDFdk3 05 uneven  - WL
	1017550
	IDFdk3
	05
	Fdi27 Pli
	
	600
	300
	300
	
	7
	0
	0
	 
	20
	Pli
	1.4

	Layer 2
	
	
	 
	 
	Fdi27,Pli
	
	800
	400
	400
	
	 
	2.0
	125
	 
	
	Fdi
	0.4

	Layer 3
	
	
	 
	 
	Fdi27 Pli
	
	1000
	500
	500
	
	 
	2.0
	125
	 
	
	 
	 

	Layer 4
	
	
	 
	 
	Fdi27 Pli
	
	1200
	700
	700
	
	 
	2.0
	125
	 
	
	 
	 

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	IDFdk3 06 - WL
	1017551
	IDFdk3
	06
	Fdi27,28 Pli
	
	1200
	700
	700
	
	7
	2.0
	125
	 
	20
	Pli
	1.4

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	
	 

	BCTS IDFdk3 Uneven Age:   Layer 1 
	IDFdk3 06 uneven  - WL
	1017552
	IDFdk3
	06
	Fdi27,28 Pli
	
	600
	300
	300
	
	7
	0
	0
	 
	20
	Pli
	1.4

	Layer 2
	
	
	 
	 
	Fdi27,28 Pli
	
	800
	400
	400
	
	 
	2.0
	125
	 
	
	Fdi
	0.4

	Layer 3
	
	
	 
	 
	Fdi27,28 Pli
	
	1000
	500
	500
	
	 
	2.0
	125
	 
	
	 
	 

	 Layer 4
	
	
	 
	 
	Fdi27,28 Pli
	
	1200
	700
	700
	
	 
	2.0
	125
	 
	
	 
	 

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	IDFdk3 07 - WL
	1017553
	IDFdk3
	07
	Fdi32 Pli Sx28
	
	1200
	700
	700
	
	7
	2.0
	125
	 
	20
	Pli
	1.4

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Sx
	0.8

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	IDFdk3 08 - WL
	1017554
	IDFdk3
	08
	Fdi1,32Pli Sx
	
	1200
	700
	700
	
	7
	2.0
	125
	 
	20
	Pli
	1.4

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Sx
	0.8

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	IDFdk3 09 - WL
	1017555
	IDFdk3
	09
	Sx1,32 
	Pli1 
	1000
	500
	400
	
	7
	1.6
	125
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Sx
	0.6

	 
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	IDFdk4 01 - WL
	1017556
	IDFdk4
	01
	Fdi27,32 Pli
	Sx13,28 
	1200
	700
	600
	
	7
	2.0
	125
	 
	20
	Pli
	1.4

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Sx
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS IDFdk4.Uneven Age:   Layer 1 
	IDFdk4 01 uneven  - WL
	1017557
	IDFdk4
	01
	Fdi27,32 Pli
	Sx13,28 
	600
	300
	250
	
	7
	0
	0
	 
	20
	Pli
	1.4

	Layer 2
	
	
	 
	 
	Fdi27,32 Pli
	Sx13,28 
	800
	400
	300
	
	 
	2.0
	125
	 
	
	Fdi
	0.4

	Layer 3
	
	
	 
	 
	Fdi27,32 Pli
	Sx13,28 
	1000
	500
	400
	
	 
	2.0
	125
	 
	
	Sx
	0.8

	Layer 4
	
	
	 
	 
	Fdi27,32 Pli
	Sx13,28 
	1200
	700
	600
	
	 
	2.0
	125
	 
	
	 
	 

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	IDFdk4 02 - WL
	1017558
	IDFdk4
	02*
	Fdi27,28 Pli28
	 
	800
	500
	500
	
	7
	2.0
	125
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Fdi
	0.8

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS IDFdk4  Uneven Age:  Layer 1 
	IDFdk4 02 uneven  - WL
	1017559
	IDFdk4
	02*
	Fdi27,32 Pli
	 
	300
	150
	150
	
	7
	0
	0
	 
	20
	Pli
	1.0

	Layer 2
	
	
	 
	 
	Fdi27,32 Pli
	 
	400
	200
	200
	
	 
	2.0
	125
	 
	
	Fdi
	0.4

	Layer 3
	
	
	 
	 
	Fdi27,32 Pli
	 
	600
	300
	300
	
	 
	2.0
	125
	 
	
	 
	 

	Layer 4
	
	
	 
	 
	Fdi27,32 Pli
	 
	800
	400
	400
	
	 
	2.0
	125
	 
	
	 
	 

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	IDFdk4 03 - WL
	1017560
	IDFdk4
	03*
	Fdi27, 28
	
	800
	500
	500
	
	7
	2.0
	125
	 
	20
	Fdi
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS IDFdk4 Uneven Age:   Layer 1 
	IDFdk4 03 uneven  - WL
	1017565
	IDFdk4
	03*
	Fdi27, 28
	
	300
	150
	150
	
	7
	0
	0
	 
	20
	Fdi
	0.4

	Layer 2
	
	
	 
	 
	Fdi27, 28
	
	400
	200
	200
	
	 
	2.0
	125
	 
	
	 
	 

	Layer 3
	
	
	 
	 
	Fdi27, 28
	
	600
	300
	300
	
	 
	2.0
	125
	 
	
	 
	 

	 Layer 4
	
	
	 
	 
	Fdi27, 28
	
	800
	400
	400
	
	 
	2.0
	125
	 
	
	 
	 

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	IDFdk4 04 - WL
	1017566
	IDFdk4
	04* 
	Fdi27,28 Pli28
	
	1000
	500
	500
	
	7
	2.0
	125
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Fdi
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	
	 

	BCTS IDFdk4 Uneven Age:   Layer 1 
	IDFdk4 04 uneven  - WL
	1017567
	IDFdk4
	04* 
	Fdi27,28 Pli28
	
	400
	200
	200
	
	7
	0
	0
	 
	20
	Pli
	1.0

	Layer 2
	
	
	 
	 
	Fdi27,28 Pli28
	
	600
	300
	300
	
	 
	2.0
	125
	 
	
	Fdi
	0.4

	Layer 3
	
	
	 
	 
	Fdi27,28 Pli28
	
	800
	400
	400
	
	 
	2.0
	125
	 
	
	 
	 

	 Layer 4
	
	
	 
	 
	Fdi27,28 Pli28
	
	1000
	500
	500
	
	 
	2.0
	125
	 
	
	 
	 

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	IDFdk4 05 - WL
	1017568
	IDFdk4
	05
	Fdi27,28 Pli
	
	1200
	700
	700
	
	7
	2.0
	125
	 
	20
	Pli
	1.4

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS IDFdk4  Uneven Age:   Layer 1 
	IDFdk4 05 uneven  - WL
	1017569
	IDFdk4
	05
	Fdi27,28 Pli
	
	600
	300
	300
	
	7
	0
	0
	 
	20
	Pli
	1.4

	Layer 2
	
	
	 
	 
	Fdi27,28 Pli
	
	800
	400
	400
	
	 
	2.0
	125
	 
	
	Fdi
	0.4

	Layer 3
	
	
	 
	 
	Fdi27,28 Pli
	
	1000
	500
	500
	
	 
	2.0
	125
	 
	
	 
	 

	Layer 4
	
	
	 
	 
	Fdi27,28 Pli
	
	1200
	700
	700
	
	 
	2.0
	125
	 
	
	 
	 

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	IDFdk4 06 - WL
	1017570
	IDFdk4
	06
	Pli
	Sx28,32
	1000
	500
	400
	
	7
	2.0
	125
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Sx
	0.6

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	
	 

	IDFdk4 Uneven Age:  Layer 1 
	IDFdk4 06 uneven - WL
	1017571
	IDFdk4
	06
	Pli
	Sx28,32
	400
	200
	200
	
	7
	0
	0
	 
	20
	Pli
	1.0

	Layer 2
	
	
	 
	 
	Pli
	Sx28,32
	600
	300
	250
	
	 
	2.0
	125
	 
	
	Sx
	0.6

	Layer 3
	
	
	 
	 
	Pli
	Sx28,32
	800
	400
	300
	
	 
	2.0
	125
	 
	
	 
	 

	 Layer 4
	
	
	 
	 
	Pli
	Sx28,32
	1000
	500
	400
	
	 
	2.0
	125
	 
	
	 
	 

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	IDFdk4 07- WL
	1017572
	IDFdk4
	07
	Fdi27 Pli
	
	1200
	700
	700
	
	7
	2.0
	125
	 
	20
	Pli
	1.4

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	IDFdk4 08 - WL
	1017573
	IDFdk4
	08
	Pli Sx32
	
	1000
	500
	500
	
	7
	2.0
	125
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Sx
	0.6

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	IDFdk4 09 - WL
	1017574
	IDFdk4
	09
	Fdi1,32 Pli Sx
	
	1200
	700
	700
	
	7
	2.0
	125
	 
	20
	Pli
	1.4

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Sx
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	IDFdk4 10 - WL
	1017575
	IDFdk4
	10
	Sx1,32
	 Pli1
	1000
	500
	400
	
	7
	1.6
	125
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Sx
	0.6

	 
	
	 
	 
	 
	 
	
	 
	 
	 
	
	 
	 
	 
	 
	 
	 
	 

	BCTS even-aged
	IDFxm 01a - WL
	1017576
	IDFxm
	01a
	Fdi27,28
	
	1200
	700
	700
	
	7
	2.0
	125
	 
	20
	All
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	IDFxm 01b - WL
	1017577
	IDFxm
	01b
	Fdi27,28 Pli
	
	1200
	700
	700
	
	7
	2.0
	125
	 
	20
	All
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	IDFxm 02 - WL
	1017578
	IDFxm
	02* 
	Fdi27,28
	
	1000
	500
	500
	
	7
	2.0
	125
	 
	20
	Fdi
	0.6

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	IDFxm 03 - WL
	1017579
	IDFxm
	03
	Fdi27,28 Pli
	
	1000
	500
	500
	
	7
	2.0
	125
	 
	20
	Pli
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Fdi
	0.6

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	IDFxm 04 - WL
	1017580
	IDFxm
	04
	Fdi27,28
	
	1000
	500
	500
	
	7
	2.0
	125
	 
	20
	Fdi
	0.6

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	IDFxm 05 - WL
	1017581
	IDFxm
	05
	Fdi27
	
	1200
	700
	700
	
	7
	2.0
	125
	 
	20
	Fdi
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	IDFxm 06 - WL
	1017582
	IDFxm
	06
	Fdi32
	
	1200
	700
	700
	
	7
	2.0
	125
	 
	20
	Fdi
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	IDFxm 07 - WL
	1017583
	IDFxm
	07
	Fdi
	
	1200
	700
	700
	
	7
	2.0
	125
	 
	20
	Fdi
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	IDFxm 08 - WL
	1017584
	IDFxm
	08
	Fdi32 Sx
	Pli
	1200
	700
	600
	
	7
	2.0
	125
	 
	20
	All
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	IDFxm 09 - WL
	1017585
	IDFxm
	09
	Pli1 Sx1
	
	1000
	500
	500
	
	7
	1.6
	125
	 
	20
	Pli
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Sx
	0.6

	 
	
	 
	 
	 
	 
	
	 
	 
	 
	
	 
	 
	 
	 
	 
	 
	 

	BCTS even-aged
	MSdc2 01 - WL
	1017586
	MSdc2
	01
	Pli Sx28
	Bl28 Fdi32
	1200
	700
	600
	
	7
	2.0
	125
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	MSdc2 02 - WL
	1017587
	MSdc2
	02* 
	Fdi28 Pli
	Bl28 Pa53
	1000
	500
	400
	
	7
	2.0
	125
	 
	20
	Pli
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	0.6

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	MSdc2 03 - WL
	1017588
	MSdc2
	03
	Fdi Pli
	Bl28 Pa53
	1000
	500
	400
	
	7
	2.0
	125
	 
	20
	Pli
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	0.6

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	MSdc2 04 - WL
	1017589
	MSdc2
	04
	Pli Sx28 
	 Bl28
	1200
	700
	600
	
	7
	2.0
	125
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	2.0
	125
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	MSdc2 05 - WL
	1017590
	MSdc2
	05
	Sx32 Pli1
	Bl32
	1200
	700
	600
	
	7
	2.0
	125
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	MSdc2 06 - WL
	1017591
	MSdc2
	06
	Sx32 Pli1
	 Bl32
	1200
	700
	600
	
	7
	2.0
	125
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	MSdc2 07 - WL
	1017592
	MSdc2
	07
	Sx Bl
	Pli1
	1200
	700
	600
	
	7
	2.0
	125
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	MSdc2 08 - WL
	1017593
	MSdc2
	08
	Sx1,32
	Bl1,32 Pli1,32
	1000
	500
	400
	
	7
	1.6
	125
	 
	20
	Pli
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	0.6

	 
	
	 
	 
	 
	 
	
	 
	 
	 
	
	 
	 
	 
	 
	 
	 
	 

	BCTS even-aged
	MSdv 01 - WL
	1017687
	MSdv
	01
	Pli Sx32
	Bl32
	1200
	700
	600
	
	7
	2.0
	125
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	MSdv 02 - WL
	1017688
	MSdv
	02* 
	Pli28
	
	1000
	500
	500
	
	7
	2.0
	125
	 
	20
	Pli
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	MSdv 03 - WL
	1017689
	MSdv
	03
	Pli
	Sx28, 32,Bl28, 32 
	1200
	700
	600
	
	7
	2.0
	125
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	MSdv 04 - WL
	1017690
	MSdv
	4,5
	Pli
	Sx28 Bl28
	1200
	700
	600
	
	7
	2.0
	125
	 
	20
	Pli
	1.0

	
	MSdv 05 - WL
	1017691
	 
	 
	 
	
	
	
	
	
	 
	2.0
	125
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	MSdv 06 - WL
	1017692
	MSdv
	6,7
	Pli Sx32
	Bl32
	1200
	700
	600
	
	7
	2.0
	125
	 
	20
	Pli
	1.0

	
	MSdv 07 - WL
	1017693
	 
	 
	 
	
	
	
	
	
	 
	2.0
	125
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	MSdv 08 - WL
	1017694
	MSdv
	08
	Sx32 Pli1,32
	Bl32
	1000
	500
	400
	
	7
	1.6
	125
	 
	20
	Pli
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	1.6
	125
	 
	
	Others
	0.6

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	MSdv 09 - WL
	1017695
	MSdv
	09
	Sx1,32
	Pli32 Bl32
	1000
	500
	400
	
	7
	1.6
	125
	 
	20
	Pli
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	1.6
	125
	 
	
	Others
	0.6

	 
	
	 
	 
	 
	 
	
	 
	 
	 
	
	 
	 
	 
	 
	 
	 
	 

	BCTS even-aged
	MSxv 01 - WL
	1017696
	MSxv
	01
	Pli Sx28,32
	Bl16,28,32
	1200
	700
	600
	
	7
	2.0
	125
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	MSxv 02 - WL
	1017697
	MSxv
	02
	Pli32
	
	1000
	500
	500
	
	7
	2.0
	125
	 
	20
	Pli
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	MSxv 03 - WL
	1017698
	MSxv
	03
	Pli
	
	1000
	500
	500
	
	7
	2.0
	125
	 
	20
	Pli
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	MSxv 04 - WL
	1017699
	MSxv
	04
	Pli Sx32
	Bl16,28,32
	1200
	700
	600
	
	7
	2.0
	125
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	MSxv 05 - WL
	1017700
	MSxv
	05
	Pli Sx32
	Bl32
	1200
	700
	600
	
	7
	2.0
	125
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	BCTS even-aged
	MSxv 06 - WL
	1017701
	MSxv
	06
	Pli Sx32
	Bl16,32
	1200
	700
	600
	
	7
	2.0
	125
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	MSxv 07 - WL
	1017702
	MSxv
	07
	Pli Sx32
	Bl16,32 
	1000
	500
	400
	
	7
	2.0
	125
	 
	20
	Pli
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	0.6

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	MSxv 08 - WL
	1017703
	MSxv
	08
	Sx1,32
	 Pli Bl1,16,32
	1000
	500
	400
	
	7
	1.6
	125
	 
	20
	Pli
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	0.6

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	MSxv 09 - WL
	1017704
	MSxv
	09
	Sx1,32
	Bl1,32 Pli1
	400
	200
	200
	
	7
	1.6
	125
	 
	20
	Pli
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	1.6
	125
	 
	
	Others
	0.6

	 
	
	 
	 
	 
	 
	
	 
	 
	 
	
	 
	 
	 
	 
	 
	 
	 

	BCTS even-aged
	SBPSdc 01 - WL
	1017705 
	SBPSdc
	01
	Pli Sx28
	Sb28
	1200
	700
	600
	
	7
	2.0
	150
	 
	20
	Pli
	1.4

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBPSdc 02 - WL
	1017706
	SBPSdc
	02* 
	Pli28
	
	1000
	500
	500
	
	7
	2.0
	150
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBPSdc 03 - WL
	1017707
	SBPSdc
	03
	Pli
	Sb4,15,28 Sx4,28
	1200
	700
	600
	
	7
	2.0
	150
	 
	20
	Pli
	1.4

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBPSdc 04 - WL
	1017708
	SBPSdc
	04
	Pli Sx
	Sb15
	1200
	700
	600
	
	7
	2.0
	150
	 
	20
	Pli
	1.4

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBPSdc 05 - WL
	1017709
	SBPSdc
	05
	Pli Sx2
	Sb15
	1000
	500
	400
	
	7
	1.6
	150
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	0.6

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBPSdc 06 - WL
	1017710
	SBPSdc
	06
	Pli Sx32
	Sb15
	1000
	500
	400
	
	7
	1.6
	150
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	0.6

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBPSdc 07 - WL
	1017711
	SBPSdc
	07
	Sx1,32 Pli1
	Sb1
	400
	200
	200
	
	7
	1.6
	150
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	0.6

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBPSdc 08 - WL
	1017712
	SBPSdc
	08
	Sx1,32
	 Pli1 Sb15
	1000
	500
	400
	
	7
	1.6
	150
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	0.6

	 
	
	 
	 
	 
	 
	
	 
	 
	 
	
	 
	 
	 
	 
	 
	 
	 

	BCTS even-aged
	SBPSmc 01 - WL
	1017713
	SBPSmc
	1,3
	Pli
	Sb Sx
	1200
	700
	600
	
	7
	2.0
	150
	 
	20
	Pli
	1.6

	
	SBPSmc 03 - WL
	1017714
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBPSmc 02 - WL
	1017715
	SBPSmc
	02*
	Pli
	Sb Sx
	1000
	500
	400
	
	7
	2.0
	150
	 
	20
	Pli
	1.2

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	0.6

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBPSmc 04 - WL
	1017716
	SBPSmc
	04
	Pli Sx32
	Sb 
	1000
	500
	400
	
	7
	1.6
	150
	 
	20
	Pli
	1.2

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	0.6

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBPSmc 05 - WL
	1017717
	SBPSmc
	05
	Sx1,32
	 Pli1 Sb53
	1000
	500
	400
	
	7
	2.0
	150
	 
	20
	Pli
	1.2

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	0.6

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBPSmc 06 - WL
	1017718
	SBPSmc
	06
	Sx1,32 Pli1
	Sb53
	1000
	500
	400
	
	7
	1.6
	150
	 
	20
	Pli
	1.2

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	0.6

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBPSmc 07 - WL
	1017719
	SBPSmc
	07*
	Pli1 Sx1,32
	 Sb1
	400
	200
	200
	
	7
	1.6
	150
	 
	20
	Pli
	1.2

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	0.6

	BCTS even-aged
	SBPSmk 01 - WL
	1017720
	SBPSmk
	01
	Fdi14,32 Pli Sx
	
	1200
	700
	700
	
	7
	2.0
	150
	 
	20
	Pli
	1.6

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Sx
	0.8

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS Mixedwood
	SBPSmk 01 mixed wd - WL
	1017721
	SBPSmk
	01
	Fdi14,32, Pli, Sx, At
	
	1600
	1000
	1000
	600
	7
	2.0
	150
	
	20
	Fdi
	1.0

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Pli
	1.6

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Sx
	0.8

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	At
	2.0

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	BCTS even-aged
	SBPSmk 02 - WL
	1017722
	SBPSmk
	02* 
	Fdi14,28 Pli
	Sx28
	1000
	500
	400
	
	7
	2.0
	150
	 
	20
	Pli
	1.2

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Fdi
	0.8

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Sx
	0.6

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBPSmk 03 - WL
	1017723
	SBPSmk
	03
	Fdi28 Pli
	
	1200
	700
	700
	
	7
	2.0
	150
	 
	20
	Pli
	1.6

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBPSmk 04 - WL
	1017724
	SBPSmk
	04
	Fdi14,28,32 Pli Sx28
	
	1200
	700
	700
	
	7
	2.0
	150
	 
	20
	Pli
	1.6

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBPSmk 05 - WL
	1017725
	SBPSmk
	05
	Fdi14,28 Pli Sx28
	
	1200
	700
	700
	
	7
	2.0
	150
	 
	20
	Pli
	1.6

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	BCTS even-aged
	SBPSmk 06 - WL
	1017726
	SBPSmk
	06
	Pli Sx
	
	1200
	700
	700
	
	7
	2.0
	150
	 
	20
	Pli
	1.6

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Sx
	0.8

	 
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS Mixedwood
	SBPSmk 06 mixed wd - WL
	1017727
	SBPSmk
	06
	Pli, Sx, Act, At
	
	1600
	1000
	1000
	600
	7
	2.0
	150
	
	20
	Pli
	1.6

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Sx
	0.8

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Act, At
	2.0

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	BCTS even-aged
	SBPSmk 07 - WL
	1017728
	SBPSmk
	07
	Sx1,32
	 Pli1 Bl1,32
	1000
	500
	400
	
	7
	1.6
	150
	 
	20
	Pli
	1.2

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	0.6

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBPSmk 08 - WL
	1017729
	SBPSmk
	08
	Sx1,32 Pli1
	Sb1
	400
	200
	200
	
	7
	1.6
	150
	 
	20
	Pli
	1.2

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	0.6

	 
	
	 
	 
	 
	 
	
	 
	 
	 
	
	 
	 
	 
	 
	 
	 
	 

	BCTS even-aged
	SBPSxc 01 - WL
	1017730
	SBPSxc
	01
	Pli
	
	1200
	700
	700
	
	7
	2.0
	150
	 
	20
	Pli
	1.4

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS SBPSxc 1A
	SBPSxc 01 1A - WL
	1017731
	SBPSxc
	01
	Pli
	Sx
	1200
	700
	600
	
	7
	2.0
	150
	 
	20
	Pli
	1.4

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Other
	0.8

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS SBPSxc 1B
	SBPSxc 01 1B - WL
	1017732
	SBPSxc
	01
	Pli
	Fdi, Sx
	1200
	700
	600
	
	7
	2.0
	150
	 
	20
	Pli
	1.4

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Other
	0.8

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBPSxc 02a - WL
	1017733
	SBPSxc
	02a 
	Fdi9,11,18,28 Pli
	
	1000
	500
	500
	
	7
	2.0
	150
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Fdi
	0.6

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBPSxc 02b - WL
	1017734
	SBPSxc
	02b 
	Pli
	
	1000
	500
	500
	
	7
	2.0
	150
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Fdi
	0.6

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBPSxc 02c - WL
	1018588
	SBPSxc
	02c* 
	Fdi9,11,18,28 Pli
	
	1000
	500
	500
	
	7
	1.6
	150
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Fdi
	0.6

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBPSxc 03 - WL
	1018589
	SBPSxc
	03
	Pli Sx32
	
	1000
	500
	500
	
	7
	2.0
	150
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Sx
	0.6

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBPSxc 04 - WL
	1018590
	SBPSxc
	04
	Pli Sx32
	
	1200
	700
	700
	
	7
	2.0
	150
	 
	20
	Pli
	1.4

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Sx
	0.8

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBPSxc 05 - WL
	1018591
	SBPSxc
	05
	Pli1 Sx1,32
	
	1000
	500
	500
	
	7
	1.6
	150
	 
	20
	Pli
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Sx
	0.6

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBPSxc 06 - WL
	1018592
	SBPSxc
	06
	Pli Sx32
	
	1000
	500
	500
	
	7
	1.6
	150
	 
	20
	Pli
	1.0

	 
	
	 
	 
	 
	 
	
	 
	 
	 
	
	 
	 
	 
	 
	 
	Sx
	0.6

	BCTS even-aged
	SBSdw1 01- WL
	1018593 
	SBSdw1
	01
	Fdi Pli Sx28
	Bl28, 53
	1200
	700
	600
	
	7
	2.0
	150
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.4

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	1.0

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	BCTS Mixedwood
	SBSdw1 01 mixed wd - WL
	1018594
	SBSdw1
	01
	Fdi, Pli, Sx28, At, Ep
	Bl28, 53
	1600
	1000
	800
	600
	7
	2.0
	150
	
	20
	Fdi
	1.4

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Sx
	1.0

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Others
	2.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBSdw1 02 - WL
	1018595
	SBSdw1
	02* 
	Fdi28 Pli
	
	1000
	500
	500
	
	7
	2.0
	150
	 
	20
	Pli
	1.4

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBSdw1 03 - WL
	1018596
	SBSdw1
	03
	Fdi27 Pli
	
	1200
	700
	700
	
	7
	2.0
	150
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.4

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBSdw1 04 - WL
	1018611
	SBSdw1
	04
	Fdi32 Pli Sx28
	
	1200
	700
	700
	
	7
	2.0
	150
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.4

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Sx
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBSdw1 05 - WL
	1018613
	SBSdw1
	05
	Fdi Pli Sx
	
	1200
	700
	700
	
	7
	2.0
	150
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.4

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Sx
	1.0

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBSdw1 06 - WL
	1018614
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	BCTS even-aged
	SBSmw 06 - WL
	1018688
	SBSmw
	06
	Fdi, Pli, Sx
	Bl
	1200
	700
	600
	
	7
	2.0
	150
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.4

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS Mixedwood
	SBSmw 06 mixed wd - WL
	1018689
	SBSmw
	06
	Fdi, Pli, Sx, At, Act
	Bl
	1600
	1000
	800
	600
	7
	2.0
	150
	
	20
	Fdi
	1.4

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Sx, Bl
	1.0

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Others
	2.0

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	BCTS even-aged
	SBSmw 07 - WL
	1018690
	SBSmw
	07
	  Sx32Pli
	Bl32
	1200
	700
	600
	
	7
	2.0
	150
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBSmw 08 - WL
	1018691
	SBSmw
	08
	Fdi32  Sx
	Bl, Pli
	1200
	700
	600
	
	7
	1.6
	150
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.4

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS Mixedwood
	SBSmw 08 mixed wd - WL
	1018692
	SBSmw
	08
	Fdi32, Sx, At, Act, Ep
	Bl, Pli
	1600
	1000
	800
	600
	7
	2.0
	150
	
	20
	Fdi
	1.4

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Sx, Bl
	1.0

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Others
	2.0

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	BCTS even-aged
	SBSmw 09 - WL
	1018693
	SBSmw
	09
	 Sx1,32
	Bl1,32 Pli1
	1000
	500
	400
	
	7
	1.6
	150
	 
	20
	Pli
	1.4

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	
	 

	BCTS even-aged
	SBSmw 10 - WL
	1018694
	SBSmw
	10*
	Pli1 Sx1,32 
	Sb 
	400
	200
	200
	
	7
	1.6
	150
	 
	20
	Pli
	1.4

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	 
	
	 
	 
	 
	 
	 
	 
	 
	 
	
	 
	 
	 
	 
	 
	 
	 

	BCTS even-aged
	SBSwk1 01 - WL
	1018695
	SBSwk1
	01
	Fdi17 Pli Sx
	Bl 
	1200
	700
	600
	
	7
	2.0
	150
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.4

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBSwk1 02 - WL
	1018696
	SBSwk1
	02* 
	Fdi17 Pli
	Bl Sx 
	1000
	500
	400
	
	7
	2.0
	150
	 
	20
	Pli
	1.4

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBSwk1 03 - WL
	1018697
	SBSwk1
	03
	Fdi4,17,32 Pli
	Sx32 
	1200
	700
	600
	
	7
	2.0
	150
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.4

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBSwk1 04 - WL
	1018698
	SBSwk1
	04
	Fdi Pli Sx28 
	Bl28
	1200
	700
	600
	
	7
	2.0
	150
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Fdi
	1.4

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBSwk1 05 - WL
	1018699
	SBSwk1
	05
	Pli Sx
	Bl 
	1200
	700
	600
	
	7
	2.0
	150
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBSwk1 06 - WL
	1018700
	SBSwk1
	06
	Pli Sx32
	Bl32
	1200
	700
	600
	
	7
	2.0
	150
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBSwk1 07 - WL
	1018701
	SBSwk1
	07
	 Pli Sx32
	Bl32
	1200
	700
	600
	
	7
	2.0
	150
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	Others
	1.0

	
	
	
	 
	 
	 
	
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBSwk1 08 - WL
	1018702
	SBSwk1
	08
	Sx Pli
	Bl
	1200
	700
	600
	
	7
	2.0
	150
	 
	20
	Pli
	2.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	1.0

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	
	 

	BCTS even-aged
	SBSwk1 09 - WL
	1018703
	SBSwk1
	09
	Sx1,32 
	Bl1 Pli1
	1000
	500
	400
	
	7
	1.6
	150
	 
	20
	Pli
	1.4

	
	
	
	 
	 
	 
	 
	
	
	
	
	 
	
	
	 
	
	Others
	0.8

	
	
	
	 
	 
	
	 
	
	
	
	
	 
	
	
	 
	
	 
	 

	BCTS even-aged
	SBSwk1 11 - WL
	
	SBSwk1
	11*
	 Pli1 Sx1,32
	Sb
	400
	200
	200
	
	7
	1.6
	150
	 
	20
	Pli
	1.4

	
	
	
	 
	 
	
	 
	
	
	
	
	 
	
	
	 
	
	Others
	1.0

	 
	
	 
	 
	 
	
	 
	 
	 
	 
	
	 
	 
	 
	 
	 
	 
	 


Table B
	Uneven-aged Stocking Standards* -- Single-tree and Group Selection 
	
	
	

	
	
	
	
	
	
	
	
	

	Col. 1
	Col. 2
	Col. 3
	Col. 4
	Col. 5
	
	Col. 1
	Col. 2
	Col. 3
	Col. 4
	Col. 5

	Target from
	Layer**
	 Stocking*** 
	 
	 
	 
	Target from
	Layer**
	 Stocking*** 
	 
	 

	Table A standards
	 
	Target pa
	MIN pa
	MIN p
	 
	Table A standards
	 
	Target pa
	MIN pa
	MIN p

	(stems/ha)
	 
	(well-spaced/ha)
	 
	(stems/ha)
	 
	(well-spaced/ha)

	 
	 
	
	
	
	 
	
	 
	
	
	 

	1200
	1
	600
	300
	250
	 
	800
	1
	300
	150
	150

	 
	2
	800
	400
	300
	 
	
	2
	400
	200
	200

	 
	3
	1000
	500
	400
	 
	
	3
	600
	300
	300

	 
	4
	1200
	700
	600
	 
	
	4
	800
	400
	400

	 
	 
	
	
	
	 
	
	 
	
	
	 

	1000
	1
	400
	200
	200
	 
	600
	1
	300
	150
	150

	 
	2
	600
	300
	250
	 
	
	2
	400
	200
	200

	 
	3
	800
	400
	300
	 
	
	3
	500
	300
	300

	 
	4
	1000
	500
	400
	 
	
	4
	600
	400
	400

	 
	 
	
	
	
	 
	
	 
	
	
	 

	900
	1
	400
	200
	200
	 
	400
	1
	200
	100
	100

	 
	2
	500
	300
	250
	 
	
	2
	300
	125
	125

	 
	3
	700
	400
	300
	 
	
	3
	300
	150
	150

	 
	4
	900
	500
	400
	 
	
	4
	400
	200
	200

	 
	 
	 
	 
	 
	 
	 
	 
	 
	 
	 

	
MIN - minimum


	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	


	Conifer Tree Species
	Footnote #
	Footnote
	Footnote #
	Footnote

	"Ba" means amabilis fir;
	1
	elevated microsites are preferred
	46
	restricted to area north of the Dean Channel

	"Bg" means grand fir;
	2
	suitable on thick forest floors
	47
	risk of balsam wooly adelgid

	"Bl" means subalpine fir;
	3
	restricted to coarse-textured soils
	48
	risk of heavy browsing by deer

	"Bp" means noble fir;
	4
	restricted to medium-textured soils
	49
	applies only to rust resistant, Planted stock.

	"Cw" means western red cedar;
	5
	footnote retired
	50
	restricted to sites where the species occurs as a 

	"Fdi" means Douglas-fir;
	6
	restricted to nutrient-very-poor sites
	
	major species in a pre-harvest, natural stand

	"Hm" means mountain hemlock;
	7
	restricted to nutrient-medium sites
	51
	restricted to areas with proven Pli performance

	"Hw" means western hemlock;
	8
	restricted to steep slopes
	52
	restricted to sheltered microsites with deep soil

	“Lt” means tamarack;
	9
	restricted to southerly aspects
	53
	minor component

	"Lw" means western larch;
	10
	restricted to northerly aspects
	54
	risk of unsuccessful release of advance regeneration

	“Pa” means whitebark pine;
	11
	restricted to crest slope positions
	55
	acceptable in sx-sm portion of site series

	"Pli" means lodgepole pine;
	12
	suitable on cold air drainage sites
	

	"Pw" means white pine;
	13
	restricted to upper elevations of biogeoclimatic unit
	#
	Broadleaf Management Constraints

	"Py" means ponderosa pine;
	14
	restricted to lower elevations of biogeoclimatic unit
	

	“Sb” means black spruce;
	15
	restricted to northern portion of biogeoclimatic unit in region
	a
	productive, reliable, and feasible regeneration option

	“Se” means Engelmann spruce;
	16
	restricted to southern portion of biogeoclimatic unit in region
	b
	limited in productivity, reliability and/or feasibility

	"Ss" means Sitka spruce;
	17
	restricted to western portion of biogeoclimatic unit in region
	

	“Sw” means white spruce;
	18
	restricted to eastern portion of biogeoclimatic unit in region
	

	"Sx" means hybrid spruce or interior spruce;
	19
	restricted, not in Queen Charlotte Islands
	

	"Sxs" means hybrid Sitka spruce;
	20
	restricted, not near outer coast
	

	
	21
	restricted to mainland
	

	“Sxw” means hybrid white spruce;
	22
	restricted to southern Gardner Canal-Kitlope area
	

	"Yc" means yellow cedar.
	23
	restricted to trial use
	

	
	24
	suitable (as a major species) in wetter portion of biogeoclimatic unit
	

	
	
	
	

	
	
	
	


	Broadleaf Tree Species
	Footnote #
	Footnote
	

	“Acb” means balsam poplar;
	25
	suitable on sites lacking salal
	

	“Act” means black cottonwood;
	26
	suitable minor species on salal-dominated sites
	
	*  Avoid Logging
	
	
	

	“At” means trembling aspen;
	27
	partial canopy cover required for successful establishment
	
	
	
	
	
	
	

	“Dr” means red alder;
	28
	limited by moisture deficit
	
	
	

	“Ep” means common paper birch;
	29
	risk of heavy browsing by moose
	
	
	

	“Mb” means bigleaf maple;
	30
	risk of porcupine damage
	
	
	
	
	

	“Ra” means arbutus;
	32
	limited by growing-Season frosts
	
	

	
	33
	footnote retired and replaced with footnote 'a'
	
	
	
	
	

	
	34
	risk of snow damage
	
	
	
	
	
	
	

	
	35
	risk of weevil damage
	
	“Biogeoclimatic unit” or “BGC classification” means

	
	36
	suitable major species on salal-dominated sites
	
	the zone, subzone, variant and site Series described 

	
	37
	risk of heart rots
	
	in the most recent field guide published by the Ministry 

	
	38
	footnote retired
	
	of Forests for the identification and interpretation of 

	
	39
	avoid exposed and windy sites
	
	ecosystems, as applicable to a harvested area.

	
	40
	risk of redheart
	
	“MIN or “Min” means minimum.

	
	41
	limited by poorly drained soils
	
	
	
	
	
	
	

	
	42
	restricted to fresh soil moisture regimes
	
	
	
	
	
	
	

	
	43
	suitable on mainland coast only (QCI only)
	
	
	
	
	
	
	

	
	44
	suitable in areas with stronger maritime influence
	
	
	
	
	
	
	

	 
	45
	suitable in areas with stronger continental influence
	 
	 
	 
	 
	 
	 
	 


	**Stand Layer Definition
	
	
	
	
	

	
	
	
	
	
	
	

	Layer 1
	Mature
	
	trees >= 12.5 cm dbh

	Layer 2
	Pole
	
	trees 7.5 cm to 12.4 cm dbh

	Layer 3
	Sapling
	
	trees >= 1.3 m height to 7.4 cm dbh

	Layer 4
	Regeneration
	trees < 1.3 m height



In addition to the Stocking Standards Tables, the following applies:

1) Form and Vigor

Regeneration and free growing surveys will be conducted by accredited surveyors.  Trees assessed as well spaced and free growing will meet the form, vigor and damage criteria of the day.
2) Uneven-aged Management:
The uneven-aged stocking standards in the tables will be applied in situations where uneven-aged management, following harvest, is anticipated (Including; Mule Deer Winter Range, Cariboo Habitat, Uneven-aged Fir stands, salvage in mixed species stands).
Where an appropriate uneven-aged stocking standard does not already appear on Table A: Stocking Standards Table, Table B: Uneven-aged Stocking Standards table may be applied.

For Uneven-aged Fir stands, Douglas Fir will be considered Free Growing at 40cm height.

For Uneven-aged stands, there will be no minimum inter-tree distance applied to Layer 1 and the brush/conifer ratio will not apply to Layer 1 trees.

Where 12 months has past since harvest start, in Uneven-aged stands, Regen Delay and Free Growing may be declared at the same time, irregardless of age, if free growing standards are met.

3) Broadleaf:

Broadleaf trees reserved from harvest are not to be considered competing at time of free growing evaluation.  
Broadleaf is defined as: balsam poplar, black cottonwood, trembling aspen, red alder and common paper birch.
Shrubs species managed for wildlife values or erosion control are to be considered non-deleterious at the time of free growing evaluation.  Rose, soopalallie and dwarf shrubs will not be considered competing vegetation at the time of free growing evaluation.
4) Mixed Wood Stocking Standards:

For the purposes of evaluating stocking and free growing in mixed conifer and broadleaf stands managed for oriented strand board, sawlog production or landscape-level biodiversity objectives, mixed wood stocking standards, as listed in the stocking standard table may be used.  Mixed wood stocking standards are listed in the stocking standard table for the following ecosystem associations:

ICHmk3: 01, 04, 05, 06, 07


ICHwk4: 01, 05, 06, 07, 08


SBSdw1: 01, 06, 07


SBSdw2: 01, 08, 09


SBSmh: 01, 05, 06, 07, 08, 09


SBSmw: 01, 06, 08

SBPSmk: 01, 06

The mixed wood stocking standards for the above ecosystem associations include a minimum number of preferred conifer stems per hectare in addition to minimum number of preferred species per hectare.  In mixed wood stands, broadleaf trees not tallied as well-spaced free growing trees, will be considered “competing vegetation” for the purpose of assessing the free growing status of the coniferous crop trees, unless Section 2) above applies.
An acceptable hardwood crop tree must:

· Be at least 2.0 m in height and the tree pith must not be laterally displaced more than 30 cm, from the location of the root-crown pith

· not originate from a cut stump
.

· have at least one live leader
.

· not have a wound that is greater than 10% of the stem circumference nor is greater than 10% of the total length of the stem.
.

· not have any fungal infections or insect infestations affecting tissues below the bark surface, visible without destructive sampling
.

· not be browsed so as to limit its ability to become a crop tree.

5) Lodgepole Pine Dwarf Mistletoe:

Where a lodgepole pine dwarf mistletoe control treatment has been carried out post harvest to the 30 cm standard, mistletoe will be considered non-deleterious at the time of free growing.

6) Stand Density:

The maximum countable stocking, at the time of free growing declaration, for lodgepole pine leading stands where pine is > 80 percent of the inventory is 25,000 stems per hectare.  All other species and mixed pine stands where pine is less than 80 percent of the inventory will have a maximum of 10,000 countable stems per hectare at the time of free growing declaration.

7) Stratum Size:

The minimum stratum size for the purpose of assessing stocking levels will be 1.0 ha.

The minimum stratum size for the purposes of assessing stand density, deciduous competition, forest health or minimum heights at the time of free growing will be 2.0 ha.

Unlogged, residual patches > 0.25 ha will not be considered part of the Net Area to be Reforested.

Openings less than 1.0 ha will not be subject to free growing obligations.

8) Free Growing Dates

The late free growing date for all standard units will be 20 years.  There will be no stated early free growing date.  Standard Units will be assessed for free growing when free growing stocking standards are met, irregardless of age.
9) Post Spacing Densities

Appropriate post spacing minimum and maximum densities will be determined site specifically based on a professional evaluation which considers a variety of factors including crop tree species, health and vigour, site characteristics and target timber product.
10)
Reduced Minimum Inter-tree Distance and/or Stocking Standards
A two-metre minimum inter-tree distance is suitable for most sites, however, a reduced minimum inter-tree distance and/or reduced stocking standards may be appropriate for sites where plantable spots are limited by site characteristics, site condition, where a clumpy stem distribution is a normal, desirable characteristic or there is a significant risk of damage to planted or natural trees.  Examples of situations where a reduced minimum inter-tree distance and/or a reduction in the stocking standards may be appropriate include:

•
hygric or wetter sites

•
very rocky sites

•
areas where a silviculture treatment has failed due to high levels of grazing damage

•
very harsh sites where protected microsites are critical (e.g. shade, snowcreep)

•
sites with a significant number of large wildlife trees (e.g. 50 uniformly distributed trees per hectare)

•
riparian areas with a high residual component

•
sites where stump avoidance strategy is employed to manage root rot.

•
cluster planting (e.g. grizzly bear habitat)

•
partial cut area with an abundance of residual regeneration.
11)
Low Site Index

Where the site index on an SBPSxc 01 site is 12 or lower, the minimum free growing height will be reduced to 1.0 metres.
12) Stocking Standard Table A

ESSFxv2 01:  Bl as preferred
SBPSxc 01 (1A): Sx as acceptable

SBPSxc 01 (1B): Fdi and Sx as acceptable

The above acceptable and preferred species in the associated biogeoclimatic zones will only be acceptable and/or preferred well spaced and/or free growing stems where a qualified professional has determined that these species are likely to form a commercial crop tree. 

 Regeneration delay  and Free Growing can be met 12 months following harvest if the residual stand has no significant damage or pest problems and meets minimum stocking standards.  





*** pa - preferred and acceptable species       p - preferred species��Preferred and acceptable species and "Target from Table A standards' are as specified in Table A by biogeoclimatic ecosystem classification (BEC) site series.








� Stems originating from the sides or cut surface of stumps are very susceptible to breakage at the coppice point


�The objective is that the tree has a single stem that will develop into a healthy crop tree. Accordingly, a healthy, free growing aspen tree must have an identifiable live leader. It is not important if a portion, but not all, of the leader is browsed or killed for example by venturia blight. There is no agreement on a minimum leader length of a healthy aspen tree and as a result no minimum length is prescribed. 


� This criterion is modified from the conifer criterion, and threshold percent values are chosen subjectively. Research is needed to determine more exactly the size of an open wound at free growing assessment that is likely to limit the development of a healthy crop tree. A wound is defined as an injury in which the cambium is dead or completely removed from the tree exposing the sapwood. Measure the wound across the widest point of the exposed sapwood.  Healed-over wounds (= scars) are acceptable. Causes of mechanical damage to aspen commonly include gnawing by beaver, cattle, deer, elk or moose; logging activities; or wind throw scraping. Fire or sunscald damage can also cause wounds. Injury of young aspen stems is considered an important entry court for decay organisms. Injury of mature aspen is a lesser concern since the resulting potential damage of decays before harvesting would likely be much less.


� Visible stem infections include cyptospora canker or sooty-bark canker, and visible insect infestations, poplar borer. The significance of some diseases, such as armillaria root disease, to aspen is unknown or uncertain, and several cannot be feasibly identified by visual features during free growing surveys.
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