TSL TA1442 – WIA3E
Harvest Plan
ARCHAEOLOGICAL /CULTURAL HERITAGE:
This block is within the identified traditional territory of the Secwepemc Nation.  The consultation process has been followed.  Simpcw has completed an Office Review and determined that a Preliminary Field Review (PFR) and a Cultural Heritage Assessment are required.
A general management recommendation from Simpcw is to provide increased riparian protection on NCDs.  A 5m MFZ has been established on portions of NCD-4, NCD-5, NCD-10 and NCD-11.  Refer to the Harvest Plan and Support Document for specific details on each riparian feature associated with this block.
Forest management practices will cease and a representative from BCTS will be immediately notified if additional features of cultural or archaeological significance are discovered during operations.
LEAVE TREES AND BIODIVERSITY
Dispersed Retention:
HU’A’:
Where safe to do so within the block, reserve:
• 20% of the live hemlock stems 47.5cm dbh and greater (6-7 stems/ha or 1.44-1.60m2/ha)
Where operationally feasible and safe to do so, reserve 3-5 cut snags per hectare. Snags should be between 1.5m to 3.0m in height for biodiversity and cavity nesting habitat.
WILDLIFE
Migratory Bird Strategy:
WIA3E is located in the contiguous Moderately High Migratory Bird Risk polygon.  
To reduce Incidental Take for Migratory Birds, the following Beneficial Management Practices (BMPs) may be implemented during harvesting activities:
Management Practice Categories (from Appendix D Beneficial Management Practices Summary):
PL2 (Planning): Patch/edge retention around biodiversity anchors.  Refer to the Stand Level Biodiversity and Leave Tree Sections in the Site Plan for reserve trees in the block (DoP 2).
LO4 (Layout): Retention of WTRAs, WTs and Stub snags for cavity nesting birds.  Refer to the Stand Level Biodiversity and Leave Tree Sections in the Site Plan for reserve trees in the block (DoP 2).
SO1: Scheduling high risk blocks outside the nesting period.  Since WIA3E is located in the contiguous Moderately High Migratory Bird Risk polygon, this action may be required to sufficiently reduce the risk of Incidental Take (DoP 3).
SO4 (Strategic Operations): Chance encounters during harvesting activities where an active nest occurs.  If an active nest is detected, stop work and contact a BCTS supervisor.  
Where operationally feasible, reserve area around the detected nest for protection or delay harvesting outside of the period for nesting (DoP 1).
Harvesting and Road Construction Activities within the Restricted Period 2 (Area 2, May 15 to July 20):  All harvesting and roads within WIA3E are located in the contiguous Moderately High Migratory Bird Risk polygon.  WIA3E (Harvesting and Road Construction activities) may be implemented during the Restricted Period 2 if two or more of the BMPs that have DoP 2 designation for the site have been applied.  To further reduce the risk of incidental take, the licensee should schedule operations outside the nesting period.
SLOPES
SU-1 slopes range from 9-50% (average 23%).  
Approved safe work procedures must be followed on steep slopes.  See Harvest Plan map for locations.
CWD
The Nicola Thompson Fraser Sustainable Forest Management Plan (2011) requires consideration of coarse woody debris (CWD) to be retained on site postharvest.  Current preharvest levels are ~10-20m3/ha.  It is expected that through standard harvesting practices a minimum of 20m3/ha will be left on site post-harvest (existing CWD plus decay, waste and breakage). This strategy will meet the minimum requirements and will be consistent with FPPR Section 68(1)(b) and/or the KLRMP.
SOILS
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Harvesting should be conducted on a snowpack, frozen ground or during dry soil conditions to reduce the risk of soil disturbance.  
RIPARIAN FEATURES
This block is not located in a Community Watershed
	Riparian I.D and (Class)
	RMZ Width
(m)
	RRZ (m)
	Stream 
Crossing/Yarding
	Leave Trees
Species, BA or SPH Retained
	Comments


	NCD-3, 5, 9, 11
(NCD)
	0
	0
	Yes
	Within the 5m MSZ, reserve understory brush species to the fullest extent practicable.
	NCD centerlines are marked with red NCD ribbon.

	NCD-4, 5, 10, 11
(NCD)
	0
	0
	No
	Reserve all understory brush, advanced regeneration and nonmerchantable trees within the 5m MFZ to the fullest extent practicable.
	NCD centerlines are marked with red NCD ribbon.  Portions of these NCDs are also marked with a minimum 5m MFZ adjacent to the NCD.

	S6-1, S6-2
(Small S6)
	20
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	No
	Leave trees are outside of the block boundary.
	Streams are more than 20m outside of the harvest boundary.

	S6-L-1
(Large S6)
	15
	10
	No
	Leave trees are outside of the block boundary.
	Stream is more than 20m outside of the harvest boundary.


DEACTIVATION/REHABILITATION
All proposed landings, road CL WIA3E.01 and bladed skid trails are temporary access structures.  Temporary access structures will be deactivated or rehabilitated following harvest completion.  All structures will be removed.  Water bars and cross ditches will be established where necessary and slopes will be recontoured where required. 
OTHER
Harvesting:
This block is designed for ground skidding.  There are existing trails from previous logging history within the block. Utilize these trails first where practicable before constructing any new trails.  Trails outside of the harvest area are not to be used and are not covered under this site plan.
Trans Mountain Pipeline:
TMPL would like to be contacted two weeks prior to harvesting and road construction activities as the Licensee and TMPL may be sharing Smoke Creek FSR.
Contact:  Maria Frankova:  Telephone: 604-268-3094;  Email:  maria_frankova@transmountain.ca
BC Hydro:
BC Hydro Transmission Line crosses over existing Roads CL8090.01 and CL8090.02.  Licensee is to follow BC Hydro SOPs while conducting harvest operations and hauling under transmission lines. 
BC HYDRO: SPECIAL CONDITIONS:
1. A BC Hydro transmission line is adjacent to the southwest boundary of the block.  Where road construction or harvest activities are adjacent to a BC Hydro transmission line, the Licensee will contact BC Hydro 2-4 weeks prior to the commencement of activities.  If required, the two parties will meet jointly to conduct an onsite prework meeting to review the site and complete a sign-off.
2. Logging and felling of trees near powerlines outside the Limits of Approach (LOA) shall abide by the Occupational Health and Safety Regulations.  Any trees that may be felled within the LOA will need to be done in accordance with BC Hydro's guidelines.
3. Also, any such work must be performed under supervision of a qualified electrical worker (Certified Utility Arborist - CUA) who is onsite.  The CUA will conduct authorized felling, removing, topping or pruning of any trees that may fall within the LOA or may fall and damage electrical structures or guylines.  The Licensee is to contact Jason LaBonte, Transmission Vegetation Coordinator, at 250-371-6926 or jason.labonte@bchydro.com for further information.
4. Logging adjacent to the cleared BC Hydro Right of Way (ROW) must ensure that there are no residual trees left standing along the ROW edge of the block postharvest.
Trapper:
Where operationally feasible and safe to do so within the block, reserve one debris pile per hectare (approximately 3m x 3m in size) postharvest to accommodate small fur-bearing animals.
Mike Wiegele Helicopter Skiing (MWHS):
Licensee must contact MWHS two weeks prior to start of industrial activities.  MWHS uses the Smoke Creek FSR to access their ski area.
Contact Matic Vecko, General Manager; Office: 250-673-2415. Cell: 778-915-0644; Email: matic@wiegele.com
