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	Ministry of
Forests,
Lands and Natural Resource Operations

	Road Layout and Design Criteria


Forest Stewardship Plan:  BCTS Merritt TSA FSP (commencing July 1, 2018).                    
Mapsheet: 092H026/027      Date:  December 30, 2019
Road Name and Number:  ME3600.19, ME3600.20, and ME3600.21, 
	SECTION (station  - station)


	ME3600.19 (0+000 – 
0+900)
	ME3600.20
(0+000 – 0+658)
	ME3600.21
(0+000 – 0+753)
	

	New Construction                            (C)
	C
	C
	C
	

	Upgrade                                           (U)
	n/a
	n/a
	n/a
	

	Road type – Operational                  (O)
	O
	O
	O
	

	Road Type – On-block                    (B)
	n/a
	n/a
	n/a
	

	Community watershed
(Y/N)
	N
	N
	N
	

	Likelihood of landslides (L or M/H)
	L
	L
	L
	

	Within a Riparian Management Area (Y/N)
	Y
	N
	N
	

	Average clearing width 
(m)
	20
	20
	20
	

	Subgrade width (m)
	5
	5
	5
	

	Finished road width  
(m)
	5
	5
	5
	

	Ditch depth in other material 
(m)
	0.3
	0.3
	0.3
	

	Ditch depth in rock 

(m)
	0.3
	0.3
	0.3
	

	Usable turnout length/width 
(m)
	20m X 8m
	20m X 8m
	20m X 8m
	

	Turnouts:  intervisible
(Y/N)
	Y
	Y
	Y
	

	Turnouts:  minimum # per km
	3
	3
	3
	

	Min. Curve radius  
(m)
	35
	35
	35
	

	Max. Fav. Sustained grade  
(%)
	24
	24
	24
	

	Max. Adv. Sustained grade 
(%)
	-14
	-14
	-14
	

	Max. Fav. Short pitch grade 
(%)
	24
	24
	24
	

	Max. Adv. Short Pitch grade  
(%)
	-14
	-14
	-14
	

	Switchback Maximum gradient (%)
	20
	20
	20
	

	Professional prescriptions or assessments attached  

(Y/N)
	N
	N
	N
	

	Stabilizing required of road surface, with rock ballast or pit-run gravel (Y/N)
	Y
	Y
	Y
	

	Stumps left in place  
(Y/N)
	Y
	Y
	Y
	

	Disposal of slash/debris          (Y/N)
	Y
	Y
	Y
	

	
End haul                            (Y/N)
	N
	N
	N
	

	
Bury                                  (Y/N)
	N
	N
	N
	

	
Pile                                    (Y/N)
	N
	N
	N
	

	Organics in fill
            (Y/N)
	Y
	Y
	Y
	

	Construction survey
(Y/N)
	N
	N
	N
	

	Full bench construction   (Y/N)   (end hauling)
	N
	N
	N
	

	Minimum cross drain culvert size (round mm)
	600
	600
	600
	

	Other shapes (opening size mm X mm)
	
	
	
	

	Other:  Specify
	
	
	
	


Comments:
15
1

