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	BCTS Timber Sale Planning Safety
Checklist 18-1



The purpose of this checklist is to confirm that the required steps in the timber sale planning process as they relate to safety have been considered and integrated into the licence document or tender.
	DATE: JANUARY 15, 2021

	Timber Sale Licence #: TA0904-3

	BCTS Representative:

	Safety Considerations
[image: BD21301_] = Applicable    |_|= Not applicable
	COMMENTS

	Any Known Hazards (on-site / adjacent)
[bookmark: Check1]|X| Overhead hazards (snags/power lines)
|_| Previous activities such as road building have not created hazards such as unstable fill slopes, rocks or log decks that will effect harvesting?
|X| Steep Slopes  (+35% for ground based harvesting) information to be provided to prospective licensees to support their harvest planning such as: 
· Slopes that exceed 35%
· Long pitches of continuous slope 
· Terrain Stability Features e.g. fracture rock formation
· Ground Roughness e.g. hummocks, depressions steep, ravines
· Soil Conditions e.g. soil depth, exposed rock, loose gravels or soft mud.  
· Timber size and quality 
· Slopes or benches less than 35% but located above areas of greater slope.    
|_| Dangerous Terrain (gullies, ridges, cliffs)
|_| Identified Terrain Assessment safety considerations
|_| Unstable Surfaces (wet, soft)
|_| Wind throw / Heavy Slash
|X| Road Hazards (Road grades exceeding 18%).
|_| Road Excavation hazard (road sections in terrain >33% + anticipated cutbanks >6m in height + any other area that shows sign of instability). 
|_| Road Construction Initiated Landslides Hazards (signs of instability, broken rock, transition zones).
|X| Wildlife 
|_| Mines / Electrical / Pipelines 
|X| Other Risks / Hazards on site / adjacent / Root rot centres or infection levels
	Overhead hazards: This block has been damaged by wildfire of varying severity. In areas of greater burn severity, tree roots have been burnt out rendering trees highly unstable. There is a high hazard of sudden tree fall. Workers are to stay in machinery when working in such areas. Do not take breaks out of equipment in highly damaged areas. Monitor winds as risk of tree fall increases with increasing wind speeds. 

In areas of greater burn severity, trees may be structurally compromised and may break suddenly creating widowmakers that pose high hazard to workers. 

Steep Slopes: Short pitches of >35% occur in the block.. Prior to any machinery working on slopes exceeding the manufacturer recommended limit or if not available (>35%), a steep slope hazard assessment must be completed and documented by qualified personel. 
Large boulders are present and could dislodge if disturbed. Workers must not work downslope of such hazards where machinery is working above. 

Heavy Windthrow: Windthrow is present in the block.

Road Hazards: Danger trees occur along all access routes for this block. Danger trees are to be removed where they can strike landings, decking areas. Prior to operations, the harvesting supervisor should check access routes for downed trees blocking roads and ensure they are cleared. 

At the start of the Bear West FSR, a steep grade with narrow width occurs. While this pitch is accessible for logging trucks, drivers must exercise extreme caution when coming down loaded as there is a tight corner with steep dropoff. This should not be driven in icy or slippery muddy conditions. 

The Bear Main accesses the Bear Lake Recreation site. Public traffic is possible. Signage indicating that active falling and hauling are taking place are to be posted at the start of the Bear Main FSR and at the entry of the work area. 

Wildlife: Wildlife may frequent burns for foraging regrowth.  


	Term
|X| Adequate time to complete work given seasonal and access considerations?
	No conflicts anticipated. 


	Access 
|X| Has access route been assessed for hazards?
|_| Is their a hazard mitigation strategy in place that will be enacted prior to worker exposure?
|X| Will access routes accommodate the nature of traffic?
(See Checklist 23-1 for more comprehensive guidance)




	[bookmark: _GoBack]Access route will need to be checked for downed trees blocking the route and danger trees along roadways removed.  

	Safety Considerations
[image: BD21301_] = Applicable    |_|= Not applicable
	COMMENTS

	Adjacent Operations
|X| Are there conflicts with adjacent operations relative to timing or hazards (major licensees, salvage, silviculture, other industrial or public operations, phase congestion)?

	No conflicts anticipated. 

	
Site Plan and harvest systems:
|_| Have the proposed plans been reviewed with consideration toward worker safety?
|X| Have all known hazards been documented (high retention, wind throw, snags, unstable slopes, steeps slopes)?
	Known safety hazards have been identified, and where applicable indicated on maps. Slopes >35% are indicated on the harvest plan maps. 

	ESSENTIAL ELEMENTS
	COMMENTS

	Other Factors:
	

	
	

	
	

	
	

	
	

	
	

	Follow-up Action Required:
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