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Checklist 19-1

The purpose of this checklist is to confirm that the required steps in the contract planning process as they relate to safety have been considered and integrated into the tender provisions and contract expectations.

	DATE:

	Contract #:  SP22TFH006 Mechanical Site Prep East Kootenays

	BCTS Representative: Stacey Jacobs

	Safety Considerations
[image: BD21301_] = Applicable    |_|= Not applicable
	COMMENTS

	Any Known Hazards (on-site / adjacent)
[bookmark: Check1]|X| Overhead hazards (snags/power lines)
|_| Previous activities such as road building have not created hazards such as unstable fill slopes, rocks or log decks that will effect harvesting?
|X| Steep Slopes  (+35% for ground based harvesting) information to be provided to prospective licensees to support their harvest planning such as: 
· Slopes that exceed 35%
· Long pitches of continuous slope 
· Terrain Stability Features e.g. fracture rock formation
· Ground Roughness e.g. hummocks, depressions steep, ravines
· Soil Conditions e.g. soil depth, exposed rock, loose gravels or soft mud.  
· Timber size and quality 
· Slopes or benches less than 35% but located above areas of greater slope.    
|_| Dangerous Terrain (gullies, ridges, cliffs)
|X| Unstable Surfaces (wet, soft)
|X| Wind throw / Heavy Slash
|_| Road Hazards (Road grades exceeding 18%).
|_| Road Excavation hazard (road sections in terrain >33% + anticipated cut-banks >6m in height + any other area that shows sign of instability). 
|_| Road Construction Initiated Landslides Hazards (signs of instability, broken rock, transition zones).
|X| Wildlife 
|X| Mines / Electrical / Pipelines 
|_| Other Risks / Hazards on site / adjacent / Root rot centres or infection levels
	Safety around the following have been discussed:
-Working in hazardous conditions slips trips and falls – appropriate footwear
-Wildlife and insect encounters
-Weather conditions: excessive rain, heat, wind, or snow
-Working during wildfire season – shutdowns, tools – keeping  informed
-Access to first aid
-A92788-6 contains slopes close to 40% where site prep will not be completed
-Mine located on Kootenay FSR between 8- 10km – should not be an issue to drive low bed past mine site as Kootenay FSR wide and mine site off main Kootenay.
-Range land fence located in A94609-1 & 2 not to be damaged
-North road running through A94609-2 main access into Old Town community (private land owners) road is not to be blocked by machinery.





	Term
|X| Adequate time to complete work given seasonal and access considerations?
	-A90843-6 & A92788-6 to be completed in spring prior to planting.  Kootenay East, accessing A92788-6 may have ravelling rock or snow along shaded creek crossing  BCTS will provide removal if necessary.

	Access 
|X| Has access route been assessed for hazards?
|_| Is their a hazard mitigation strategy in place that will be enacted prior to worker exposure?
|_| Will access routes accommodate the nature of traffic?
(See Checklist 23-1 for more comprehensive guidance)
	-Access into A75158-3 McNair FSR is rutted, narrow and contains steep sections with long distances between pull outs. 
-Waterbars on main road into A94609 blocks not to be disturbed.

	Adjacent Operations
|X| Are there conflicts with adjacent operations relative to timing or hazards (major licensees, salvage, silviculture, other industrial or public operations, phase congestion)?
	-Planting contractor may be in adjacent blocks during site prep of A92788-6.



	ESSENTIAL ELEMENTS
	COMMENTS

	Project Plan:
|X|  Have the proposed plans been reviewed with consideration toward worker safety (consider multiple employer work situations in relation to phase congestion)?
|X|  Have all known hazards been documented (high retention, wind throw, snags, unstable slopes, steep slopes )?
	-Review of contractor safety protocol
-A92788-6 contains slopes up to 40% where site prep will contour beneath.
-A90843-6 ,A75158-3 A94609-1,2 & 3 contain L1 seed trees which excavator will need to be aware of when maneuvering.

	Qualifications:
|X|  Have contract eligibility criteria been set with respect to performing works in a safe manner?
|_|  Does BCTS plan on establishing a multi employer workplace via multiple principle contracts to address this project?
|_|  If BCTS created MEWP which tender is most logical to function as prime contractor and have qualification parameters been established?
	-all training certificates supplied to contract manager.

	Other Factors:

	

	

	

	

	

	

	Follow-up Action Required:
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