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SMALL SCALE SALVAGE

FLTC MAPPING REQUIREMENTS




DATE: March 12, 2009

	PURPOSE

	To outline the Headwaters District Small Scale Salvage mapping process and the minimum acceptable mapping standards required for a Forestry License To Cut submission.


	ELECTRONIC MAPPING PROCESS (RESULTS, EZ-LINK, ESF)

	The licensee will be required to submit an electronic PDF map of the salvage area and “shape files” in BC Albers projection to the MOFR. These shape files are to include all salvage block boundaries, skid trails and individual patch points. The MOFR will create an xml file in ez-link and submit the data electronically via ESF (Electronic Submission Framework) into FTA (Forest Tenure Administration).


	FLTC CASH SALES (<50 M3)

	The MOFR prepares all FLTC Cash Sale documents and maps. No digital data or maps are required from the licensee.


	FLTC PROFESSIONAL SALVAGE APPLICATIONS/PSA’S (50-2000 M3)

	· Licensee must submit 4 color maps at a scale of 1 :5,000 or 1 :10,000

· Licensee must also submit 1 color overview map at a scale of 1:20,000 or 1:30,000

· “General” Map info must include:

□ Map Title

□ Legend
□ Scale 
□ Forest Region
□ Lats/Longs

□ Forest District
□ TSA
 
□ PSYU
□ FIZ 


□ Compartment

□ Region

□ Licensee Name

□ Mapsheet

□ North Arrow   □ Timber Supply Area

□ Timber Supply Block 

□ Geographic Description

□ Maximum, Minimum and Average Elevation

□ Mapping Company Info/Created By 

□ Total Area (Ha) and area of individual patches

· “Operational” and “Other” Map info must include but is not limited to:

□ Any watercourse, lake or wetland including classification

□ Riparian Reserve Zones
(RRZ)


□ Creek/Watercourse crossings

□ Machine Free Zones (MFZ)


□ Trapper Cabins /features



	FLTC PROFESSIONAL SALVAGE APPLICATIONS Continued….

	· “Operational” and “Other” Map info continued……..

□ All Landings/processing areas


□ Bladed and main access

□ Special Management areas 


□ Special Resource features

□ Main and spur road names identified

□ Km reference points 

□ All Harvest areas and boundaries

□ Deactivated roads

□ Range fences/improvements


□ Safe Work Procedure Areas

□ No Harvest Areas (WTPs, OGMAs)

□ Domestic water intakes/licenses

□ Sensitive Areas




□ Plantations/Harvested Areas

□ Major Licensee operating area boundaries

□ Silviculture Survey plots 

□ Trap Tree Patches must be numbered

□ Private Land, Parks, Woodlots, Recreation features and other tenures & licenses

□ Critical Wildlife Protection/Mgmt areas (Grizzly, Caribou, Red Listed species etc.)

□ Archaeological/Cultural heritage resource features 

□ Special Government projects (growth/yield/trials/research plots)

**Access trails are main trails that that run between patches or that provide the main access to a single tree salvage area. They do not include dispersed skid trails within a salvage area.


	SUMMARY

	The MOFR reserves the right to reject or return Professional Salvage Applications which fail to meet the minimum requirements set out in this document.

For more information regarding mapping requirements and processes, please contact the undersigned.


	JIM BIAGIONI, RFT

HEADWATERS FOREST DISTRICT

SSS COORDINATOR
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_______March 30, 2009______

Date

	_________JIMMY BIAGIONI________

Signature

Contact: Jim.biagioni@gov.bc.ca or 250-587-6713
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