	

	ACCESS
INSPECTION REPORT
GUIDANCE DOCUMENT
	BCTS CHK-006 
Completed by hand, in Word as a protected form or by Hand Held digital application for entry into Cengea Forest - Resources. 



[bookmark: _GoBack]Note: Access Inspection Report to be used for FSRs built under contract only. Use Timber Sale License & Permit Operations Inspection Report for Road Permit roads.
	Section A
	Business Area:  

	Field Team:

	[bookmark: Dropdown6]ORCS/ARCS File(s):
     
	Date of Inspection
Click here to enter a date.

	
	Contract #:
[bookmark: Text51]      

	Geographic Location: 
     
	Project Name:
     

	Inspection Type:


	
	Contractor:
     
	On-site Supervisor:
     


Section A:
Business Area, Field Team, File are mandatory. Contract # is free text mandatory in Word but will be from Cengea Forest - Resources maintenance table in hand held version. Enter date in Word using date picker field. In the Hand Held, Contractor will come from Cengea Forest - Resources registrant table. Geographic location will be from planning module in Cengea Forest - Resources table, Project Name and on-site supervisor will be free text.
Inspection type is a drop-down field in Word and includes “Initial”, “Progress” and “Final”.
Note: Inspection Reports not intended to be used for monitoring. Refer to Business Area protocols for monitoring procedures.
Note: BCTS CHK-006 Inspection Report is intended for use by BCTS staff. Use BCTS Client Self Inspection Report (CHK-011) for LPC Inspections.
	Section B
	Inspection Detail & Activity Status

	
	Roads
|_| Construction
|_| Maintenance
|_| Deactivation/Rehabilitation
|_| Other (specify):
     		
	Major Structures
|_| Construction
|_| Maintenance
|_| Deactivation
|_| Other (specify):
     	

	Harvesting Activities
|_| Falling
|_| Yarding
|_| Loading
|_| Other (specify):
     	

	Log Dump
|_|Active
|_|Inactive
|_|% Complete: 	
|_|Complete

	Contract Activity
|_|Active
|_|Inactive
|_|% Complete: 	
|_|Complete
Areas Inspected:
     		
	Applicable Legislation
|_| FRPA
|_| FPC
|_| Other (specify):      

Inspection Method:
|_|Field	              |_|Office


Section B:
In Word or as a field doc these can be ticked as indicated. Note under Roads, finished grade includes cross drain culverts. Structures refer to major culvert / bridge and stream crossings.
Indicate the Areas Inspected that are applicable to this inspection (free text).
Check applicable legislation for blocks / areas in the Inspection Other could refer to the Fort St. John Pilot Project, Stillwater Pilot project, etc.
	Section C
	Requirement ID # & Status 
	Yes: Inspector’s opinion requirement is being met. Comments optional – Section E
No: Inspector’s opinion of non-conformance requiring Corrective Actions – Section D or,
 Incident requiring Incident Root Cause Investigation Issue(s) – Section D.
ND: Not discussed.  NA: Not applicable.  Note: Refer to Guidance Document for requirement detail


Inspection will be for the purpose of confirming the Contractor’s activities were conducted in accordance with the following types of requirements:
· Conformance with the Project Plan.
· Conformance with EMS / SFM requirements (e.g. EMS training completed and documented, pre-work(s) completed and documented, eERP completed, implemented and on-site, EFPs followed and onsite, etc.) and SFMP requirements.
· Licence, permit and/or contract conditions.
· Compliance with legislation (e.g. Forest and Range Practices Act, Wildfire Act, Forest Act, Transportation of Dangerous Goods Act, etc.).
· Safety requirements
Note:
If a practice is not restricted by any of these requirements, BCTS will not indicate a non-conformance nor require a corrective action.
All findings at the time of inspection are considered opinions of the inspector.
The inspector is expected to be an average competent person who has been trained in the completion of inspections.
Nothing in this guidance will authorize a person to carry out activities that are not in compliance with legislation.
Definitions:
FRPA
Forest Practice: means a prescribed activity that is carried out by (a) the government; (b) a holder of an agreement under the Forest Act, or (c) a person in a prescribed category of persons on private land, subject to a tree farm licence, a community forest agreement or woodlot licence, or on Crown forest land;
Official: means an employee in the (a) ministry of the minister responsible for the administration of this Act, which employee is designated by name or title to be an official by that minister for the purpose of that provision, (b) ministry of the minister responsible for the Wildfire Act, which employee is designated by name or title to be an official by that minister for the purpose of that provision, or (c) Oil and Gas Commission who is designated by name or title to be an official by the minister responsible for the Oil and Gas Commission Act for the purpose of that provision;
Wildlife: means (a) vertebrates that are mammals, birds, reptiles, or amphibians and are prescribed as wildlife under the Wildlife Act, (b) fish from or in the non-tidal waters of British Columbia, including (i) vertebrates of the order Petromyzoniformes (lampreys) or class Osteichthyes (bony fishes), or (ii) invertebrates of the subphylum Crustacea (crustaceans) or phylum Mullusca (mollusks), and (c) invertebrates or plants listed by the Minister of Water, Land and Air Protection as endangered, threatened, or vulnerable species, and included the eggs and juvenile stages of these vertebrates, invertebrates and plants.
FPPR
Agreement holder: means a holder of an agreement under the Forest Act, other than a woodlot licence.  For the purpose of these inspections, this includes BCTS.
Authorized person: means a person who is an agreement holder or a person who is described in paragraph (a), (a.1) or (c) in the definition of “authorized in respect of a road”
Authorized in respect of a road: means (a) a district manager, timber sales manager or other government employee or agent who is authorized by the minister to construct, maintain or deactivate a forest service road, (a.1) a person who (i) is the holder of a road use permit for a forest service road, and (ii) receives an other from the minister under section 79 (4), (b) an agreement holder who is authorized to construct, maintain or deactivate a road under a road permit, cutting permit or an agreement that does not provide for cutting permits, and (c) a person, other that a woodlot licence holder, who is authorized to construct, maintain or deactivate a road under a special use permit or within a Provincial forest under an Act other than (i) the Transportation Act, Land Act, Local Government Act, or Pipeline Act, or (ii) the Coal Act, Mineral Tenure Act, Mines Act, or Mining Right or Way Act, if the road is located within the boundaries of a claim, lease, permit or other authorization granted or issued under the applicable Act;
Harvest: in relation to timber, means to fell or remove timber, other than under a silviculture treatment, including to (a) yard, deck or load timber, (b) process timber on site, (c) pile or dispose of logging debris, (d) construct excavated or bladed trails or other logging trails, (e) rehabilitate an area referred to in section 35, and (f) carry out sanitation treatments associated with operations referred to in paragraphs (a) to (e);
Minor Tenure: means (a) a free use permit, (b) a Christmas tree permit, (c) an occupant licence to cut, or (d) a forestry licence to cut that is not a major licence and limits (i) the area from which timber may be harvested to 1 ha or less, and (ii) the volume of timber to be harvested to 2 000 m3 or less;
Primary Forest Activity: means one or more of the following: (a) timber harvesting; (b) silviculture treatments; (c) road construction, maintenance and deactivation;
Resource Feature: means a resource feature identified under the Government Actions Regulation’
Silviculture Treatment: includes (a) site preparation for the purposed of reforestation, (b) planting trees, (c) brushing, including grazing for the purposes of brushing, (d) juvenile spacing, (e) fertilization, (f) pruning, (g) sanitation treatments associated with a silviculture treatment, and (h) pest management treatments, other than sanitation treatments;
Temporary Access Structure: means an access structure that (a) is in a cutblock, and (b) does not conform to the criteria described in paragraph (a) or (b) of the definition of “permanent access structure” and does not include a pit or quarry;
Wildfire Act/Regulation
Industrial Activity: includes (a) land clearing, and (b) other activities included in this definition by regulation, but does not include activities excluded from this definition by regulation;
Resource Management Open Fire: means an open fire that (a) burns unpiled slash over an area of any size, or (b) is not a category 1, 2 or 3 open fire and is lit, fuelled or used for silviculture treatment, forest health management, wildlife habitat enhancement, fire hazard abatement, ecological restoration or range improvement
FPC, Timber Harvesting and Silviculture Practices Regulation
Silviculture Treatment: means a treatment carried out individually or as part of a regime of treatments to create the described post harvest stand structure, site conditions or free growing conditions
	
	ID #
	01: Contract –  Safety Requirements
	Status
Y N NI NA
	0402
	Authorized Timber Harvesting specifications followed
	|_||_||_||_|

	
	0101
	SAFE Company status?
	|_||_||_||_|
	0404
	Landslide or Gully Process with Adverse Effects prevented
	|_||_||_||_|

	
	0102
	First Aid requirements met?
	|_||_||_||_|
	0405
	Fan Destabilization resulting from activities prevented
	|_||_||_||_|

	
	0104
	Evidence of adequate supervision?
	|_||_||_||_|
	0412
	General Wildlife Measures followed
	|_||_||_||_|

	
	0105
	No BCTS Safety concerns reported?
	|_||_||_||_|
	0413
	Resource Features protected
	|_||_||_||_|

	
	0106
	No Safety Incidents?
	|_||_||_||_|
	0414
	Wildlife Habitat Features protected
	|_||_||_||_|

	
	0107
	No contractor safety concerns from section 3.10?
	|_||_||_||_|
	0416
	Smoke Venting Index checked for air quality/burning in prescribed manner
	|_||_||_||_|

	
	0108
	CAL up to date?
	|_||_||_||_|
	0417
	FSP Results, Strategies & Measures followed
	|_||_||_||_|

	
	0109
	Adequate Safety ERP?
	|_||_||_||_|
	0419
	DM Notification of (re)start of Harvesting & Road Construction  
	|_||_||_||_|

	
	0110
	Safety Records
	|_||_||_||_|
	0420
	Other Legislative Requirements (Federal & BC) followed
	|_||_||_||_|

	
	0111
	Communication – signage, man check, etc.?
	|_||_||_||_|
	0421
	First Nations Requirements met
	|_||_||_||_|

	
	0112
	Conformance with Road safety protocols
	|_||_||_||_|
	ID #
	05: Legislative – Stream and Riparian Requirements
	Status
Y N NI NA

	
	0113
	 Apparent conformance with SWPs & PPE?
	|_||_||_||_|
	0501
	Road in RMA, Cutting in RRZ, RMZ Retention as authorized 
	|_||_||_||_|

	
	0118
	NOP confirmation received and recorded
	|_||_||_||_|
	0503
	Stream Crossings to protect channels and mitigate disturbance
	|_||_||_||_|

	
	0119
	Safety meeting documentation?
	|_||_||_||_|
	0504
	Fish Passage and Fish Habitat protection met
	|_||_||_||_|

	
	0120
	Manual Falling Addressed
	|_||_||_||_|
	0505
	Stream Sediment in Community Watersheds prevented 
	|_||_||_||_|

	
	ID #
	02: Multiple Employer Workplace (applied to Prime Contractor)
	Status
Y N NI NA
	0506
	Drinking Water Quality & Licensed Waterworks protected
	|_||_||_||_|

	
	0201
	PC designation? 
	|_||_||_||_|
	ID #
	06: Legislative – Road, Trail and Structure Requirements
	Status
Y N NI NA

	
	0205
	Communication of hazards by Prime Contractor?
	|_||_||_||_|
	0602
	Re-vegetate Roads within 2 years 
	|_||_||_||_|

	
	0206
	Adequate coordination by Prime Contractor?
	|_||_||_||_|
	0605
	Road & Structures Constructed & Maintained to be Sound & Safe 
	|_||_||_||_|

	
	0207
	PC roles & responsibilities clear?
	|_||_||_||_|
	0606
	Maintain Natural Surface Drainage Patterns in Road Construction
	|_||_||_||_|

	
	0208
	Adequate coordination & supervision?
	|_||_||_||_|
	0607
	Build, Repair and/or Install Bridges & Culverts as designed
	|_||_||_||_|

	
	0209
	Appropriate PC records?
	|_||_||_||_|
	0608
	Road Clearing Widths Appropriate for Conditions including safety 
	|_||_||_||_|

	
	0210
	CAL up to date?
	|_||_||_||_|
	0609
	Road Deactivation Requirements met 
	|_||_||_||_|

	
	ID #
	04: Legislative Area and General Requirements
	Status
Y N NI NA
	0610
	Roads Maintenance Requirements met
	|_||_||_||_|

	
	0401
	Damage to the Environment prevented
	|_||_||_||_|
	0611
	48 Hour Notification for Road Works in Community Watersheds provided 
	|_||_||_||_|




	
	ID #
	08: Environmental Emergency Response Requirements
	Status
Y N NI NA
	1202
	Timber Marking Practices followed
	|_||_||_||_|

	
	0801
	Env Emergency Response Plan onsite, location known
	|_||_||_||_|
	1203
	Dangerous Tree requirements met
	|_||_||_||_|

	
	0802
	Awareness of roles, responsibilities and procedures confirmed
	|_||_||_||_|
	ID #
	14:  Specific Conditions of Licence, Road, Log Dump Permit or Contract
	Status
Y N NI NA

	
	0803
	Incident Reporting documented and reported
	|_||_||_||_|
	1402
	Administrative requirements met
	|_||_||_||_|

	
	0804
	Test and Drills scheduled and completed
	|_||_||_||_|
	1403
	Environmental requirements met
	|_||_||_||_|

	
	0805
	Emergency response equipment onsite and maintained 
	|_||_||_||_|
	1404
	Other Utilities and Occupiers of Land requirements met
	|_||_||_||_|

	
	0806
	24 hour contact # provided to local Protection Fire Center Office
	|_||_||_||_|
	1405
	Construction Specifications followed
	|_||_||_||_|

	
	0807
	Appropriate Fire Danger Class discussed 
	|_||_||_||_|
	1407
	Debris disposed of properly
	|_||_||_||_|

	
	0808
	Fire Hazard Assessments and Abatement conducted, as required
	|_||_||_||_|
	1408
	Subgrade compaction followed
	|_||_||_||_|

	
	ID #
	09: EMS – Documents, Records & General Requirements
	Status
Y N NI NA
	1409
	Deactivation Schedule conditions met
	|_||_||_||_|

	
	0901
	Pre-work meetings done & documented
	|_||_||_||_|
	1410
	Maintenance Schedule conditions met
	|_||_||_||_|

	
	0902
	Self Inspections & Corrective Actions complete, documented and followed-up
	|_||_||_||_|
	1411
	Log Dump specifications met
	|_||_||_||_|

	
	0903
	Project Plan documents on-site and available
	|_||_||_||_|
	ID #
	80: Sustainable Forest Management Certification
	Status
Y N NI NA

	
	0904
	Training Current  - records completed, updated and available
	|_||_||_||_|
	8001
	SFM Certification Requirements met
	|_||_||_||_|

	
	0905
	Industrial Waste contained and timely removal
	|_||_||_||_|
	ID #
	90: Business Area Specific Requirements
	Status
Y N NI NA

	
	0906
	Conformance to BCTS Fuel handling (EFP 06) requirements 
	|_||_||_||_|
	9001
	
	|_||_||_||_|

	
	0907
	Other Environmental Field Procedures on site and followed
	|_||_||_||_|
	9002
	
	|_||_||_||_|

	
	ID #
	10: General Contractual Conditions
	Status
Y N ND NA
	9003
	
	|_||_||_||_|

	
	1006
	Industrial Camp Standards Requirements
	|_||_||_||_|
	9004
	
	|_||_||_||_|

	
	ID #
	12: General Contractual Conditions of Licence
	Status
Y N NI NA
	9005
	
	|_||_||_||_|

	
	1201
	Designated Supervisors directing workers
	|_||_||_||_|
	
	
	



	ID#
	Hand Held Version
	Form Version
	01: Contract – Safety Requirements

	0101
	SAFE Company
	SAFE Company status?
	[bookmark: OLE_LINK1][bookmark: OLE_LINK2]Is contractor & any subcontractors maintaining BCTS expectations for SAFE Company registration / certification as per the contract (see FS 1315).  Are the same parties involved as identified at prework and is their SAFE status still current and appropriate. Oral response from workers and supervisors will be adequate information unless BCTS feels follow up with BCFSC is warranted. Inspector can check by viewing list on BCFSC website at:  http://www.bcforestsafe.org/safe_companies/whos_safe.html

This requirement is N/A if company or contractor is exempted from SAFE Co. requirements.
In General:
For contracts advertised after April 1 2007 requirements were that all parties working on or bidding on the contract were to be registered with BCFSC and pursuing S.AF.E. Company certification.  
All contracts remain under the requirements applicable at the time of advertisement or award hence specific documents must be referenced to verify expectations.
For contracts advertised after Dec 31 2008 requirements changed to expectation for certification as follows:
All parties bidding on or working under the contract including subcontractors are to be S.A.F.E certified.
Some exemptions and provisions for new firms as well as alternate certification may apply; staff should be familiar with document expectations and other applicable policy matters before making final determination as to performance.

	0102
	First Aid
	First Aid requirements met?
	Yes indicates that First Aid resources are available as per 1st aid  resource assessment and  WSBC requirements according to type of work, location of worksite, and number of people on site. Observation must consider all workers on site if this is a MEWP.  
Inspectors should see first aid kit/resources and record of designated first aid attendant(s) as per WSBC OSH Regulation part 3.14 and Schedule 3 – Minimum levels of First aid.  
http://www2.worksafebc.com/publications/OHSRegulation/Part3.asp#SectionNumber:3.14

	0104
	Supervision
	Evidence of adequate supervision?
	Yes indicates functional safety supervision, workers on site recognize they are well supervised and know who the supervisor is, they are aware of their ability to report safety concerns to their supervisor and indicate that these are addressed appropriately by their supervisor. This is not in reference to BCTS contract administrator.

	0105
	No Owner Concerns
	NO BCTS Safety concerns reported?
	[bookmark: OLE_LINK9][bookmark: OLE_LINK10][bookmark: OLE_LINK7]Yes indicates that the contractor did not report any safety concerns to BCTS since the last BCTS inspection or prework-- that the contractor believed to be the responsibility of BCTS – form 15-1 could be used for this, or report could be verbal or via email.  (In addition yes indicates the contractor’s on site supervisor  is aware of the expectation for communicating any future situation)
[bookmark: OLE_LINK5][bookmark: OLE_LINK6]See http://www.for.gov.bc.ca/bcts/safety/contractor.htm 

	0106
	Reporting Unsafe Conditions
	No Safety Incidents?

	Yes indicates that contractor has not reported any safety close calls or incidents as required by the contract since the last recorded BCTS inspection.  No indicates that since the last recorded BCTS inspection contractor has reported one or more close calls or incidents. Current requirement in most contracts is to notify BCTS of any incidents reportable to WSBC.   ( Observation will generate necessary information for management review and may initiate an action plan if BCTS or contractor believe that BCTS planning of contract was a contributing factor)

	0107
	Employer concerns
	No contractor safety concerns from section 3.10?
	Yes indicates that the BCTS inspector on site did NOT see any safety concerns / hazards which required notification of the site supervisor/employer and/or WSBC.    Any one (including BCTS) on a work site who identifies a safety concern or hazard is obligated under WSBC regulations to report it to the supervisor on site.
 No indicates that the BCTS inspector did identify a safety concern with respect to contractor’s activities and reported same to contractor’s supervisor. The contractor’s supervisor is required to address the concern without undue delay.  If a BCTS inspector feels the contract supervisor did not adequately address the concern then they should follow up with their BCTS supervisor, BCTS management, and WSBC if warranted.

see:  http://www2.worksafebc.com/publications/OHSRegulation/Part3.asp#SectionNumber:3.10

	0108
	Corrective Action Log
	CAL up to date?
	Contractor must be able to demonstrate that they have followed up and implemented corrective actions where applicable, and have a system in place such as a Corrective Action Log.  This field may be N/A if company is exempted from SAFE Co. requirement. 

	0109
	Safety ERP
	Adequate Safety ERP?
	Functionality of ERP for worker safety needs is apparent? Emergency Response Plan must be on site, tested, documented, and communicated to all employers & workers within the workplace.  It should be applicable to the logistic circumstances of the workplace, for example providing for air and or marine support for evacuation of injured workers as necessary.  All workers should know its location & general content. ERP documents could be integrated with EMS required ERP but must address worker safety distinctly to ensure workers injured or at risk are able to secure necessary assistance and support.  Observation could be reviewed simultaneous with 0501 EMS ERP but must be recorded for reporting distinctly to confirm ERP addresses worker safety needs.

	0110
	Safety Records
	Safety Records
	Safety records such as training records, toolbox meetings, pre-works, inspections, certificates, incidents & hazard reports must be provided by the contractor when requested.  All records, such as training, meeting minutes, maintenance records, are reasonably available as per WSBC regs.

	0111
	Communication
	Communication – signage, man check, etc.?
	Appropriate communication must be on site – including signage, sign in/out procedures, training, radio procedures etc
for man check requirements see:
http://www2.worksafebc.com/publications/OHSRegulation/Part4.asp#SectionNumber:4.21

	0112
	Road protocols
	Conformance with Road safety protocols
	Evidence is apparent that contractor and their staff are aware of and following applicable road safety protocols such as radio procedures and hazard notifications etc.

	0113
	SWP & PPE
	Apparent conformance with SWPs & PPE?
	From BCTS observations on site – do workers appear to be conforming to safe work procedures and PPE requirements?  If not BCTS inspector should respond as per OHS Reg Sec 3.10 – inform the on site supervisor, and follow up as required.
(note – contractors are not required to conform with BCTS SWPs and PPE requirements, only with their own safety program requirements and WSBC regulations).

	0118
	NOP
	NOP confirmation received and recorded
	Has a Notice of Project (NOP), if required, been submitted to WSBC (and have operations commenced in accordance with the submitted NOP for all employers within the workplace)?
It is the responsibility of BCTS to ensure a NOP has been submitted to WSBC for projects expected to last more than 5 days, excluding timber cruising, road & cutblock layout, and surveying. The act of submitting the NOP is delegated to the contractor.
For workplaces where NOP applies, ensure the contractor has provided a valid NOP confirmation form to BCTS prior to commencing work. BCTS inspector must ensure that the NOP confirmation form has been received by BCTS and the number recorded in the General Pre-Work Comments section of the pre-work report. If NOP is in place, have operations commenced in accordance with the submitted NOP for all employers within the workplace?
Regulatory requirements for Notice of Project are available at: 
http://www2.worksafebc.com/publications/OHSRegulation/Part26.asp#SectionNumber:26.4

	0119
	Safety meetings
	Safety meeting documentation?
	Contractor has a mechanism on a regular and routine basis that allows for discussion and communications of safety information such as hazard alert changes to safety protocols and provides opportunity for workers to discuss safety concerns among themselves.



	0120
	Falling Addressed
	Manual Falling Addressed
	If no Manual tree falling (falling trees >6”DBH) is or will occur under this contract than this observation is N/A
   A qualified supervisor remains designated to site
   Fallers on site are certified and supervisors are verifying qualifications
   A falling plan is evident that addresses:
1. hazard identification, mitigation, 
1. emergency response plan, 
1. alternative methods for danger trees, 
1. monitoring and evaluating of fallers practices 
1. qualified assistance identified and evident
1. Man check provisions
Important!!! Staff should not approach active falling operations to verify this observation. The normal point of contact with the contractor should be used to explore adherence to these expectations and if necessary appropriate arrangements to discuss matters with the falling supervisor should be made in advance to ensure BCTS staff are not at risk from active falling.  BCFSC can provide further guidance regarding appropriate falling plans and monitoring processes that are recommended or encouraged.  BCTS is to verify that processes are evident but is not expected to have sufficient expertise to determine the adequacy or validity of these. 

	ID#
	Hand Held Version
	Form Version
	02: Multiple Employer Workplace (applied to Prime Contractor)

	0201
	Prime Designation
	PC designation?
	Is PC designation still applicable for the workplace. Consider changes to worksite and employers and nature of work to ensure PC designation remains appropriate and applicable. If changes are expected all parties must be informed and new PC qualification must be considered. Note only one PC can be appointed per workplace and all other contractors must be aware and cooperate.  FS1354 and FS1313 included in signed Contract.  Note, the FS1354 must be signed by BCTS and the contractor to allow the contractor to assume the responsibilities of prime contractor

http://www2.worksafebc.com/publications/OHSRegulation/Part26.asp#SectionNumber:26.1.1

	0205
	PC Hazard Communication
	Communication of hazards by PC?
	Has the PC been informed of known hazards and is there evidence of communication of known hazards to all employers & workers on an ongoing basis?  (see toolbox meetings, prework records etc)

	0206
	PC Coordination
	Adequate coordination by PC?
	Prime Contractor has a system to address safety co-ordination and compliance with the safety program.  see FS 1354 and WSBC WCA 118 and regulations for requirements.  Does the Prime Contractor’s safety program include the other employers on site?  I.e. – PC should have evidence of review of other employer’s safety programs, training records etc. 
http://www2.worksafebc.com/publications/OHSRegulation/Part26.asp#SectionNumber:26.1.1

	0207
	PC roles and responsibilities
	PC roles & responsibilities clear?
	Have the roles & responsibilities of the Prime contractor been communicated to all employers and workers in the workplace?  Demonstrated by worksite signage, minutes from pre works & safety meetings.

	0208
	Safety Supervision
	Adequate coordination & supervision ?
	Does the site supervisor / safety rep know other employer contacts, and is there adequate workplace coordination and supervision?

	0209
	PC Records
	Appropriate PC records?
	Is there appropriate PC record management? See FS 1354 for details – records could include:  safety meeting minutes from the prime contractor & other contractors & subcontractors; workplace inspection results for the prime contractor, other contractors, and subcontractors; a system for first aid coordination; emergency transportation provisions; and the Contractors safety program.

	0210
	PC CAL
	CAL up to date?
	Prime Contractor must have documentation that corrective actions are occurring with respect to reported hazards, incidents, or deficiencies from inspections


	ID#
	Hand Held Version
	Form Version
	04: Legislative - Area and General Requirements

	0401
	Damage to the environment
	Damage to the Environment prevented 
	FRPA
S 46 Protection of the environment
A person must not carry out a forest practice, a range practice or another activity that results in damage to the environment, unless in doing so
a) the person
i) is acting in accordance with a plan, authorization or permit under this Act,
ii) is not required to hold a plan or permit because of an exemption under this Act and is acting in accordance with this Act, the regulations and the standards, or
iii) repealed
iv) is acting in accordance with another enactment, and
b) the person does not know and cannot reasonably be expected to know that, because of weather conditions or site factors, the carrying out of the forest practice, range practice or other activity may result, directly or indirectly, in damage specified by regulation
FPPR
S 3 Damage to the environment
For the purpose of section 46 (1) [protection of the environment] and (1.1) of the Act, "damage" means any of the following that adversely alters an ecosystem:  landslide; a gully process on the Coast; a fan destabilization on the Coast; soil disturbance; the deposit into a stream, wetland or lake of a petroleum product, a fluid used to service industrial equipment, or any other similar harmful substance; a debris torrent that enters a fish stream; changes to soil.

	0402
	Authorized Timber Harvest
	Authorized Timber Harvesting specifications followed
	FRPA
S 52. Unauthorized Timber Harvesting
1. A person must not cut, damage or destroy Crown timber unless authorized to do so
a) under this Act, the Forest Act or an agreement under the Forest Act,
b) by the minister, for silviculture, stand tending, forest health, abating a fire hazard related to wildfires or another purpose, 
c) under a grant of Crown land made under the Land Act,
d) under the Park Act, or
e) under the regulations, in the course of carrying out activities
i) under an authorization referred in section 51 or 57, or
ii) that are incidental to or required to carry out activities authorized or approved under this Act, the Forest Act, the Range Act or another prescribed enactment.
A person is authorized to cut, damage or destroy Crown timber for the purpose of carrying out a forest practice that is funded under a vote as defined in section 1 of the Financial Administration Act.
A person must not remove Crown timber unless authorized to do so
f) under the Forest Act or an agreement under the Forest Act,
g) under a grant of Crown land made under the Land Act, or
h)  under the Park Act.
If a person, at the direction of or on behalf of another person,
i) cuts, damages or destroys Crown timber contrary to subsection (1), or
j) removes Crown timber contrary to subsection (3),
that other person also contravenes subsection (1) or (3)

	0404
	Landslide and Gully Processes
	Landslide or Gully Process with Adverse Effects prevented 
	FPPR
S 37 Landslides
An authorized person who carried out a primary forest activity must ensure that the primary forest activity does not cause a landslide that has a material adverse effect in relation to one or more of the subjects listed in section 149 (1) of the Act.
S 38 Gully processes 
An authorized person who carries out a primary forest activity on the Coast must ensure that the primary forest activity does not cause a gully process that has a material adverse effect in relation to one or more of the subjects lists in section 149 (1) of the Act

	0405
	Fan Destabilization Prevented
	Fan Destabilization resulting from activities prevented 
	FPPR
S 54 Fan destabilization
An authorized person who carries out a primary forest activity on the Coast must ensure that the primary forest activity does not cause fan destabilization that has a material adverse effect in relation to one or more of the subjects listed in section 149 (1) of the Act.

	0412
	Wildlife Measures
	General Wildlife Measures followed  
	FPPR
S 69 General wildlife measures
An authorized person who carries out primary forest activities on an area must comply with each general wildlife measure that applies to the area.

	0413
	Resource Features
	Resource Features protected  
	FPPR
S 70 Resource features and wildlife habitat features
An authorized person who carries out a primary forest activity must ensure that the primary forest activity does not damage or render ineffective a (1) resource feature or 

	0414
	Wildlife Habitat Features
	Wildlife Habitat Features protected
	FPPR
S 70 Resource features and wildlife habitat features
1. An authorized person who carries out a primary forest activity must ensure that the primary forest activity does not damage or render ineffective a wildlife habitat feature.
Wildlife Act
S 7. Damage to land set aside for wildlife
1. A person commits an offence if the person 
a) alters, destroys or damages wildlife habitat, or 
b) deposits on land or water a substance or manufactured product or by product 
in a manner that is harmful to 
c)  wildlife, or 
d)  wildlife habitat
in a wildlife management area, except as permitted under section 4 (4) or by the regulations or a permit.
S 34. Birds, nests and eggs
A person commits an offence if the person, except as provided by regulation, possesses, takes, injures, molests or destroys 
4. a bird or its egg, 
f) the nest of an eagle, peregrine falcon, gyrfalcon, osprey, heron or burrowing owl, or 
g)  the nest of a bird not referred to in paragraph (b) when the nest is occupied by a bird or its egg.

	0416
	Smoke Venting
	Smoke Venting Index checked for air quality/burning in prescribed manner
	Open Burning Smoke Control Regulation
Schedule B, S 8 Favourable weather for smoke dispersion
1. Unless otherwise specified for smoke management purposes in a Ministry of Forests burning permit or in a burn plan approved by the Ministry of Forests, open burning of debris must not be initiated unless the ventilation index is forecast as
a)  "good" for the day the open burning is to be started, and
b)  "good" or "fair" on the second day the debris is anticipated to release smoke.
If the ventilation index required by subsection (1) is not publicly available, a person who proposes to open burn debris must conduct a test burn, lasting no longer than 60 minutes, of sufficient debris on the site to evaluate the weather conditions so as to ensure that smoke from any subsequent open burning, initiated on the same day as the test burn, will not negatively impact on a nearby population.
Open burning of debris must not be initiated if the local air flow will cause the smoke to negatively impact on a nearby population.
Unless otherwise exempted for smoke management purposes by a Ministry of Forests burning permit or in a burn plan approved by the Ministry of Forests, open burning of debris must not be initiated if atmospheric mixing at the site where the debris is to be burned is insufficient to provide rapid dispersion of the smoke.
S 24 Burn registration number
1. The following is the information to be provided under section 22 (1) (c) (ii) and 23 (1) (d) (ii):
a) the name, address, and telephone or facsimile number, or other means of immediate contract, of the person who proposes to light, fuel or use the open fire;
b)  the whereabouts of the parcel of land that contains the proposed burn area, including legal description of the parcel if available;
c)  the category of the proposed open fire
d)  other information relating to the proposed open fire that the official or the person answering the telephone number requires.
 A person answering the burn registration telephone number or an official who receives an application from a person in accordance with subsection (1) may
e) assign a burn registration number to the person unless the proposed open fire has been prohibited or restricted under section 10 of the Act, and
f)  specify a date on or before which the open fire must be extinguished.
 A person who has been assigned a burn registration number must provide it to an official immediately on request.

	0417
	FSP Results, Strategies & Measures
	FSP Results, Strategies & Measures followed
	FRPA
S 47 Invasive plants
A person carry out a forest practice or a range practice carry out measures that are 
g)  specified in the applicable operational plan, or 
h)  authorized by the minister
to prevent the introduction or spread of prescribed species of invasive plants.
S 48 Natural range barriers
A person carrying out
6. a forest practice, or
j) a range practice
That directly or indirectly removes or renders ineffective a range barrier must carry out measures that are 
k) specified in an operational plan for the area, or
l) authorized by the minister
To mitigate the removal or the ineffectiveness of the natural range barrier.
FPPR
[bookmark: section106-2]S 106.2 Requirements specific to timber sale licences
A holder of a timber sale licence who carries out a primary forest activity on an area that is in a forest development unit of a forest stewardship plan prepared by a timber sales manager must ensure that the activity is consistent with (a) the intended results or strategies that are identified by the timber sales manager and that (i) relate to the area, (ii) apply to the area in the manner that under section 10 (2) (c) of the Act is identified in the site plan for the area, and (iii) are contained in a forest stewardship plan
 S 17 Invasive plants
For the purpose of section 47 (invasive plants) of the Act, a person who prepares a forest  stewardship plan must specify measures in the plan to prevent the introduction or spread of species that are invasive plants under the Invasive Plants Regulation, if the introduction or spread is likely to be the result of the person’s forest practice
 S 18 Natural range barriers
For the purpose of section 48(natural range barriers) of the Act, a person who prepares a forest stewardship plan must specify measures to mitigate the effect of removing or rendering ineffective natural range barriers.


	0417
	FSP Results, Strategies & Measures followed (Continued)
	FSP Results, Strategies & Measures followed (Continued)
	FPPR
S 5 Objectives set by government for soils
The objective set by government for soils is, without unduly reducing the supply of timber from British Columbia’s forests, to conserve the productivity and the hydrologic function of soils.
S 7 Objectives set by government for wildlife
(1) The objective set by government for wildlife is, without unduly reducing the supply of timber from British Columbia’s forests, to conserve sufficient wildlife habitat in terms of amount of area, distribution of areas and attributes of those areas, for
(a) the survival of species at risk,
(b) the survival of regionally important wildlife, and
(c) the winter survival of specified ungulate species.
(2) A person required to prepare a forest stewardship plan must specify a result or strategy in respect of the objective stated under subsection (1) only if the minister responsible for the Wildlife Act gives notice to the person of the applicable
(a) species referred to in subsection (1), and
(b) indicators of the amount, distribution and attributes of wildlife habitat described in subsection (1).
(3) If satisfied that the objective set out in subsection (1) is addressed, in whole or in part, by an objective in relation to a wildlife habitat area or an ungulate winter range, a general wildlife measure, or a wildlife habitat feature, the minister responsible for the Wildlife Act must exempt a person from the obligation to specify a result or strategy in relation to the objective set out in subsection (1) to the extent that the objective is already addressed.
(4) On or after December 31, 2004, a notice described in subsection (2) must be given at least 4 months before the forest stewardship plan is submitted for approval.
S 8 Objectives set by government for water, fish, wildlife and biodiversity within riparian areas
The objective set by government for water, fish, wildlife and biodiversity within riparian areas is, without unduly reducing the supply of timber from British Columbia’s forests, to conserve, at the landscape level, the water quality, fish habitat, wildlife habitat and biodiversity associated with those riparian areas.
S 8.1 Objectives set by government for fish habitat in fisheries sensitive watersheds
(1) In this section, “fisheries sensitive watershed” means an area identified in Schedule 2 of this regulation
(a) with significant downstream fisheries values continued under section 180 (f) of the Act and significant watershed sensitivity continued under section 180 (g) of the Act, and
(b) for which there is no fisheries sensitive watershed objective
(2) Until December 31, 2005 the objective set by government for fish habitat in fisheries sensitive watersheds is to prevent to the extent described in subsection (3) the cumulative hydrological effects of primary forest activities in the fisheries sensitive watershed from resulting in a material adverse impact on the habitat of the fish species for which the fisheries sensitive watershed was established.
(3) The objective set by government under subsection (2) applies only to the extent that it does not unduly reduce the supply of timber from British Columbia’s forests.
(4) If satisfied that the objective set out in subsection (2) is not required to provide special management, the minister responsible for the Wildlife Act must exempt a person from the requirement to specify a result or strategy in relation to the objective.
(5) If satisfied that the objective set out in subsection (2) is addressed, in whole or in part, by an enactment, the minister responsible for the Wildlife Act must exempt a person from the requirement to specify a result or strategy in relation to the objective set out in subsection (2) to the extent that the objective is already addressed.
S 8.2 Objectives set by government for water in community watersheds
(1) In this section, “community watershed” means a community watershed
(a) that is continued under section 180 (e) of the Act, and
(b) for which a water quality objective has not been
(i) continued under section 181 of the Act, or
(ii) established under the Government Actions Regulation.
(2) The objective set by government for water being diverted for human consumption through a licensed waterworks in a community watershed is to prevent to the extent described in subsection (3) the cumulative hydrological effects of primary forest activities within the community watershed from resulting in
(a) a material adverse impact on the quantity of water or the timing of the flow of the water from the waterworks, or
(b) the water from the waterworks having a material adverse impact of human health that cannot be addressed by water treatment required under
(i) an enactment, or
(ii) the licence pertaining to the waterworks.
(3) The objective set by government under subsection (2) applied only to the extent that it does not unduly reduce the supply of timber from British Columbia’s forests.
(4) If satisfied that the objective set out in subsection (2) is not required to provide special management the minister responsible for the Wildlife Act must exempt a person from the requirement to specify a result or strategy in relation to the objective.
(5) If satisfied that the objective set out in subsection (2) is addressed, in whole or in part, by an enactment, the minister responsible for the Wildlife Act must exempt a person from the requirement to specify a result or strategy in relation to the objective set out in subsection (2) to the extent that the objective is already addressed.


	0417
	FSP Results, Strategies & Measures followed (Continued)
	FSP Results, Strategies & Measures followed (Continued)
	
S 9 Objectives set by government for wildlife and biodiversity – landscape level
The objective set by government for wildlife and biodiversity at the landscape level is, without unduly reducing the supply of timber from British Columbia’s forests and to the extent practicable, to design areas on which timber harvesting is to be carried out that resemble, both spatially and temporally, the patterns of natural disturbance that occur within the landscape.
S 9.1 Objectives set by government for wildlife and biodiversity – stand level
The objective set by government for wildlife and biodiversity at the stand level is, without unduly reducing the supply of timber from British Columbia’s forests, to retain wildlife trees.
S 9.2 Objectives set by government for visual quality
(1) In this section:
“scenic area” means an area of land established as a scenic area under the Forest Practices Code of British Columbia Act on or before October 24, 2002 and continued as a scenic area under section 180 (c) of the Act;
“visual quality class” means a visual sensitivity class established on or before October 24, 2002, particulars of which are publicly available in the Land and Resource Data Warehouse maintained by the minister responsible for the Land Act.
(2) The objective set by government in relation to visual quality for a scenic area, that
(a) was established on or before October 24, 2002, and
(b) for which there is no visual quality objective
Is to ensure that the altered forest landscape for the scenic area
(c) in visual sensitivity class 1 is in either the preservation or retention category,
(d) in visual sensitivity class 2 is in either the retention or partial retention category,
(e) in visual sensitivity class 3 is in either the partial retention or modification category,
(f) in visual sensitivity class 4 is in either the partial retention or modification category,
(g) in visual sensitivity class 5 is in either the modification or maximum modification category.
S 10 Objectives set by government for cultural heritage resources
The objective set by government for cultural heritage resources is to conserve, or, if necessary, protect cultural heritage resources that are
(a) the focus of a traditional use by an aboriginal people that is of continuing importance to that people, and
(b) not regulated under the Heritage Conservation Act


	0419
	DM Notification
	DM Notified of start or re-start of Harvesting & Road Construction  
	FPPR
S 85 Notification of timber harvesting or road construction 
An agreement holder must notify the district manager before(a) beginning (i) timber harvesting, or(ii) construction of a road that is not a temporary access structure, and(b) re-starting the activities described in paragraph (a) (i) and (ii) in a cutblock after an inactive period of 3 months or more.
A notice under subsection (1) must specify(a) the location of the timber harvesting or road, including any administrative identifier that relates to the location, (b) a contact name and contact information, and(c) the projected date for beginning timber harvesting or road construction.

	0420
	Other Legislative Requirements
	Other Legislative Requirements (Federal & BC) followed
	In addition to FRPA, FPPR and the Wildfire Act, the following are examples of Federal and BC legislative requirements that may be applicable to the project:
	Federal
	BC
	Occupational Health & Safety Regulation

	Fisheries Act
	Wildlife Act & Regulations
	Waste Management Acct

	Species at Risk Act
	Fish Protection Act
	Special waste Regulation

	Migratory Birds Act
	Water Act
	Contaminated Sites Regulation

	Canadian Wildlife Act
	BC Fire Code
	WHMIS

	Canadian Environmental Protection Act
	Environmental Management Act, Spill Reporting, Hazardous Waste & Contaminated Sites Regulations
	Integrated Pest Management Act & Regulations

	Canada Water Act
	Cultural Heritage Act
	Pesticide Control Act

	Navigable Water Act
	Heritage Conservation Act
	Pest Control Products Act

	Transportation of Dangerous Goods Act & Regulations
	Workers Compensation Act
	Applicable GAR Orders

	National Fire Code
	Employment Standards Act
	Applicable HLP Orders

	
	
	Applicable LRMP commitments


Legislation specifically applicable to the project should be indicated in associated contract documents, schedules or appendices, TSO significant environmental aspects lists, and/or forest planning documents.

	0421
	First Nations Requirements
	First Nations Requirements followed
	Discussion / implementation of any project specific outcomes from First Nations consultation and / or referral packages.




	ID#
	Hand Held Version
	Form Version
	05: Legislative – Stream and Riparian Requirements

	0501
	Riparian Resource Values
	Road in RMA, Cutting in RRZ, RMZ Retention as authorized 
	FPPR
S 50 Restrictions in a riparian management area
1. A person must not construct a road in a riparian management area, unless one of the following applies: 
7. locating the road outside the riparian management area would create a higher risk of sediment delivery to the stream, wetland or lake to which the riparian management area applies;
7. there is no other practicable option for locating the road; 
7. the road is required as part of a stream crossing.
If a road is constructed within a riparian management area, a person must not carry out road maintenance activities beyond the clearing width of the road, except as necessary to maintain a stream crossing.
A person who is authorized in respect of a road must not remove gravel or other fill from within a riparian management area in the process of constructing, maintaining or deactivating a road, unless (a) the gravel or fill is within a road prism, (b) the gravel or fill is at a stream crossing, or(c) there is no other practicable option.
S 51 Restrictions in a riparian reserve zone
1. An agreement holder must not cut, modify or remove trees in a riparian reserve zone, except for the following purposes: 
8. felling or modifying a tree that is a safety hazard, if there is no other practicable option for addressing the safety hazard; 
8. topping or pruning a tree that is not wind firm; 
8.  constructing a stream crossing; 
8. creating a corridor for full suspension yarding; 
8. creating guyline tiebacks; 
8. carrying out a sanitation treatment; 
8. felling or modifying a tree that has been windthrown or has been damaged by fire, insects, disease or other causes, if the felling or modifying will not have a material adverse impact on the riparian reserve zone; 
8. felling or modifying a tree under an occupant licence to cut, master licence to cut or free use permit issued in respect of an area that is subject to a licence, permit, or other form of tenure issued under the Land Act, Coal Act, Geothermal Resources Act, Mines Act, Mineral Tenure Act, Mining Right of Way Act, Ministry of Lands, Parks and Housing Act, Petroleum and Natural Gas Act or Pipeline Act, if the felling or modification is for a purpose expressly authorized under that licence, permit or tenure; 
8.  felling or modifying a tree for the purpose of establishing or maintaining an interpretive forest site, recreation site, recreation facility or recreation trail.
An agreement holder who fells, tops, prunes or modifies a tree under subsection (1) may remove the tree only if the removal will not have a material adverse effect on the riparian reserve zone.
S 52 Restrictions in a riparian management zone
1. An authorized person who cuts, modifies or removes trees in a riparian management zone for an S4, S5 or S6 stream that has trees that contribute significantly to the maintenance of stream bank or channel stability must retain enough trees adjacent to the stream to maintain the stream bank or channel stability, if the stream
9. is a direct tributary to an S1, S2 or S3 stream, (b) flows directly into the ocean, at a point near to or where one or more of the following is located: 
0. a herring spawning area; 
0. a shellfish bed; 
0. a saltwater marsh area; (iv) an aquaculture site;

	0503
	Stream Crossings
	Stream Crossings to protect channels and mitigate disturbance   
	S 55 Stream crossings
1. An authorized person who builds a stream crossing as part of a road, a temporary access structure or permanent access structure must locate, build and use the crossing in a manner that(a) protects the stream channel and stream bank immediately above and below the stream crossing, and(b) mitigates disturbance to the stream channel and stream bank at the crossing.
An authorized person who builds a stream crossing as part of a temporary access structure must remove the crossing when it is no longer required by the person.

	0504
	Fish Passage & Habitat
	Fish Passage and Fish Habitat protection met 
	FPPR
S 56 Fish passage
1. An authorized person who carries out a primary forest activity must ensure that the primary forest activity does not have a material adverse effect on fish passage in a fish stream. 
An authorized person who maintains a fish stream crossing built after June 15, 1995, must ensure that the crossing does not have a material adverse effect on fish passage. 
 Despite subsections (1) and (2), an authorized person may temporarily allow a material adverse effect on fish passage to construct, maintain or deactivate a road, including a stream crossing, if(a) fish are not migrating or spawning, and(b) the source of the material adverse effect is removed immediately on completion of the construction, maintenance or deactivation. 
S 57 Protection of fish and fish habitat
An authorized person who carries out a primary forest activity must conduct the primary forest activity at a time and in a manner that is unlikely to harm fish or destroy, damage or harmfully alter fish habitat.
Federal Fisheries Act
S 35.  Harmful alteration, etc., of fish habitat
1.  No person shall carry on any work or undertaking that results in the harmful alteration, disruption or destruction of fish habitat.
S 36.  Throwing overboard of certain substances prohibited
1. Subject to subsection (4), no person shall deposit or permit the deposit of a deleterious substance of any type in water frequented by fish or in any place under any conditions where the deleterious substance or any other deleterious substance that results from the deposit of the deleterious substance may enter any such water.
Note: The approved forest stewardship plan (FSP) may specify results and strategies that go beyond the Practice Requirements set out in the Forest Planning and Practices Regulation (FPPR). Refer to the applicable site plan as to how the intended results and strategies apply to the site.

	0505
	Community Watershed
	Stream Sediment, in Community Watersheds prevented 
	FPPR
S 61 Excavated or bladed trails
An agreement holder who(a) carries out timber harvesting, and(b) constructs an excavated or bladed trail in a community watershed must ensure that doing so does not cause sediment that is harmful to human health to enter a stream, wetland or lake from which water is being diverted for human consumption by a licensed waterworks.

	0506
	Drinking Water Protected
	Drinking Water Quality & Licensed Waterworks Protected
	FPPR
S 59 Protecting water quality
An authorized person who carries out a primary forest activity must ensure that the primary forest activity does not cause material that is harmful to human health to be deposited in, or transported to, water that is diverted for human consumption by a licensed waterworks.
S 60 Licensed waterworks
1. An authorized person who carries out a primary forest activity must ensure that the primary forest activity does not damage a licensed waterworks. (2) An authorized person must not harvest timber or construct a road in a community watershed if the timber harvesting or road construction is within a 100 m radius upslope of a licensed waterworks where the water is diverted for human consumption, unless the timber harvesting or road construction will not increase sediment delivery to the intake.
S 62. Roads in a Community Watershed
1. To prevent interference with the subsurface flow path of a drainage area that contributes to a spring that is a source of water for a licensed waterworks, the minister may
a) identify a spring in a community watershed, 
b) specify a distance from the spring within which a person who constructs a road must not locate the road, and
c) permit a person who constructs a road to locate the road closer to the spring than the distance specified under paragraph (b).
If the minister does not specify a distance under subsection (1) (b), a person who constructs a road must not locate the road closer than a 100 m radius upslope of the spring identified under subsection (1) (a), unless the construction does not interfere with the subsurface flow path of a drainage area that contributes to the spring.
Water Regulation
S 41. Protection of Water Quality
A person making a change in and about a stream must ensure that
d) no substance, sediment, debris or material that could adversely impact the stream is
i) allowed or permitted to enter or leach or seep into the stream from any activity, construction, worksite, machinery or from components used in the construction of any works, or
ii) placed, used or stored within the stream channel,
e) no standards or objectives published under section 2 (e) of the Environment Management Act by the Ministry of Water, Land and Air Protection for the protection of ambient water quality are exceeded or not attained now or in the future due to the change,
f)  there is no disturbance or removal of stable natural materials and vegetation in and about a stream that contribute to stream channel stability except as authorized under this regulation and in accordance with the terms and conditions specified by the habitat officer,
g)  temporary material, fill, bridge, culvert, pump, pipe, conduit, ditch or other structure used to assist in the construction of any works are constructed and maintained only during the period of construction, and are removed on completion of the works,
h)  all cast-in-place concrete and grouting is completely separated from fish bearing waters for a minimum of 48 hours,
i)  rock from acid-generating rock formations is not used for construction, and
j)  the stream is restored to its natural state on completion of the change in and about a stream.–
S 43. Protection of Other Water Users 
1. A person making a change in and about a stream, other than a change under section 44 (1) (o) to (s) or (2), must ensure that persons who are lawfully diverting or using water under the Water Act will not be adversely affected.
 Despite subsection ( 1), if persons who are lawfully diverting or using water under the Water Act may be adversely affected, a person proposing to make a change in and about a stream, other than a change under section 44 (1) (o) to (s) or (2), must give 3 days notice to those persons prior to commencing to make the change and must provide an adequate supply of water to those persons, if required by those persons.

	ID#
	Hand Held Version
	Form Version
	06: Legislative – Road, Trail and Structure Requirements

	0602
	Revegetation
	Re-vegetate Roads within 2 years 
	FPPR
S 40 Revegetation
An authorized person who constructs or deactivates a road must ensure that soil exposed by the construction or deactivation is revegetated within two years after the construction or deactivation is completed if it is reasonably foreseeable that(a) the erosion of the soil would cause(i) sediment to enter a stream, wetland or lake, or(ii) a material adverse effect in relation to one or more of the subjects listed in section 149 (1) of the Act, and(b) revegetation would materially reduce the likelihood of erosion.

	0605
	Roads & Structures
	Road & Structures Constructed & Maintained to be Sound & Safe 
	FPPR
S 72 Roads and associated structures
A person who constructs or maintains a road must ensure that the road and the bridges, culverts, fords and other structures associated with the road are structurally sound and safe for use by industrial users.

	0606
	Maintain Natural Surface Drainage 
	Maintain Natural Surface Drainage Patterns in Road Construction
	FPPR
S 39 FPPR Natural surface drainage patterns 
1. If an authorized person constructs a road, a temporary access structure or a permanent access structure on an area, the person must maintain natural surface drainage patterns on the area both during and after construction.
Despite subsection (1), if it is not practicable for an authorized person to maintain natural surface drainage patterns during the construction of a road, a temporary access structure or permanent access structure, the person must ensure the altered surface drainage pattern is compatible with the original natural surface drainage pattern by the earlier of (a) the end of the construction, and(b) the next freshet.

	0607
	Structure Design
	Build, Repair and/or Install Bridges & Culverts as designed 
	[bookmark: section73]S 73 Design of bridges
A person who builds a bridge for the purpose of constructing or maintaining a road must ensure that the design and fabrication of the bridge(a) meets or exceeds standards applicable to roads at the time the design or fabrication is done, in respect of(i) bridge design, as established by the Canadian Standards Association, Canadian Highway Bridge Design Code, CAN/CSA-S6, and(ii) soil properties, as they apply to bridge piers and abutments, as established by the Canadian Foundation of Engineering Manual, and(b) takes into account the effect of logging trucks with unbalanced loads and off-centre driving.
[bookmark: section74]S 74 Peak flow
1. A person who builds a bridge across a stream or installs a culvert in a stream for the purpose of constructing or maintaining a road must ensure that the bridge or culvert is designed to pass the highest peak flow of the stream that can reasonably be expected within the return periods specified below for the length of time it is anticipated the bridge or culvert will remain on the site: 
	Anticipated period the bridge or culvert will remain on the site
	Peak flow return period

	For a bridge or culvert that will remain on site for up to 3 years
	10 years

	For a bridge that will remain on site from 3 to 15 years
	50 years

	For a bridge that will remain on site for over 15 years
	100 years

	For a culvert that will remain on site for over 3 years
	100 years

	For a bridge or culvert within a community watershed that will remain on site for over 3 years
	100 years


A person may build a bridge that will not conform to the requirements of subsection (1) if
a) the bridge will pass the flow that will occur during the period the bridge remains on the site, (
b) the construction of the bridge occurs during a period of low flow, and
c) the bridge, or a component of the bridge that is vulnerable to damage by high flow, is removed before any period of high flow begins.
A person may install a culvert that will not conform to the requirements of subsection (1) if
d) the installation is temporary and the person does not expect to subsequently install a replacement culvert at that location, 
e) the stream in which the culvert is being installed is not a fish stream, 
f) the culvert will pass the flow that will occur during the period the culvert remains on the site, 
g) the installation of the culvert occurs during a period of low flow, and
h) the culvert is removed before any period of high flow begins.
[bookmark: section75]S 75 Structural defects
A person who maintains a road must do one or more of the following if a structural defect or deficiency occurs on a bridge that is part of that road: (a) correct the defect or deficiency to the extent necessary to protect(i) industrial users of the bridge, and(ii) downstream property, improvements or forest resources that could be affected if the bridge fails; (b) close, remove or replace the bridge; (c) restrict traffic loads to a safe level; (d) place a sign, on each bridge approach, stating the maximum load capacity of the bridge. 
S 77 Retaining information
1. A person who builds a bridge or major culvert for the purpose of constructing or maintaining a road must do all of the following:
a) prepare or obtain
i) pile driving records,
ii) for new materials used to build the bridge or major culvert, mill test certificates, in-plant steel fabrication drawings, and concrete test results,
iii)  soil compaction results, and
iv)  other relevant field and construction data;
b) prepare as-built drawings of the bridge or major culvert;
c) retain the information referred to in paragraphs (a) and (b) until the earlier of the date that
i) the bridge or major culvert is removed, and
ii) the person is no longer required to maintain the road.
Subject to subsection (3), a person responsible for maintaining a road must retain a copy of inspection records for a bridge or major culvert associated with the road for at least one year after the bridge or major culvert is removed from the site.
Unless the road has been deactivated, a person must submit to the district manager or the timber sales manager, as applicable, the documents, drawings and records described in subsections (1) and (2) in respect of a road if the person is no longer required to maintain the road because the district manager or timber sales manager
d) cancelled the road permit, road use permit or special use permit for the road, and
e) does not require the road to be deactivated.

	0608
	Road Clearing Width
	Road Clearing Widths Appropriate for Conditions including safety 
	[bookmark: section78]S 78 Clearing widths
A person who constructs or maintains a road must ensure clearing widths are at least the minimum width necessary to accommodate the road, having regard to all of the following: (a) the safety of industrial users; (b) the topography of the area; (c) the drainage of water in the area; (d) the stability of terrain in the area; (e) operational requirements, including(i) the placement of pits, quarries, landings or waste areas, (ii) the storage of bridge or culvert material, (iii) the amount of area required to operate equipment within the clearing width, including equipment turnaround sites, (iv) snow removal, and(v) fencing and other ancillary structures.

	0609
	Road Deactivation
	Road Deactivation Requirements met 
	[bookmark: section82]S 82 Road deactivation
1. A person who deactivates a road must do the following: (a) barricade the road surface width in a clearly visible manner to prevent access by motor vehicles, other than all-terrain vehicles; (b) remove bridge and log culvert superstructures and stream pipe culverts; (c) remove bridge and log culvert substructures, if the failure of these substructures would have a material adverse effect on downstream property, improvements or forest resources; (d) stabilize the road prism or the clearing width of the road if the stabilization is necessary to reduce the likelihood of a material adverse effect in relation to one or more of the subjects listed in section 149 (1) of the Act.
A person may submit to the district manager, in writing, a request for an exemption from the requirements of subsection (1) (a) if
a) the person has not begun deactivating the road, and
b) the road does not contain any bridges or major culverts.
The minister, in a notice given to a person who submits a request under subsection (2), may exempt the person if the minister is satisfied that the effectiveness of the works described in subsection (1) will not be negatively impacted by motor vehicle use.
If a road deactivated under this section is a road that was used under the authority of a road permit associated with, or a cutting permit issued under, a tree farm licence, the holder of the tree farm licence must maintain the stability of each part of the road that was deactivated.
[bookmark: section83]S 83 Hazard warning
At all times while a road is being deactivated, a person must have a sign posted that warns users of the deactivation.

	0610
	Road Maintenance
	Road Maintenance Requirements met
	FRPA
S 22.1. Industrial use of a road
1. A person must not use a road for 
a) timber harvesting, including the transportation of the timber or associated machinery, materials or personnel, or 
b) access for tree planting requiring more than 12 months to complete, or silvicultural treatments requiring transportation of machinery, 
except in one or more of the following circumstances:
c) the person 
i) is authorized to do so under a timber sale licence that does not provide for a cutting permit or under a woodlot licence, cutting permit, road permit or forestry licence to cut, or 
ii) is exempted under subsection (4);
d) the road is a forest service road, and the person is authorized to use the road under a road use permit or is exempted under subsection (4);
e) the road is one for which another person has a timber sale licence that does not provide for a cutting permit or has a woodlot licence, cutting permit, road permit or special use permit.
FPPR
S 79. Road maintenance
1. A person may maintain a road only if authorized or required to do so under the Act or this regulation.
A person who is authorized in respect of a road must maintain the road, including bridges, culverts, fords and other structures associated with the road, until
a) the road is deactivated,
b) the district manager notifies the person that the road should not be deactivated due to use or potential use of the road by others,
c) a road permit or special use permit for the road is issued to another person, or
d) the road is declared a forest service road under the Forest Act.
Subject to subsection (4), the government must maintain a forest service road, including bridges, culverts, fords and other structures associated with the road, until the road is deactivated.
1.  A person required to maintain a road must ensure all of the following:
a) the structural integrity of the road prism and clearing width are protected;
b) the drainage systems of the road are functional;
c) the road can be used safely by industrial users.

	0611
	Community Watershed Notification
	48 Hour Notification for Road Works in Community Watersheds provided 
	FPPR
[bookmark: section84]S 84 Notice - road in community watershed 
At least 48 hours before commencement of road construction or deactivation in a community watershed, a person must notify affected water licensees or affected water purveyors.

	ID#
	Hand Held Version
	Form Version
	08: Environmental Emergency Response Requirements

	0801
	Environmental ERP
	Environmental Emergency Response Plan onsite, location known
	Ensure BCTS clients are aware of their emergency response roles and responsibilities as it applies to the specific project and activity.  Key areas include:
Maintain completed eERP onsite 
Worker training, comprehension and awareness 
Onsite emergency response equipment (spill kits, fire response equipment (hand tools, suppression system)  
Periodic tests and drills

	0802
	Roles and Responsibilities
	Awareness of roles, responsibilities and procedures confirmed
	The EMS Manual refers to the EOPs and EFPs to define roles and responsibilities for implementation, maintenance and reporting on the performance of the EMS.  EFP-02 clearly defines a Contract Supervisor’s responsibilities to conduct and document a pre-work.

	0803
	Incident/Event procedures
	Incident Reporting  documented and reported (BCTS, PEP, MFR)
	In the event of an incident – did BCTS clients follow the procedures outlined in the environmental Emergency Response Plan and Incident Report?
EMS incident reporting roles and responsibilities are outlined in the Incident report EOP and referenced in the eERP.  Conformance to these requirements are linked to terms and conditions found in the TSL and contract documents.  
Reportable EMS Incidents include: Emergency Response Events (Fires, Spills, Erosion), Potential Non-compliance and Significant Non-conformance.

	0804
	Tests and Drills
	Test and Drills scheduled and completed
	Definitions:
Test – a comprehensive testing of the environmental emergency response procedures to ensure that they are adequate to address
emergency events. This includes full, hands on scenario testing of equipment, communications, and procedures as outlined in the eERP.
Drill – a due diligence exercise to ensure that onsite personnel have adequate levels of comprehension and awareness of environmental emergency preparedness and response procedures. This involves a demonstration of workers level of knowledge and training, and may include:
1. Review of eERP procedures,
1. Employee interviews,
1. Equipment testing,
1. Review of onsite ER equipment.
Tests are to be documented on the “CHK-010 Test-Drill Report Form”, maintained on site and results forwarded to BCTS representative. Results of drills may be documented on the CHK-010 and maintained on site.

	0805
	Emergency Response Equipment
	Emergency response equipment onsite and maintained 
	Emergency Response Equipment includes:
1. Spill kits 
1. Fire Hand tools for all industrial activities 
1. Fire Suppression system for high risk activities
References:
1. S 5 Sufficient fire fighting hand tools for an industrial activity
1. S6.3 High Risk activities must keep at the activity site a adequate Fire Suppression system
1. BCTS’ Fuel Handling (EFP 06) describes requirements for spill kits and training
Also refer to Ministry of Forests “Interpretative Bulletin for the Application of Wildfire Regulation Application for the Forest Industry” at the following website; http://bcwildfire.ca/Prevention/Industry/

	0806
	24 hour contact
	24 hour contact # provided to local Fire Centre
	Wildfire Regulation
S 4 Requirement to provide contact details
Before March 1 of each year, a person who, under the Forest Act, is the holder of
23. a major licence,
e) a timber sale licence that is not a major licence,
f) a community forest agreement, or
g) a woodlot licence
Must provide an official with a 24 hour a day contact telephone number if the person proposes to carry out an industrial activity on or after March 1 and before November 1 of that year.
Note: The intent is that Contractors notify Fire Centre where industrial activities are being conducted.

	0807
	Danger Rating
	Appropriate Fire Danger Class determined and activities restrictions implemented
	SCHEDULE 3 RESTRICTIONS ON HIGH RISK ACTIVITIES
	Danger Class
	Restriction
	Duration

	III moderate
	After 3 consecutive days of DGR III or greater, maintain a fire watcher after work for a minimum of one hour
	Until after the fire danger class falls below DGR III

	IV high
	Maintain a fire watcher after work for a minimum of 2 hours
	Until after the fire danger class falls below DGR III

	
	After 3 consecutive days of DGR IV, cease activity between 1 p.m. PDT (Pacific Daylight Saving Time) and sunset each day
	Until after the fire danger class falls to DGR III for 2 consecutive 
days, or falls below DGR III

	V extreme
	Cease activity between 1 p.m. PDT (Pacific Daylight Saving Time) and sunset each day and maintain a fire watcher after work for a minimum of 2 hours 
	Until after the fire danger class falls below DGR IV for 2 or 
more consecutive days

	
	After 3 consecutive days of DGR V, cease activity all day
	Until after the danger class falls below DGR V for 3 or more 
consecutive days, or falls below DGR IV


Wildfire Regulation
S 6 High risk activities
1. In this section, "fire season", in relation to an area, means the period
24. beginning on
0. the third day after the area is snow free, or(
0. in areas where snow cover is often absent, the third consecutive day that the temperature at noon is at least 12 degrees, and
24. ending on whichever occurs first
i) the first day after October 1 on which each of the following is present:
A) the daily fine fuel moisture code value is 75 or less;
B) the daily duff moisture code value is 6 or less;
b) the drought code value is 15 or less, or
i) (ii) noon of the first day on which the area becomes snow covered.
A person who carries out a high risk activity on or within 300 m of forest land or grass land during a fire season must determine the Fire Danger Class for the location of the activity
c) by reference to representative weather data for the area, 
d) by reference to
i) the Danger Region from Schedule 1, 
ii) the applicable numerical rating under the Buildup Index, and
iii) the applicable numerical rating under the Fire Weather Index, and
e) by cross-referencing the Buildup Index with the Fire Weather Index, for the applicable Danger Region, under Schedule 2.
If there is a risk of a fire starting or spreading, a person carrying out a high risk activity on or within 300 m of forest land or grass land must
f) do so in accordance with the applicable restriction and duration set out in Schedule 3 for the Fire Danger Class, and
g) keep at the activity site
i) fire fighting hand tools, in a combination and type to properly equip each person who works at the site with a minimum of one fire fighting hand tool, and
ii) an adequate fire suppression system.
A person who, in accordance with subsection (3) (a) and Schedule 3, is required to maintain a fire watcher, must ensure that the fire watcher
h) can reasonably see the site of the high risk activity during the time the fire watcher is required, 
i) has at least one fire fighting hand tool, 
j) actively watches and patrols for sparks and fires on the site of the high risk activity, 
k) immediately carries out fire control and extinguishes the fire, if practicable, and
l) has the means on site to report the fire.
High Risk Activities (Wildfire Regulation) include:
24. mechanical brushing;
n) disk trenching;
o) preparation or use of explosives;
p) using fire- or spark-producing tools, including cutting tools;
q) using or preparing fireworks or pyrotechnics;
r) grinding, including rail grinding;
s) mechanical land clearing;
t) clearing and maintaining rights of way, including grass mowing;
u) any of the following activities carried out in a cutblock excluding a road, landing, roadside work area or log sort area in the cutblock:
i) operating a power saw;
ii) mechanical tree felling, woody debris piling or tree processing, including de-limbing;
iii) welding;
iv) portable wood chipping, milling, processing or manufacturing;
v) skidding logs or log forwarding unless it is improbable that the skidding or forwarding will result in the equipment contacting rock;
vi) yarding logs using cable systems

	0808
	Fire Hazard Assessment and Abatement
	Fire Hazard Assessments and Abatement conducted, as required
	Wildfire Regulation
S 11 Hazard assessment
1. For the purposes of section 7 of the Act, 
a) each of the following is a prescribed activity under subsections (1) and (2) of that section: 
i) operating a waste disposal site; 
ii) operating a dry land sort; 
iii)  operating a camp associated with an industrial activity, and
b) each of the following is a prescribed circumstance under subsection (1) of that section: 
i) an industrial activity or an activity prescribed under paragraph (a) of subsection (1) creates or increases a fire hazard or is likely to do so; 
ii) an official notifies a person carrying out an industrial activity or an activity prescribed under paragraph (a) of subsection (1) that a fire hazard exists at the site of the activity or operation.
The prescribed intervals, at which persons described in section 7 (1) of the Act must conduct fire hazard assessments, are
c) 3 month intervals during the period in which the persons are carrying on the industrial activity or the prescribed activity in an area inside, or within 2 km of, the boundaries of
i) a local government under paragraphs (d) to (f) of the definition of "local government" in section 1 of the Act, or
ii) a fire protection district in a regional district, and
d) the shorter interval between the most recent 3 month interval and the date on which the activity ceases for an expected period of 3 months or more. 
The prescribed intervals, at which persons described in section 7 (1) of the Act must conduct fire hazard assessments, are
e) 6 month intervals during the period during which the persons, in any area other than the area described in subsection (2), are carrying on the industrial activity or the prescribed activity, and
f) the shorter interval between the most recent 6 month interval and the date on which the activity ceases for an expected period of 6 months or more. 
A person required to conduct a fire hazard assessment under section 7 (1) of the Act must
g) ensure that the fire hazard assessment includes an assessment of the fuel hazard and its associated risk of a fire starting or spreading, and
h) provide a copy of the fire hazard assessment when requested to do so by an official.
Wildfire Regulation
S 12 Hazard abatement
1. The following periods are prescribed as the periods in which persons described in section 7 (2) of the Act must abate fire hazards of which the persons are aware: 
a) for an area described in section 11 (2) (a) of this regulation, each of the 6 month periods beginning on the dates on which the persons are required under section 7 (1) of the Act to conduct fire hazard assessments; 
b) for an area other than an area described in section 11 (2) (a) of this regulation, each of the 12 month periods beginning on the dates on which the persons are required under section 7 (1) of the Act to conduct fire hazard assessments. 
A person required to abate a fire hazard under section 7 (2) of the Act must reduce the fuel hazard on the site of the industrial activity or prescribed activity as necessary to ensure that carrying out the activity 
c) does not increase the risk of a fire starting on the site, and 
d) if a fire were to start, would not increase the fire behaviour or fire suppression associated with the fire.

	ID#
	Hand Held Version
	Form Version
	09: EMS – Documents, Records & General Requirements

	0901
	Pre-work
	Pre-work meetings done and documented
	EFP-02 clearly defines a LPC Supervisor’s responsibility to conduct and document a pre-work

	0902
	Self Inspections
	Self Inspections & Corrective Actions complete, documented and followed-up
	The EMS manual describes requirements of the LPC to monitor themselves by:
Monitoring their activities for conformance with the requirements of the EMS and compliance with legal requirements.  BA staff will ensure that the acceptance of this monitoring responsibility is acknowledged through signing of contract documents and pre-work forms.

	0903
	Project Plan
	Project Plan documents on-site and available
	EFPs require all LPCs to have copies of any relevant plans on site and available to workers

	0904
	Training records
	Training Current  - records completed, updated and available
	The EMS manual describes requirements of LPCs to ensure their workers meet the relevant training requirements of the EMS, SFM, and legislation, and to maintain records of the training on Table EMS 008-1A or equivalent. 

	0905
	Industrial Waste
	Industrial Waste contained and timely removal
	EFPs require regular removal of industrial waste from the site.

	0906
	Fuel Handling
	Conformance to BCTS Fuel handling (EFP 06) requirements 
	EFP -06 outlines fuel storage and handling that should be followed by LPCs as well as a procedure to stop work if an incident occurs

	0907
	Other EFPs
	Other Environmental Field Procedures on site and followed
	The EFPs comprise part of the EMS program as defined in the EMS manual

	ID#
	Hand Held Version
	Form Version
	10: General Contractual Conditions

	1006
	Industrial Camp Standards
	Industrial Camp Standards Requirements
	Advisory Bulletin No. 2011-03-22 (External) – Industrial Camp Standards
This Advisory Bulletin provides guidance to BCTS staff and contractors on industrial camp standards for work performed under contract to BC Timber Sales. The Bulletin is available from the following link: http://www.for.gov.bc.ca/bcts/policy/

	ID#
	Hand Held Version
	Form Version
	12: General Contractual Conditions of Licence

	1201
	Designated supervisor
	Designated Supervisors directing workers
	FS 623
Paragraph 6.05
The Contractor shall designate a representative, who shall have full authority to act on behalf of the Contractor in connection with the Work and the Agreement and who shall be available at all times to the Ministry Representative.
Paragraph 6.07
The Contractor shall not substitute a representative without the written consent of the Ministry Representative..

	1202
	Timber marking
	Timber Marking Practices followed
	FLtC
Paragraph 8.01
The timber mark for timber cut under the Licence is:
{Business Area Timber mark}
 or
The timber mark(s) for timber cut and removed under this Licence is/are:
{FLtC Timber mark}

	1203
	Dangerous Tree 
	Dangerous Tree requirements met
	FLtC
Paragraph 6.02
The Licensee may fell trees outside of the clearing area if the person conducting tree felling determines that the tree is a dangerous tree according to Workers’ Compensation Board regulations.
Paragraph 6.03
The Licensee may remove a tree felled under Paragraph 6.02 if this Licence authorizes the removal of Crown timber from the clearing area, unless directed otherwise by the Timber Sales Manager.
FLtC Sched A
Part 2.00 Dangerous Trees clauses (if applicable)
2.02	The Licensee may cut a tree outside of the cutting authority if a person authorized by the Licensee reasonably believes that the tree represents a safety hazard

	ID#
	Hand Held Version
	Form Version
	14: Specific Conditions of Licence, Road, Log Dump Permit or Contract

	1402
	TSM Notified
	Administrative clauses met
	FLtC  Schedule A
Part 1.00 Administrative clauses (if applicable)
0.01	The Licensee must
(a)	notify the Timber Sales Manager of the date that the Licensee intends to begin timber harvesting or road construction at least [Number of days] days before the date that the Licensee intends to begin either of those activities, informing the Timber Sales Manager of the date that the Licensee intends to begin each of those activities respectively and,
if the Licensee intends to stop operations on the cutting authority area for longer than 14 consecutive days, the Licensee will
(b)	notify the Timber Sales Manager within 5 working days of after the commencement of that shutdown, and
(c)	notify the Timber Sales Manager at least 2 working days before recommencing operations on the cutting authority area.

	1403
	Environmental
	Environmental clauses met
	FLtC Schedule A
Part 3.00  Environmental clauses (if applicable)
3.04	The Licensee must
a)	supply, use and maintain at least one self-contained chemical toilet for every ten (10) persons working in the cutting authority area on or near a landing approved by the Timber Sales Manager when conducting operations under this licence, and
b)	discharge those toilets only at tan approved disposal site that is not on the cutting authority area. 

	[bookmark: _Hlk215298034]1404
	Other occupiers of land
	Other Utilities and Occupiers of Land clauses met
	FLTC Schedule A
 Part 4.00 Other Utilities & occupiers of land clauses (if applicable)
4.01	The Licensee must not unreasonably interfere with the exercise of the following rights of use or occupation held by the following person(s):
(a)	[Describe each person and the rights held by that person]
and must notify that person or each of those persons at least 14 days before commencing activities on the cutting authority area.
4.02	The Licensee, before commencing operations on the cutting authority area, must
(a)	identify the location of each water intake and pipeline and,
(b)	locate and mark every skid trail that will cross an intake or pipeline.
4.03	The Licensee
(a)	must repair any improvement belonging to a third party that is damaged because of operations conducted under this license, and
(b)	if the Licensee fails to repair an improvement, must pay the full cost a repair completed by another person.
4.04	The Licensee, before operating within two tree lengths of a statutory right-of-way, utility, or private property, must
(a)	notify the offices of [appropriate agency] at least seven (7) days before commencing those operations and
(b)	comply with that party’s guidelines and applicable Workers’ Compensation Act regulations in respect of conducting activities in the vicinity of that right-of-way.
4.05	The Licensee must
(a)	before commencing operations in the vicinity of a recreation trail, post signs on the trail warning of those operations,
(b)	not skid logs along the trail, and
(c)	repair any damage to the trail surface, cut banks, or other structures caused by the cutting or removal of timber.
4.07	The Licensee will comply with the terms and conditions of a Site Alteration Permit issued to BC Timber Sales under Section 12 of the Heritage Conservation Act, to the extent that the aforesaid Permit applies to the cutting authority area, by
(a)	collecting and labelling [number] stem round samples, and
(b)	delivering those stem round samples to the BCTS field team office before [Date (with 4 digit year)].

	1405
	Construction Specs
	Construction Specifications followed
	FS 623  Schedule C
Part 4 Construction Controls
No Design 
In addition to applicable requirements stipulated in Schedule D of this contract, the Contractor shall construct the works in accordance with the following diagram and accompanying tabular construction specifications:
Drawings
In addition to applicable requirements stipulated in Schedule D of this contract, the Contractor shall construct the works in accordance with the following drawings: 
( Contractor Coordinator: double click on a box to check or uncheck its applicability.)
|_|	Plan - drawing number insert number
|_|	Plan and Profiles -drawing numbers insert number(s)
|_|	Detailed Cross Sections - drawing or sheet numbers insert number(s)
|_|	Drainage Structures (other than bridges) drawings and specifications - drawing or sheet numbers insert number(s)
|_|	Special Structures drawings and specifications - drawing or sheet numbers insert number(s)
|_|	Other (specify) - insert other drawing or sheet types and numbers

	1407
	Debris Disposal
	Debris disposed of properly
	FS 623  Schedule C
Part 5 Site Preparation
Debris Disposal
When disposing of debris in accordance with Schedule D, debris must be disposed of in the following manner(s) for the designated sections of the road contract.
	
	DISPOSAL METHOD

	Road Section
	Piling 
	Piling and Burning
	Scattering
	Burying
	End Haul to a Disposal Site

	Insert section(s)
	Insert "X" or N/A
	Insert "X" or N/A
	Insert "X" or N/A
	Insert "X" or N/A
	Insert "X" or N/A




	1408
	Subgrade compacted
	Subgrade compaction followed
	FS 623  Schedule C
Part 6  Roadway and Drainage Excavation
In addition to the requirements for embankment compaction in Schedule D, the contractor must:
· Insert additional compaction requirements
The specifications for ballast size and depth are:
· Insert ballast specifications
Ballast materials must be placed and compacted such that the road will support a fully loaded gravel truck without leaving ruts.

	1409
	Deactivation
	Deactivation Schedule conditions met
	As per applicable deactivation schedules in contract

	1410
	Maintenance
	Maintenance Scheduled conditions met
	As per applicable maintenance schedules in contract

	1411
	Log Dump
	Log Dump specifications met
	As per applicable log dump construction schedules in permit and/contract

	ID#
	Hand Held Version
	Form Version
	80: Sustainable Forest Management Certification Requirement

	8001
	SFM Requirements
	SFM Requirements met
	Review the sustainable forest management plan that your BA is part of and ensure the LPC understands their requirements

	ID#
	Hand Held Version
	Form Version
	90: Business Area Specific Requirements

	9001 to 9005
	BA Specific Requirements
	BA Specific Requirements
	If any BA has some specific requirements – this is the section to track them and insert as many as required


If any requirement is a “No”, it must be included in actions below. There may be additional actions that follow but at the time of the pre-work indicate the immediate actions that the Contractor agrees to. In a hand held application, the “No” would trigger an auto populate ID #, requirement statement into the actions below.
Keep in mind that BCTS does not provide a safety program to our contractors or licensees but rather monitors at levels commensurate with our obligations their discharge of contract or licence expectations.  This will alter the nature of actions and follow up required for negative safety observations and should be guided by the safety manual and applicable document conditions.
As a Word document or as a form  there will be room for 2 actions after which additional pages must be added. In the hand held application any number of actions can be added.
In a hand held application the actions would generate and populate an action plan in Cengea Forest - Resources.
	ID #
	CORRECTIVE ACTION - 1

	    
	[bookmark: Text64]Requirement:       
	[bookmark: Text62]Responsibility:      

	[bookmark: Text65]Description:       
	Target Date:
 Click here to enter a date.
	Completion Date: 
Click here to enter a date.

	[bookmark: Text59]Corrective Action:      
	Follow-up:      

	ID #
	CORRECTIVE ACTION - 2

	    
	Requirement:       
	Responsibility:      

	Description:       
	Target  Date: 
Click here to enter a date.
	Completion Date: 
Click here to enter a date.

	Corrective Action:      
	Follow-up:      

	ID #
	CORRECTIVE ACTION - 3

	    
	Requirement:       
	Responsibility:      

	Description:       
	Target Date:
Click here to enter a date.
	Completion Date:
Click here to enter a date.

	Corrective Action:      
	Follow-up:      

	ID #
	CORRECTIVE ACTION – 4 (add extra sheets for more actions)

	    
	Requirement:       
	Responsibility:      

	Description:       
	Target  Date:
Click here to enter a date.
	Completion Date: 
Click here to enter a date.

	Corrective Action:      
	Follow-up:      



	ISSUE(S)
	Complete Incident Report Form for each incident type. Enter in Issue Tracking System (ITS) linked to the Inspection. ITS required for significant or repeat non-conformance, potential non-compliance, or Incident (as defined in EOP-04).

	[bookmark: Text74]Issue #:       Issue Type: 	

[bookmark: Text75][bookmark: Dropdown10]Issue #:       Issue Type: 	


Action Plans for both safety & EMS requirements should be generated for corrective and preventative actions, as agreed to by the inspector and the Licensee / Contractor. An Action Plan should be the process followed for the majority of findings.  Creation and documentation of an Action Plan (including closure) is required to show diligence in following up on non-conformances identified during pre-works and inspections. Local guidance may also be available.
An EMS Incident (with entry into Cengea ITS) is generated in the case of a reportable spill, fire, or landslide, significant non-conformance to BCTS management systems (SNC) or potential non-compliance with legislation (PNC) – local guidance may be available to determine what qualifies as a SNC or PNC.  Typically a PNC decision for an issue is when the finding has been reported to C&E, or the PNC has led to an impact that was intended to be avoided.  For a SNC the decision should again be in regard to whether an impact occurred or not, or if the SNC was a systematic breakdown and Timber Sales staff intends to proceed with contract or TSL action, i.e. Notice to Comply, Notice to Suspend, or Stop Work Order.
A safety incident would be generated in cases where the LPC has contacted BCTS with a hazard they believe to be the responsibility of BCTS, or potentially if BCTS staff have identified a safety issue on the LPC worksite which they have reported to WSBC.  In the case of an LPC incident or close call, the Licensee or Contractor would follow their own incident investigation process as required by their safety program.  BCTS would use the ITS process to investigate any portions of the incident / close call for which BCTS or the Licensee / Contractor felt may have been contributed by BCTS planning of operations and practices during operations (block & road layout, or other operations nearby etc).
In the case of an LPC incident or close call where BCTS staff was exposed, the incident would be investigated in two parts.  A) The role that BCTS may have played in the LPC incident would be entered into Cengea ITS as a safety issue and investigated through the ITS system.  B) The safety aspects related to the BCTS staff member would be investigated through the process described in chapter 15 of the safety manual.  For privacy reasons, any investigations for incidents / close calls in which BCTS staff were directly involved will not be entered into Cengea ITS.

	GENERAL INSPECTION COMMENTS
(Reference Requirement ID # where appropriate, add extra sheets for more comments)









	[bookmark: Text69]      

	     

	[bookmark: Text72]     


General comments do not generate actions. However the inspector can indicate where a condition was borderline, and can be useful information for subsequent inspections. The inspector can also clarify exactly where and what was reviewed and by default what was not reviewed to provide due diligence for the inspector in the event of a discovery later on. Reference the requirement ID # where appropriate to provide context for comments.
In Cengea Forest - Resources and in the Hand Held application this comment section will be one free text field. Lines on the form are only to facilitate use as the form in the field.
	[bookmark: Text36]Inspected by:       	
Signature X: 	
 
	[bookmark: Text37]Received by:      	
Signature X: 	
 I accept receipt of this inspection and am in agreement with the stated actions.

	[bookmark: Text38]Attachment: 
[bookmark: Check36][bookmark: Check37][bookmark: Check38]Additional Pages |_|	Photos |_|	Maps |_| 
[bookmark: Check39][bookmark: Check40]Correspondence |_|	Incident Report |_|	Other |_|
	Date of Delivery to Contractor: 
Click here to enter a date.	
Next Planned Inspection Date:
Click here to enter a date.	
	Delivery Method:
[bookmark: Check32]On-site  |_|	Email  |_|
[bookmark: Check33][bookmark: Check34][bookmark: Check35]Fax  |_|	Mail  |_|	Hand Delivered  |_|
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