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High Streamflow Advisory:  East Vancouver Island, including:  
· Puntledge River (Courtenay)           



· Tsolum River (Courtenay) 

· Nanaimo River
· Ash River
The Flood Warnings and Flood Watches in place for portions of Vancouver Island are downgraded to a High Streamflow Advisory. Significant rainfall on Vancouver Island largely ended near midnight, with most rivers rising to peak levels between 1AM and 8AM this morning.  The freezing elevation has dropped from overnight, but is remains near 1500 metres and some snowmelt is continuing.
All gauged rivers on Vancouver Island are now falling, with many dropping below warning level. Rivers in the Courtenay area remain high, with the Puntledge River and Browns River in the affected by releases from the Comox Lake reservoir.  Now that the flood peaks are receding, BC Hydro is increasing releases from the Comox Lake reservoir to increase storage capacity in the reservoir.
The Tsolum River at Courtenay has dropped 1 metre from its peak level, and is currently at a discharge of 146 cubic metres per second (m3/s).  This is slightly below the 2-year return period discharge. 
The Puntledge River at Courtenay peaked at 540 m3/s at midnight, fell to 180 m3/s at 8AM, and has risen again to 280 m3/s as of 1PM as a result of releases from the Comox Lake reservoir.  This is near a 2 year return period level.
The Browns River at Courtenay: The water level gauge appears to have suffered damage; however, BC Hydro reports the current discharge as 50 m3/s.  This is well below warning level. 
The Oyster River (between Courtenay and Campbell River) has dropped 0.5 metre from its peak level, and has a current discharge of 170 m3/s at 1AM.  This is now below warning level.
The Cruikshank River (Courtenay area) is falling and has a current discharge of 180 m3/s.  This is now below warning level. 
The Nanaimo River is falling but remains high.  It has dropped 0.9 metre from its peak level, and has a current discharge of 510 m3/s, which is at the 2-year return period level.
The Englishman River (Parksville) is falling and has a current discharge of 125 m3/s.  This is well below warning level. 

The Chemainus River is falling and has a current discharge of 170 m3/s.  This is well below warning level. 

The Cowichan River (Duncan) is falling but remains high.  It has dropped 0.15 metre from its peak level, and has a current discharge of 230 m3/s, below warning level.
The Ash River (north of Port Alberni) is falling but remains high.  It has dropped to a current discharge of 290 m3/s, which is near a 3-4 year return period.

Rivers (with the exception of the Puntledge and Browns rivers, affected by Comox Lake releases) will continue receding today, Wednesday and into Thursday.  Water levels will remain high, however, as the accumulated rainfall and snowmelt drains from their respective basin areas.  The forecast from Environment Canada is for only light and/or scattered rain today and tomorrow, with temperatures cooling.  However, another warm and wet frontal system is forecast to push across Vancouver Island again Thursday PM and Friday, which may cause rivers to rise again on Friday.
A High Streamflow Advisory means that river levels are rising or expected to rise rapidly, but that no major flooding is expected.  Minor flooding in low-lying areas is possible.

A Flood Watch means that river levels are rising and will approach or may exceed bankfull.  Flooding of areas adjacent to affected rivers may occur.

A Flood Warning means that river levels have exceeded bankfull or will exceed bankfull imminently, and that flooding of areas adjacent to the rivers affected will result.  


