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Corporate Bridge Register
Structure Inventory Data Form : CULVERTS
(June 12, 2013 Draft: revised to match CBR TEST version 1.08.06)



	Directional & Numbering Conventions Used:

Girders and piles are numbered from upstream to downstream. 

Left or right is determined facing downstream (except for delineators). 
Spans and piers are numbered from the left end when facing downstream.

	GENERAL

	*Structure #
	*Site #:

	*Type/Class:

(  Major Culvert

(  Woodbox/Log Culvert


	
	

	
	

	
	

	Built For:
(  BC Timber Sales


(  Operations Division


(  Other Commercial Users

(  Road Permit Holder


(  Road Use Permit Holder

	Year Superstructure Fabricated:
	Year Superstructure Installed:

	Year Added to Inventory:

	*Source:
(  Inherited:  Found Structure


(  Inherited:  From Oil & Gas/ Other Ministry
(  Inherited:  Non-Status Road


(  Inherited:  Reallocation
(  Inherited: Transfers from Other Ministries
(  New Structure
(  Replacement Structure

	
	

	
	

	*Primary User Client Number:
	*Client Location Code:

	Primary User Name:

	As Built Information on File?
(  Yes

(  No

	Installation Cost ($):

	Material Cost ($):

	Portable Structure?

(  Yes

(  No

	

	

	
	

	

	

	

	



	

	*Culvert Number:  (  of  (

	*Culvert Length (metres):
	Gradient:

	*Culvert Type:
( Box     ( Elliptical     ( Open Bottom     ( Round     ( Woodbox/log culvert


	*Culvert Material:
( Concrete     ( Corrugated Steel     ( Log     ( Other     ( Steel (Non-Corrugated)
* If “Other” is chosen; please specify in the line below:

	

	Inlet Cover Depth (mm):
	Outlet Cover Depth (mm):

	*Opening Height (mm):
	*Opening Width (mm):

	Headwall Location:

(  Both

(  Inlet
(  None

(  Outlet
	Open Bottom Substructure:
(  Cast in Place Concrete Footing
(  Lock-Block Footing
(  Piles
(  Precast Concrete Footing
(  Steel Footing

	


	Comments:



	*LOAD RATING DETAILS

	Current Load Rating GVW (tonnes):

	Are Load Posting Signs Warranted?

(yes

(no

(unknown

	Load Rating Unknown?


(yes

(no

	Original Design Load Rating GVW (tonnes):

	Design Vehicle Configuration:
(  BCL625
(  CL625
(  L100
(  L120
(  L150
(  L165
(  L45

(  L60

(  L75

(  L90

(  Other
* If “Other” is chosen; please specify in the line below:

	

	REPLACEMENT HISTORY

	This structure replaced structure #:

	This structure was replaced by structure #:

	REPLACEMENT DETAILS

	Estimated Closure (year):

	Light Vehicle Traffic Replacement (year):


	*Full Log Haul Traffic Replacement (year):

	Estimated Replacement Cost ($):

	Replacement Cost Comments:


	INSPECTIONS

	Planned Inspection Comments:



	Close Proximity Inspection Required?

( yes


(no

	Close Proximity Special Equipment Required:
( Peeper Truck

( Scuba

	Next Planned Close Proximity Inspection (yyyy/mm/dd):

	*Next Planned Routine Inspection (yyyy/mm/dd):


* Denotes Mandatory Information for Corporate Bridge Register
FS 1343 HTH
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