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overview

The goal of GIS department at BCTS is to have all supplied digital data arrive in a condition that maximizes its ability to be incorporated into our GIS System and Land Resource Manager - LRM (formerly Cengea Resources), in the most efficient and accurate means possible.  To meet this goal, all contractors, consultants and data suppliers must adhere to the following criteria for digital data standards.

The ArcGIS suite of software is being utilized within the BCTS GIS department. Therefore, spatial data will only be accepted in the Shapefile format. The table structures for the different types of data are described in detail under the “Shapefile Specifications” section.  

This document will be revised annually but may be updated periodically during the year as well.  If there are any changes or updates, release notes will be sent out at that time.

BCTS GIS Contacts

Khan, Lubna- GIS Analyst

250-398-4498 
     Lubna.Khan@gov.bc.ca
Jayalakshmi Krishnan - GIS Analyst
250-398-4410 
    Jayalakshmi.Krishnan@gov.bc.ca
BCTS SDE DATA CUT LOCATION (FOR REFERENCE PURPOSE)
These data can be used for reference to identify and copy Cut Block location by Timber Sale Licence (TSL) number

ftp://ftp.for.gov.bc.ca/TCC/external/!publish/Digital_Files/Shapefiles/ 

digital data standards

· All spatial data will be submitted via ESRI standard Shapefile format or in Personal Geodatabase format 
· All data must be spatially referenced to NAD83 and projected to BC Environment Albers. 

· All shapefiles must be submitted with a .prj file defining this projection and coordinate system. 

Projection Information


Projection: 



Albers Conic Equal Area

Central Meridian:


-126.0 degrees

First standard parallel:

50.0 degrees

Second standard parallel:

58.5 degrees

Latitude of reference:


45.0 degrees

False Easting:



1000000 meters

False Northing:


0 meters

· All spatial data must be topologically correct (no overlaps, no gaps).  

· All spatial data must have the correct spatial reference (positioned in the correct geographic location)

· Snapping should be set before commencing data edits so that line works and polygons will be snapped appropriately where needed

File Naming Convention

SHAPEFILE
Beetle_Recce_YYYY*1
*1If you are working on the Beetle Recce Project for the 2009 fiscal year then YYYY = 4 digits Year (Example: Beetle Recce 2009)

PERSONAL GEODATABSE

DDMMYY*2_BEETLE_RECCE_DBS

*2Geodatabse name must begin with a date (Data submission date to BCTS, if you are submitting a geodatabase)
shapefile / GEODATABASE specifications

SHAPEFILE

The following layers and types may be required to be submitted depending on the services being requested. 

	Layer
	TYPE or FEATURE CLASS

	Beetle Recce YYYY*1
	Polygon


PERSONAL GEODATABSE

Database Name: 
DDMMYY*2_BEETLE_RECCE_DBS
Feature Dataset:
Beetle_Recce

Feature Class:
Beetle_Recce_YYYY*1
Feature Type:
Polygon
DATABASE FIELD SPECIFICATIONS
Beetle Recce YYYY (Feature Class)
The shapefile / geodatabase schema for Beetle Recce YYYY must be as follows:

	Field Name
	Alias
	Field Length
	Data Type

	OP_AREA
	OPERATING AREA
	20
	Text

	AREA_NAME
	LOCATION
	50
	Text

	AREA_NUM
	AREA NUMBER
	10
	Text

	YR
	YEAR
	4
	Text


Attribute Codes
OP_AREA:

BCTS Operating Area (acceptable values are written below)


AREA_NAME:
Location information in detail (Optional if the Recce area is within an operating area)
· This field must have the corresponding TSL number if the Recce polygon is outside of an operating area
· If there is no TSL number available then a detail location information will suffice
AREA_NUM: 
Area Number within an operating area
· It is designated by 4 digits year, followed by a hyphen (dash) and a sequential number (ex:- 2009-1) to designate more than one Beetle Recce area within an operating area (ex:- 2009-1, 2009-2 etc)

YR: 
4 digits fiscal year 
Acceptable Values for OP_AREA (OPERATING AREA)
	CODE
	DESCRIPTION

	Ahbau
	Ahbau

	Bambrick
	Bambrick

	Batnuni
	Batnuni

	Bells
	Bells

	Big Creek
	Big Creek

	Big Valley
	Big Valley

	Cariboo Lake
	Cariboo Lake

	Charleson
	Charleson

	Clisbako
	Clisbako

	Coglistiko
	Coglistiko

	Dash
	Dash

	Enterprise
	Enterprise

	Gaspard
	Gaspard

	Gerimi
	Gerimi

	Hawks Creek
	Hawks Creek

	Kluskus
	Kluskus

	Landslide
	Landslide

	Little River
	Little River

	Little Swift
	Little Swift

	Mackin
	Mackin

	Maud
	Maud

	McIntosh
	McIntosh

	Meldrum
	Meldrum

	Milburn
	Milburn

	Morris
	Morris

	Mud Creek
	Mud Creek

	Nazko
	Nazko

	Piltz
	Piltz

	Punky Moore
	Punky Moore

	Quesnel Lake
	Quesnel Lake

	Ramsey
	Ramsey

	Sky Ranch
	Sky Ranch

	Tete Angela
	Tete Angela

	Tibbles
	Tibbles

	Twan
	Twan

	NA
	Outside of the OP Area * OP = Operating Area


SHAPEFILE / GEODATABASE TEMPLATE LOCATION
Personal Geodatabase / Shapefile templates with correct schema are available on the MOF FTP site under the following directory:

ftp://ftp.for.gov.bc.ca/TCC/external/!publish/Data_Standards/ArcGIS/Beetle_Recce/ 
http://www.for.gov.bc.ca/ftp/TCC/external/!publish/Data_Standards/ArcGIS/Beetle_Recce/ 
sUBMISSION GUIDELINES
· You can submit a personal geodatabase following the format mentioned above
· You also have the option to submit the feature class as a shape file by selecting the feature you want to export as a shape file

· Follow the naming convention mentioned above

· Spatial data can be delivered by CDs or DVDs or you will use the MOF FTP site (ftp://ftp.for.gov.bc.ca/TCC/external/incoming/) for spatial submission. Please find your submission directory on the FTP location mentioned above. 

· You must email your GIS contact at BCTS just after the file submission on the FTP location, because files are kept there only for 7 days.

· If the file size is not significantly large (less than 5MB) , you can email the required spatial data upon getting request or confirmation by your GIS contacts at BCTS
· Spatial data and documents must be free of computer viruses
Questions/Concern
Please check GIS contacts section for BCTS (Cariboo-Chilcotin)
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