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BRITISH
COLUMBIA




	Ministry of

Forests, Lands, Natural Resource Operations and Rural Development
	Schedule B1
UNITS OF WORK


File:  10005-40/PL23TEG871
Attachment to the Agreement with ________ for Spring 2022 Spring Planting - 100 Mile House Field Team.
	TSL
	Block Name
	UBI #
	FUNDING
	Plant
	EST. AREA
	TARGET Density
	EST trees
	Plant type

	
	
	
	
	Type
	(HA)
	
	
	 

	A87213
	MHG56
	BE7D7
	FTM
	Fill NSR holes
	6.0
	2000
	
	Raw

	A92120
	CH8JZ
	BE8JZ
	FTM
	PL
	1.3
	2000
	
	Raw

	A92330
	JI8GZ
	BE8GZ
	FTM
	PL
	13.5
	2000
	
	DT

	A93319
	JI8PF
	BE8PF
	FTM
	PL
	6.3
	2000
	
	Raw

	A93571
	MH8SV
	BE8SV
	FTM
	Rehabed road
	0.3
	
	
	Road

	A94869
	JI9LU
	BE9LU
	FTM
	PL
	19.5
	2000
	
	OF from 2021

	A95415
	RF9PX
	BE9PX
	FTM
	PL
	8.9
	2000
	
	Raw/DT

	TA0001
	CC9FC
	BE9FC
	FTM
	PL
	58.6
	2000
	
	Rip

	
	CC9FH
	BE9FH
	FTM
	PL
	100.6
	2000
	
	Rip

	TA0059
	RF9P9
	BE9P9
	FTM
	PL
	88.7
	2000
	
	Raw /DT

	TA0071
	RF9EW
	BE9EW
	FTM
	PL
	7.4
	2000
	
	Rip

	
	RF9F1
	BE9F1
	FTM
	PL
	116.3
	2000
	
	Rip

	TA0377
	MS9M7
	BE9M7
	FTM
	PL
	13.6
	2000
	
	Raw

	
	MS9MA
	BE9MA
	FTM
	PL
	4.2
	2000
	
	RAW

	
	MS9MD
	BE9MD
	FTM
	PL
	8.6
	2000
	
	Raw

	
	MS9MG
	BE9MG
	FTM
	PL
	9.5
	2000
	
	Rip

	
	MS9MJ
	BE9MJ
	FTM
	PL
	2.5
	2000
	
	Raw/DT

	
	MS9P3
	BE9P3
	FTM
	PL
	6.2
	2000
	
	Raw/DT

	
	MS9PH
	BE9PH
	FTM
	PL
	1
	2000
	
	Raw/DT

	A94680
	LA94C
	BE94C
	FTM
	PL
	7.6
	2000
	
	Raw

	
	
	
	
	
	
	
	
	

	TOTALS
	20
	
	
	
	488.9 Ha
	
	Sown

1,191,280
	


Note:
Block allocations will be finallised in the formal tender document  that will follow this viewing. Actual seedlings available will be finalized once nursery lift numbers have been reconciled early in the new year. Block allocations before planting will be set up in a Plant Wizard file and made availbile to the successful Bidder.
 
Details for planting by block  will be on each seperate block map,  however in general  by the TSL’s  the methods below are what will be expected of the planters. Final seedling allocation for each block will be done after final nursey lifts and will be completed using Plant Wizard for the project.
A87213  Potenially a small Fill plant in the NSR patches possibly the burn piles.
A92120  Plant burn piles along the road plant tens  No seedlings allocated for this plan on using overrun or overflow trees from other plant units.

A92330  Plant Mid trench Pli only in the burn piles and on the rehabbed roads.

A93319  Raw plant (boot) screef  the best microsite  in a plantable medium, close attention must be paid to meeting the target density.

A93571 100% pine plant on the 250 meters of rehabbed road, expect to use over runs or overflow seedlings from oter blocks.

A94869  Raw plant with a screef selecting the best microsite, portions of the block was planted in 2021 will need last years planting map.

A95415 Target plant density 2000 screef raw ground  may have some Disc trenching 60% pine plant spruce in the wetland. May need Heli to tranfers seedlings into block.
TA0001 Plant 10's trees should be planted at the bottom of the trench where a prepped spot does not exist, at target spacing, target the north side of obstacles; trees should not be planted in the open, without protection. An unprotected tree (not on an onstacle or in a trench) will be faulted. Plant Fdi within 5m of timber edges, Pli/ Py throughout the body of the block; Py should not appar more than once per plot. Elephant Hill Principles require designated trails and roads to be used for travel only. No ATV trails to be punched into the block during planting activites. 
TA0059 Attempt to plant 2000 sph Plant the bottom of the trench, protecting the seedling Prioritize Fdi in the most protected sites Pli on rehabbed roads and burn piles Fdi planted without protection will be fined.
TA0071 Attempt to plant 2000 sph Plant the bottom of the trench, protecting the seedling Prioritize Fdi in the most protected sites Pli on rehabbed roads and burn piles Fdi planted without protection will be fined.
TA0377 Strict obstacle plant for Fdi Plant bottom of trenches, where trenches don't exist, plant a substantial obstacle on the North East quadrent, separate blocks in this TSL will have minor variations to this general rule.
A94680  Micro site planting with screefing to a plantable medium and meeting the target plant density being key to success.

Schedule B1 – Units of Work
CSNR-FSB November 17, 2014
Page 1 of 1
PL20TEG032 - Schedule B1 – Units of Work
CSNR-FSB November 17, 2014
Page 2 of 2

