[bookmark: _GoBack]Objective: To remove burnt area from TSL A94253 Block 4, and link modified shapes to tabular records:
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1. Digitized a line along the burnt part to use it with ‘flatten tool’ for removing burnt area.
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2. On attempting to link shapes, a spatial validation error was thrown up, similar to the screenshot below (the error seen below is from a different block)
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3. This block did not have any topological errors in the Cengea Resources system. Topology checks had been previously run before data was migrated to LRM. 
4. To double-check this, I used ‘Erase’ tool to find the difference between Block and Standard Unit, and the output did not have any slivers or overlaps.
5. Deleted all the linked shapes, and modified all the shapes in ArcMap (not in spatial view).
6. Linked the modified block shape to ‘Cut Block shape’.
7. Clipped the other shapes to this new block boundary and tried to link the remaining shapes (Standard unit, ecology etc), but the Spatial business rule violation error was seen again.
8. Under Tools > Options > Spatial View > Tolerance, I changed the Sliver polygon size from the default of 10 square metres to just above the error value, which was around 21 square metres after the block shape was modified.
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9. After this I was able to link all the shapes of this block to tabular records.
10.  Final block shape:
[image: ]
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