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Results and Strategies
	Result/Strategy
	How the Result/Strategy applies to the site

	FSJ or VHF 5.1.1 Ag Development Areas
	The road(s) included in this Site Plan is/are outside of Agricultural Development Areas and Settlement Reserve Areas.

	FSJ or VHF 5.1.2 Landscape Biodiversity
	The road(s) included in this Site Plan is/are consistent with the Order – Establishing Landscape Biodiversity Objectives for the Prince George TSA (October 20, 2004).

	FSJ 5.1.3 Community Forest
	The road(s) included in this Site Plan is/are outside of the applicable area for Community Forest Agreement K4B.

	FSJ or VHF 5.2.1 Soils
	Soils Disturbance Limits: The area contained within this Site Plan is a road right of way, not within a cutblock, therefore, Forest Planning and Practices Regulation (FPPR), section 35 does not apply.
Permanent Access Structure Limits: The area contained within this Site Plan is a road right of way, not within a cutblock, therefore, Forest Planning and Practices Regulation (FPPR), section 36 does not apply.

	FSJ 5.2.2.1 Northern Caribou
	The road(s) included in this Site Plan is/are not within spatially identified areas capable of providing Species at Risk Elements (migration corridors, calving range or rutting range) for Northern Caribou as specified in the Notice – Indicators of the Amount, Distribution and Attributes of Wildlife Habitat Require for the Survival of Species At Risk In the Fort St James Forest District for Northern Caribou.
or 
All or a portion of the road(s) included in this Site Plan is/are within one or more spatially identified areas capable of providing Species at Risk Elements (migration corridors, calving range or rutting range) as specified in the Notice – Indicators of the Amount, Distribution and Attributes of Wildlife Habitat Required for the Survival of Species At Risk In the Fort St James Forest District for Northern Caribou.  The road(s) has/have been located and/or timing of Primary Forest Activities limited such that key habitat attributes for Northern Caribou are protected consistent with the Notice.

	VHF 5.2.2.1 Northern Caribou
	The road(s) included in this Site Plan is/are not within spatially identified areas capable of providing Species at Risk Elements for Northern Caribou as specified in the Notice – Indications of the Amount, Distribution and Attributes of Wildlife Habitat Required for the Survival of Species at Risk in the Vanderhoof Forest District for Northern Caribou.
or 
All or a portion of the road(s) included in this Site Plan is/are within one or more spatially identified areas capable of providing Species at Risk Elements (calving range, rutting range, connectivity matrix, or mineral licks) for Northern Caribou as specified in the Notice – Indicators of the Amount, Distribution and Attributes of Wildlife Habitat Required for the Survival of Species At Risk In the Vanderhoof Forest District for Northern Caribou.  The road(s) has/have been located and/or timing of Primary Forest Activities limited such that key habitat attributes for Northern Caribou are protected consistent with the Notice. 

	FSJ 5.2.2.2 Winter Survival of Northern Caribou
	The road(s) included in this Site Plan is/are not within the High or Medium Value areas of High Elevation Winter Range or the Low Elevation Pine-Lichen Ungulate Winter Range areas as specified in Notice – Indicators of the Amount, Distribution and Attributes of Wildlife Habitat Required for the Winter Survival of Ungulate Species in Fort St James District Within the Prince George Timber Supply Area for Northern Caribou.
or
If all or a portion of the road(s) is/are located within one of the applicable areas of the Notice listed above, specific wording will be required.

	FSJ or VHF 5.2.3 Riparian Areas

	Stream, Wetland and Lake Riparian Classes applicable to the road(s) included in this Site Plan have been assessed and are detailed in the Support Document.  The basal area retention in the Riparian Management Zone(s) is not applicable.
No roads included in this Site Plan are proposed within Riparian Management Areas other than those required for authorized stream crossings.

	FSJ or VHF 5.2.4 Fisheries Sensitive Watersheds - FPPR 8.1

	Within the Stuart Nechako Forest District, no Fisheries Sensitive Watersheds were identified in Schedule 2 of the FPPR.
FSJ Only: Fisheries Sensitive Watersheds have since been established by regulation and are addressed in section 5.3.3 of the Forest Stewardship Plan and this Site Plan.
VHF Only: Within the Vanderhoof FDU, no Fisheries Sensitive Watersheds have since been established by regulation.

	FSJ or VHF 5.2.5 Community Watersheds
	No community watersheds have been designated within the Stuart Nechako Forest District.

	FSJ or VHF 5.2.6 Landscape Level Biodiversity
	As per FSP 5.1.2, the road(s) included in this Site Plan is/are consistent with the Order - Establishing Landscape Biodiversity Objectives for the Prince George Timber Supply Area.

	FSJ or VHF 5.2.7 Stand Level Biodiversity
	The area contained within this Site Plan is a road right of way, not within a cutblock, therefore, Forest Planning and Practices Regulation (FPPR), section 9.1 does not apply.

	















FSJ 5.2.8 Cultural Heritage Resources






VHF 5.2.8 Cultural Heritage Resources

	.BC Timber Sales shares information about proposed road and cutblock development in an information sharing process and strives to undertake meaningful consultation as set out in the Province of British Columbia consultation procedures and agreements such as the Carrier Sekani Pathway Forward 2.0 Amending Agreement #2(2022) where applicable.
BC Timber Sales seeks further information about Cultural Heritage Resources (CHR) associated with the development areas from First Nations.  Where site-specific traditional use Cultural Heritage Resources of ongoing importance are identified by BCTS, the location of the resource is recorded and shared with First Nations.  Information sharing between First Nations and BCTS is also sought on an on-going basis during development, and includes discussion of potential impacts to CHR and measures utilized to mitigate impacts to CHR.

Although every attempt has been made to locate and record all archaeological and CHR features associated with the block, the possibility exists that some features may have been missed. If any previously unidentified archaeological or CHR features are discovered during Primary Forest Activities or other block activities, work in the nearby vicinity must immediately stop and the Timber Sales Manager immediately notified.  Before activities can proceed, an appropriate plan to manage the discovered features must be determined.

The road(s) has/have been reviewed in consideration of the Fort St. James District Archaeological Predictive Model.  As the road(s) is/are located within a zone of Low Archaeological Potential and no CHR were identified during development, no further archaeological assessment is required.
or
Fort St James:
The road(s) has/have been reviewed in consideration of the Fort St. James District Archaeological Predictive Model.  A [Archaeological Overview Assessment (AOA), Archaeological Impact Assessment (AIA) or Preliminary Field Review (PFR)] has been completed by [Contractor] in [month, year] in conjunction with the associated cutblock.  The Site Plan is consistent with the recommendations of this assessment.  These assessments are shared with potentially affected First Nations as per the archaeological permit under which the assessment is completed.  Specifically,      
Although every attempt has been made to locate and record all archaeological and CHR features associated with the road(s), the possibility exists that some features may have been missed. If any previously unidentified archaeological or CHR features are discovered during road construction, work in the nearby vicinity must immediately stop and the Timber Sales Manager immediately notified.  Before activities can proceed, an appropriate plan to manage the discovered features must be determined.

The road(s) has/have been reviewed in consideration of the Vanderhoof District Archaeological Potential Model.  An Archaeological Impact Assessment (AIA) has been undertaken by [Contractor] on [date].  The Site Plan is consistent with the recommendations of this assessment.  Specifically,      
Or
Vanderhoof:
The road(s) is/are located within a zone of Low Archaeological Potential, as assessed via the Vanderhoof District Archaeological Potential Model.  An Archaeological Impact Assessment (AIA) has not been undertaken.  No Cultural Heritage Resource (CHR) information has been brought forward by First Nations or any other source during the information sharing process.  No CHR features were noted during the development of this road and thus no further mitigative measures are prescribed. 


	FSJ 5.3.1 Scenic Areas and VQO
	The road(s) included in this Site Plan is/are not located within a Scenic Area.
or
All or a portion of the road(s) included in this Site Plan is/are within a Scenic Area possessing a Visual Quality Objective of [Maximum Modification, Modification, Partial Retention, Retention or Preservation].  The visually altered landscape resulting from the road(s) included in this Site Plan is consistent with this Visual Quality Objective.

	VHF 5.3.1 Northern Caribou Ungulate Winter Range
	No roads are proposed within the applicable areas of Order – Ungulate Winter Range U7-012 (Northern Caribou).

	FSJ 5.3.2 General Wildlife
	No roads is/are proposed within the applicable areas of Order – Ungulate Winter Range U7-003 (Mountain Caribou), Order – Wildlife Habitat Areas U7-016, 7-019 to 7-022, 7-024 to 7-044 and 7-061 (Caribou), Order – Moose Ungulate Winter Range U7-018 and U7-020 (Moose Ungulate Winter Range), Order – Ungulate Winter Range U7-019 (Mountain Goat), Order – Northern Caribou High Elevation Ungulate Winter Range U7-026.
or
If all or a portion of the road(s) is/are located within one or more of the applicable areas of the Orders listed above, specific wording will be required.

	VHF 5.3.2 Scenic Areas and VQO
	The road(s) included in this Site Plan is/are not located within a Scenic Area.
or
All or a portion of the road(s) included in this Site Plan is/are within a Scenic Area possessing a Visual Quality Objective of [Maximum Modification, Modification, Partial Retention, Retention or Preservation].  The visually altered landscape resulting from the road(s) included in this Site Plan is consistent with this Visual Quality Objective.

	FSJ 5.3.3 Fisheries Sensitive Watersheds
	The road(s) included in this Site Plan is/are not located within a Fisheries Sensitive Watershed.
or
If all or a portion of the road(s) is/are located within a Fisheries Sensitive Watershed, specific wording will be required to ensure consistency with the results and strategies pertinent to FSW.

	VHF 5.3.3 Moose Ungulate Winter Range
	The road(s) included in this Site Plan is/are not within the applicable areas of Order – Moose Ungulate Winter Range U7-018 and U7-020.
or
If all or a portion of the road(s) is/are located within one or more of the applicable areas of the Orders listed above, specific wording will be required.

	FSJ 5.4.1 Mule Deer Designations

VHF 5.4.1 Mule Deer Designations
	The road(s) included in this Site Plan is/are not within the applicable areas of Order - Ungulate Winter Range U7-002 (Mule Deer).

The road(s) included in this Site Plan is/are not within the applicable areas of Order - Ungulate Winter Range U7-011 (Mule Deer).

If all or a portion of the road(s) is/are located within the applicable area of the Order listed above, specific wording will be required.

	FSJ 5.4.2 Recreation Designations
	The road(s) included in this Site Plan is/are not within 200 metres of a designated Recreation Site, Recreation Trail or Interpretive Trail.
or
The road(s) included in this Site Plan is/are within 200 metres of [name of Recreation Site, Recreation Trail or Interpretative Trail] and was determined according to the requirements identified in the approved Forest Stewardship Plan and authorized by the District Manager.

	FSJ 5.4.3 Lakeshore Classification
	The grand-parented lake class designations are reflected in the Forest Stewardship Plan and the lake riparian class and associated riparian management areas, riparian reserve zones and riparian management zones are consistent with the Fort St James lakeshore classification designations as per Table 1 of subparagraph 5.2.3.1 of the Forest Stewardship Plan (FSP). 

	FSJ or VHF 6.1 Invasive Plant Measure

	The road(s) included in this Site Plan is/are not located within an area where the spread of invasive plants pose an extremely high, high or moderate risk.  No further mitigative measures are required.
or
All or a portion of the road(s) included in this Site Plan is/are located within an area where the spread of invasive plants poses an extremely high risk.  Areas of disturbed soils within the road right of way 0.25 hectares or greater which are located within 5 km of highly susceptible areas (such as seed or other high-value agricultural crops and private land), that will not be reforested, must be seeded with grass and legumes within 6 months of completing Primary Forest Activities.  These sites must be monitored following seeding and re-seeded within one year of inspection as per the Forest Stewardship Plan measure.
or
All or a portion of the road(s) included in this Site Plan is/are located within an area where the spread of invasive plants poses a high risk.  Areas of disturbed soils within the road right of way 0.5 hectares or greater which are within 5 km of a site identified as containing extremely or very invasive plants (as described by the Northwest Invasive Plant Committee), that will not be reforested, must be seeded with grass and legumes within 1 year of completing Primary Forest Activities.  These sites must be monitored following seeding and re-seeded within one year of inspection as per the Forest Stewardship Plan measure.
or
All or a portion of the road(s) included in this Site Plan is/are located within an area where the spread of invasive plants poses a moderate risk.  Areas of disturbed soils within the road right of way 0.5 hectares or greater which are within 5 km of a site identified as containing invasive or aggressive invasive plants (as described by the Northwest Invasive Plant Committee), that will not be reforested, must be seeded with grass and legumes within 2 years of completing Primary Forest Activities.  These sites must be monitored following seeding and re-seeded within one year of inspection as per the Forest Stewardship Plan measure.

	FSJ or VHF 6.2 Range Barrier Measure

	The road(s) included in this Site Plan is/are not located within a Range Tenure area.
or
All or a portion of the road(s) included in this Site Plan is/are located within the [Range Tenure type held by Range Tenure holder name].  The tenure holder has not identified the removal of natural range barriers through the construction of the road(s).  No further mitigative measures are required.
or
All or a portion of the road(s) included in this Site Plan is/are located within the [Range Tenure type held by Range Tenure holder name].  The tenure holder has satisfactorily demonstrated that the construction of the road(s) will remove a natural range barrier.  As such, BCTS will mitigate the effects by [constructing/installing an artificial range barrier.  Installation of a cattle guard and associated wing fencing on either side of the access into the block will occur prior to [date] as mutually agreed to by BCTS and the Range Tenure holder].
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Supporting Information
The following is attached for information only and does not form part of the Road Site Plan.

	[bookmark: Check25][bookmark: Check26]Visual Impact Assessment			|_| required	|_| not required
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	Archaeological Impact Assessment		|_| required	|_| not required
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	Terrain Stability Assessment			|_| required	|_| not required
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	Riparian Assessment				|_| required	|_| not required
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	Soils Information (for construction cost reporting purposes)
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Construction Specifications
	1. Revegetation specifications

	Licensee will ensure revegetation of all exposed soils in accordance with the current legislative requirements.  BC Timber Sales will ensure revegetation of exposed soils as per Forest Stewardship Plan Invasive Plant Measure.



	2. Road widening on curves – the widening required on curves shall be:

	[bookmark: Check1][bookmark: Check2]	|X| provided in Forest Road Engineering Guidebook or |_| as per table below:

	radius of curve (m)
	180
	90
	60
	45
	35
	25
	20
	15

	minimum subgrade width required (m)
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	3. Maximum dimensions and weights of the intended loaded vehicle for use on the road are:

	[bookmark: Check3][bookmark: Check4][bookmark: Check5]	|_| conforms to MoTH regulations (CL625), |X| L100, or |_| other - if other, complete the following:

	length (m)
	0.0

	width (m)
	0.0

	height (m)
	0.0

	maximum log length (m)
	0.0

	overhang beyond rear trailer bunk (m)
	0.0

	weight axle - tandem (kg)
	0

	GVW (kg)
	0



	4. Attachments:

	[bookmark: Check7]	|_| Geometric Road Design 	|_| Road Design Drawings	|X| Road Site Plan Map
[bookmark: Check9][bookmark: Check10]	|_| Assessments		|_| Other Reports
[bookmark: Check17][bookmark: Check18]	|X| Schedule A1 (Design Criteria & Road Specs)			|_| Schedule A2 (Crossings Table)





Schedule A1 – Design Criteria & Road Specs

	Road Name/Reference No.:
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	Section length (km – km)
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Design Criteria
	Construct and maintain road
	[bookmark: Check19]|_|
	|_|
	|_|
	|_|

	Modify and/or maintain road
	[bookmark: Check20]|_|
	|_|
	|_|
	|_|

	Road Type1
	[bookmark: Dropdown1]
	
	
	

	Soil type
	     
	     
	     
	     

	Likelihood of landslides (L or M/H)
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	Road location Survey Level (1, 2, 3 or 4)
	
	
	
	

	Maximum stripping width (m)
	10.0
	10.0
	10.0
	10.0

	Max/Min road subgrade width (m)
	[bookmark: Text33]6.0/5.0
	6.0/5.0
	6.0/5.0
	6.0/5.0

	Ditch depth in OM (m)
	0.0
	0.0
	0.0
	0.0

	Ditch depth in rock (m)
	0.0
	0.0
	0.0
	0.0

	Minimum usable turnout length/width (m)
	[bookmark: Text48]30.0/9.0
	30.0/9.0
	30.0/9.0
	30.0/9.0

	Turnouts – planned distance between (m)
	350
	350
	350
	350

	Minimum curve radius (m)
	35
	35
	35
	35

	Maximum adverse sustained grade (%)
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	Maximum favourable sustained grade (%)
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	Maximum adverse short pitch (<100m) grade (%)
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	Maximum favourable short pitch (<150m) grade (%)
	[bookmark: Text42]     
	     
	     
	     

	Minimum cross-drain culvert size (mm)2
	[bookmark: Text43]400 or ADS
	400 or ADS
	400 or ADS
	400 or ADS

	Junction with a FSR (Y/N)3
	
	
	
	

		Minimum site distance (m)
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		Junction angle (deg.)
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		Road approach grade (%)
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1Road Type options:	Long Term (LT) – continuous raised sub-grade and ditch line.
     (appraised)	Short Term (ST) - bladed running surface (possible elements of stumping, ditching and elevated grade)
	Snow/Ice – single lane seasonal winter road (surface may or may not have stumps removed)

2ADS: Appropriate Drainage Structure (ie. capable of maintaining natural drainage pattern).

3A road that junctions with an FSR must have a stop sign, road sign, radio channel and cross-drain culvert (min 400 mm) or ADS.




Road Specifications
	Stumps, roots or logs in road prism outside subgrade (Y/N)
	[bookmark: Dropdown6]
	
	
	

	Stumps, roots, or logs under road subgrade width (Y/N)
	
	
	
	

	Organic material in fill (Y/N)
	
	
	
	

	Disposal of slash/debris
	
	
	
	

	Width required for slash/debris disposal4
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	Full bench construction (end hauling) (Y/N) – site specific
	
	
	
	

	Surfacing depth (mm)
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	[bookmark: Text49]Other:      
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	Number of R/W landings per km
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4width between toe of fill and lower clearing boundary





Schedule A2 – Crossings Table

List bridges, culverts and engineered structures for all stream and drainage crossings.

	Block/ Road Name
	Stream ID/ Riparian Class
	Fish Stream
(Y/N)
	Structure Location
(km)
	Structure Class1
	Structure Size2
	Prof. Design (Y/N)
	TWC3 Permitted
	Comments
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1Structure Class:	Bridge – Semi-permanent (BS), Permanent (BP) or Temporary (BT)
		Culvert – Round (CR), Elliptical (CE) or Arch (CA)
		Design Vehicle – L75, L100 or L625
		eg. BT/L75 (temporary bridge with load rating of L75)

2Structure Size:	For bridges, detail span length and height of abutment
		For culverts, detail opening dimension
		For log culverts, detail span length (< 6.0m) and sill log height

3TWC: Temporary Winter Crossing (as defined in FPI Temporary Winter Crossings brochure).

Note: Where appropriate, significant drainage (NCD) crossings should also permit the installation of an Appropriate Drainage Structure (eg. under Structure Class, can list as “CR or ADS”).
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